(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "PGA-103+ Preamplifier, Version 2.0.0.0")
    (date "2024-03-11")
    (rev "A")
    (company "VTGS, GSN-SDA")
    (comment 1 "Preamplifier for VHF/UHF Satellite Rx")
    (comment 2 "creativecommons.org/licenses/by/4.0/")
    (comment 3 "License: CC BY 4.0")
    (comment 4 "Author: Zach Leffke, KJ4QLP")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 120.65 107.95)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "Net-(U1-BP)")
  (net 4 "Net-(JP1-C)")
  (net 5 "Net-(J1-In)")
  (net 6 "+5V")
  (net 7 "Net-(JP1-B)")
  (net 8 "Net-(J2-In)")
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(JP2-C)")
  (net 11 "Net-(U1-EN)")
  (net 12 "Net-(U1-OUT)")
  (net 13 "Net-(C11-Pad1)")
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 125.095 114.681 180)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at -2.413 0) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.95) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 180) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 180) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(JP1-C)") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 112.395 115.57 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -1.27 1.27 90) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(U1-EN)") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Plated_Hole_D4.0mm" (layer "F.Cu")
    (at 104.648 127.889)
    (descr "Plated Hole as test Point, diameter 4.0mm")
    (tags "test point plated hole")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at -5.207 0) (layer "F.SilkS"))
    (fp_text value "Hole" (at -5.08 3.429) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.207 -1.016) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 129.159 111.76 90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "1000pF" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(JP2-C)") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 113.919 111.76 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -2.54 0 90) (layer "F.SilkS"))
    (fp_text value "1.0uF" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (at 127 120.65)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 3-pole, open")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 1.524) (layer "F.SilkS"))
    (fp_text value "bias-tee" (at 0 1.9) (layer "F.Fab"))
    (fp_text user "1" (at -2.54 0) (layer "F.SilkS"))
    (fp_text user "3" (at 2.54 0) (layer "F.SilkS"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(JP1-B)") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(JP2-C)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "+12V") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 117.729 111.76 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at -2.54 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U1-OUT)") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 114.935 107.95)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.27) (layer "F.SilkS"))
    (fp_text value "1000pF" (at 0 1.95) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-In)") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C10-Pad2)") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 121.539 111.76 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at -2.54 0 90) (layer "F.SilkS"))
    (fp_text value "1.0uF" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "+5V") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm" (layer "F.Cu")
    (at 124.46 125.095)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 6.985 1.27) (layer "F.SilkS"))
    (fp_text value "+12V" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.985 0) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 1 "+12V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (at 121.285 120.65)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 3-pole, open")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 1.524) (layer "F.SilkS"))
    (fp_text value "bias-tee" (at 0 1.9) (layer "F.Fab"))
    (fp_text user "1" (at -2.54 0) (layer "F.SilkS"))
    (fp_text user "3" (at 2.54 0) (layer "F.SilkS"))
    (pad "1" smd custom (at -1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 6 "+5V") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(JP1-C)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(JP1-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount" (layer "F.Cu")
    (at 143.9275 107.95 90)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J2" (at -3.81 -2.975 270) (layer "F.SilkS"))
    (fp_text value "RF_OUT" (at 0 13 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at -3.175 2.6 90) (layer "Dwgs.User"))
    (fp_text user "Board Thickness: 1.57mm" (at 0 12.9175 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 4.79 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0.2 90) (size 1.27 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J2-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at -2.825 0 90) (size 1.35 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (pad "2" smd rect (at -2.825 0 90) (size 1.35 4.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (pad "2" smd rect (at 2.825 0 90) (size 1.35 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (pad "2" smd rect (at 2.825 0 90) (size 1.35 4.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount" (layer "F.Cu")
    (at 97.3725 107.95 -90)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J1" (at 3.81 -2.9575 90) (layer "F.SilkS"))
    (fp_text value "RF_IN" (at 0 13 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 3.81 2.6 90) (layer "Dwgs.User"))
    (fp_text user "Board Thickness: 1.57mm" (at 0 14.805 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 5.2975 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0.2 270) (size 1.27 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at -2.825 0 270) (size 1.35 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (pad "2" smd rect (at -2.825 0 270) (size 1.35 4.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (pad "2" smd rect (at 2.825 0 270) (size 1.35 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (pad "2" smd rect (at 2.825 0 270) (size 1.35 4.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (zone_connect 2))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 115.824 111.76 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at -2.54 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 125.73 107.95)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.27) (layer "F.SilkS"))
    (fp_text value "1000pF" (at 0 1.95) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J2-In)") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 120.015 116.459 180)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.95) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 180) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 180) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(U1-BP)") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 123.444 111.76 90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 2.506 0 90) (layer "F.SilkS"))
    (fp_text value "220nH" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(JP1-C)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C11-Pad1)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Plated_Hole_D4.0mm" (layer "F.Cu")
    (at 136.652 88.011)
    (descr "Plated Hole as test Point, diameter 4.0mm")
    (tags "test point plated hole")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.826) (layer "F.SilkS"))
    (fp_text value "Hole" (at -0.127 -6.858) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -4.826) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 119.634 111.76 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at -2.54 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "+5V") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 127.254 111.76 90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L2" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "220nH" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(JP2-C)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 90) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(J2-In)") (pinfunction "2") (pintype "passive"))
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 120.015 114.681)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.95) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U1-OUT)") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "+5V") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 115.7025 115.475)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "500mA Low drop-out regulator, Fixed Output 5.0V, SOT-23-5")
    (property "ki_keywords" "REGULATOR LDO 5.0V")
    (attr smd)
    (fp_text reference "U1" (at -1.0215 2.127) (layer "F.SilkS"))
    (fp_text value "SPX3819M5-L-5-0" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U1-EN)") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(U1-BP)") (pinfunction "BP") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1-OUT)") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 113.03 104.4725 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "BAV99 High-speed switching diodes, SOT-23")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D1" (at -1.4755 -0.0485 -90) (layer "F.SilkS"))
    (fp_text value "BAV99" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J1-In)") (pinfunction "K") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 112.014 111.76 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -2.413 0 90) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(J1-In)") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm" (layer "F.Cu")
    (at 113.665 125.095)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 10.795) (layer "F.SilkS"))
    (fp_text value "PTT" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.635 12.065) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(U1-EN)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm" (layer "F.Cu")
    (at 120.015 125.095)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 8.255) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.635 9.525) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (at 121.285 106 90)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "50-4000MHz +11dB Low Noise Amplifier, SOT-89")
    (property "ki_keywords" "RF amplifier")
    (attr smd)
    (fp_text reference "U2" (at 2.114 -1.905 180) (layer "F.SilkS"))
    (fp_text value "PGA-103" (at 0 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.2 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -1.5 90) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C10-Pad2)") (pintype "input"))
    (pad "2" smd custom (at -1.8625 0 90) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
          )
          (width 0) (fill yes))
      ))
    (pad "3" smd rect (at -1.95 1.5 90) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(C11-Pad1)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RF_Shielding:Wuerth_36103205_20x20mm" (layer "F.Cu")
    (at 120.65 107.95)
    (descr "WE-SHC Shielding Cabinet SMD 20x20mm")
    (tags "Shielding Cabinet")
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Two-piece EMI RF shielding cabinet")
    (property "ki_keywords" "RF EMI shielding cabinet")
    (attr smd)
    (fp_text reference "J3" (at -6.35 -9.525) (layer "F.SilkS"))
    (fp_text value "RFShield_TwoPieces" (at 0 11.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -6.35 -9.525) (layer "F.Fab"))
    (pad "1" smd rect (at -10.25 -10.25) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -10.25 -8.6) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -10.25 -3.75) (size 1 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -10.25 3.75) (size 1 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -10.25 8.6) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -10.25 10.25) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -8.6 -10.25) (size 2.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -8.6 10.25) (size 2.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -3.75 -10.25) (size 2.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at -3.75 10.25) (size 2.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 3.75 -10.25) (size 2.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 3.75 10.25) (size 2.6 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 8.6 -10.25) (size 2.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 8.6 10.25) (size 2.3 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 10.25 -10.25) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 10.25 -8.6) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 10.25 -3.75) (size 1 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 10.25 3.75) (size 1 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 10.25 8.6) (size 1 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "1" smd rect (at 10.25 10.25) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/RF_Shielding.3dshapes/Wuerth_36103205_20x20mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:0805" (layer "F.Cu")
    (at 125.349 111.76 -90)
    (property "Sheetfile" "pga103_v2.0.0.0.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at -2.54 0 90) (layer "F.SilkS"))
    (fp_text value "1000pF" (at 0 1.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 270) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(JP1-C)") (pintype "passive"))
  )
  (gr_line (start 139.7 92.71) (end 139.7 83.82)
    (layer "Edge.Cuts"))
  (gr_line (start 101.6 132.08) (end 129.54 132.08)
    (layer "Edge.Cuts"))
  (gr_line (start 101.6 123.19) (end 101.6 132.08)
    (layer "Edge.Cuts"))
  (gr_line (start 146.05 92.71) (end 146.05 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 129.54 123.19) (end 146.05 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 95.25 92.71) (end 95.25 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 111.76 83.82) (end 111.76 92.71)
    (layer "Edge.Cuts"))
  (gr_line (start 111.76 92.71) (end 95.25 92.71)
    (layer "Edge.Cuts"))
  (gr_line (start 146.05 92.71) (end 139.7 92.71)
    (layer "Edge.Cuts"))
  (gr_line (start 95.25 123.19) (end 101.6 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 129.54 132.08) (end 129.54 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 83.82) (end 111.76 83.82)
    (layer "Edge.Cuts"))
  (gr_text "TRUE" (at 105.41 102.235 90) (layer "F.SilkS"))
  (gr_text "RF IN" (at 100.965 107.95 90) (layer "F.SilkS"))
  (gr_text "+12V" (at 124.46 127.635) (layer "F.SilkS"))
  (gr_text "1-2" (at 107.95 106.045 90) (layer "F.SilkS"))
  (gr_text "GND" (at 120.015 127.635) (layer "F.SilkS"))
  (gr_text "5V COAX" (at 107.95 116.84 90) (layer "F.SilkS"))
  (gr_text "1-2" (at 105.41 109.855 90) (layer "F.SilkS"))
  (gr_text "2-3" (at 107.95 109.855 90) (layer "F.SilkS"))
  (gr_text "KJ4QLP, 20231002" (at 123.19 131.445) (layer "F.SilkS"))
  (gr_text "G:" (at 135.255 97.155) (layer "F.SilkS"))
  (gr_text "JP2" (at 104.14 106.045 90) (layer "F.SilkS"))
  (gr_text "~{PTT}" (at 113.665 127.635) (layer "F.SilkS"))
  (gr_text "RF OUT" (at 138.43 107.95 90) (layer "F.SilkS"))
  (gr_text "BAND:" (at 118.745 94.615) (layer "F.SilkS"))
  (gr_text "SN:" (at 133.985 121.285) (layer "F.SilkS"))
  (gr_text "FALSE" (at 107.95 102.235 90) (layer "F.SilkS"))
  (gr_text "MODE" (at 104.14 116.84 90) (layer "F.SilkS"))
  (gr_text "12V COAX" (at 105.41 116.84 90) (layer "F.SilkS"))
  (gr_text "Vreg" (at 104.14 102.235 90) (layer "F.SilkS"))
  (gr_text "NF:" (at 135.255 100.965) (layer "F.SilkS"))
  (gr_text "JP1" (at 104.14 109.855 90) (layer "F.SilkS"))
  (gr_text "2-3" (at 105.41 106.045 90) (layer "F.SilkS"))
  (gr_text "12V EXT" (at 106.68 116.84 90) (layer "F.SilkS"))
  (gr_text "PGA-103+ LNA\nVersion 2.0.0.0\nRevision A\nUnfiltered" (at 112.395 88.392) (layer "F.SilkS"))
  (gr_text "OPEN" (at 106.68 106.68 90) (layer "F.SilkS"))
  (gr_text "DC IN" (at 140.335 107.95 90) (layer "F.SilkS"))
  (gr_text "1-2" (at 106.68 109.855 90) (layer "F.SilkS"))
  (gr_text "TRUE" (at 106.68 102.235 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 139.7 92.71) (xy 146.05 92.71))
    (height -14.605)
    (gr_text "250.0000 mils" (at 146.685 76.835) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 139.7 83.82) (xy 111.76 83.82))
    (height 5.715)
    (gr_text "1100.0000 mils" (at 125.73 76.955) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 101.6 132.08) (xy 129.54 132.08))
    (height 5.08)
    (gr_text "1100.0000 mils" (at 115.57 136.01) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 95.25 92.71) (xy 146.05 92.71))
    (height -20.32)
    (gr_text "2000.0000 mils" (at 120.65 71.24) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 95.25 92.71) (xy 95.25 123.19))
    (height 19.685)
    (gr_text "1200.0000 mils" (at 74.415 107.95 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 139.7 83.82) (xy 139.7 92.71))
    (height -12.7)
    (gr_text "350.0000 mils" (at 151.25 88.265 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 95.25 83.82) (xy 95.25 132.08))
    (height 27.305)
    (gr_text "1900.0000 mils" (at 66.795 107.95 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.25 92.71)
        (xy 111.76 92.71)
        (xy 111.76 83.82)
        (xy 139.7 83.82)
        (xy 139.7 92.71)
        (xy 146.05 92.71)
        (xy 146.05 123.19)
        (xy 129.54 123.19)
        (xy 129.54 132.08)
        (xy 101.6 132.08)
        (xy 101.6 123.19)
        (xy 95.25 123.19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.SilkS") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.635 95.885)
        (xy 118.745 95.885)
        (xy 118.745 93.345)
        (xy 127.635 93.345)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.SilkS") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.605 95.885)
        (xy 135.255 95.885)
        (xy 135.255 98.425)
        (xy 141.605 98.425)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.SilkS") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.605 99.695)
        (xy 135.255 99.695)
        (xy 135.255 102.235)
        (xy 141.605 102.235)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.SilkS") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.605 120.015)
        (xy 133.985 120.015)
        (xy 133.985 122.555)
        (xy 141.605 122.555)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "*.Mask") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.605 92.71)
        (xy 146.05 92.71)
        (xy 146.05 123.19)
        (xy 141.605 123.19)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "*.Mask") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.25 92.71)
        (xy 99.695 92.71)
        (xy 99.695 123.19)
        (xy 95.25 123.19)
      )
    )
  )
)
