(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 74)
    (zones 0)
    (modules 18)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.2032)
    (via_size 0.6096)
    (via_drill 0.3048)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (user_via 0.6096 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.778 1.778)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /INTB)
  (net 4 /SDA)
  (net 5 /SCL)
  (net 6 "Net-(X1-Pad1)")
  (net 7 "Net-(U1-Pad3)")
  (net 8 "Net-(C6-Pad2)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 "Net-(R1-Pad2)")
  (net 11 "Net-(R2-Pad1)")
  (net 12 "Net-(C7-Pad2)")
  (net 13 "Net-(C7-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.1524)
    (add_net +3V3)
    (add_net /INTB)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(X1-Pad1)")
  )
  (module Connector_Coaxial:U.FL_Molex_MCRF_73412-0110_Vertical (layer B.Cu) (tedit 5D124F51)
    (at 129.667 103.378)
    (descr "Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference REF** (at 0 -3.5) (layer B.SilkS) hide)
    (fp_text value U.FL_Molex_MCRF_73412-0110_Vertical (at 0 3.302) (layer B.Fab))
    (fp_text user %R (at 0 -3.5) (layer B.Fab))
    (pad 1 smd rect (at 0 -1.5) (size 1 1) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 1.5) (size 1 1) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 1.575 0) (size 0.9 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -1.575 0) (size 0.9 1.9) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connector_Coaxial:U.FL_Molex_MCRF_73412-0110_Vertical (layer B.Cu) (tedit 5D124F51)
    (at 129.667 98.298)
    (descr "Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference REF** (at 0 -3.5) (layer B.SilkS) hide)
    (fp_text value U.FL_Molex_MCRF_73412-0110_Vertical (at 0 3.302) (layer B.Fab))
    (fp_text user %R (at 0 -3.5) (layer B.Fab))
    (pad 2 smd rect (at -1.575 0) (size 0.9 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 1.575 0) (size 0.9 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 1.5) (size 1 1) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at 0 -1.5) (size 1 1) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module custom-footprints:SON50P400X400X80-13N (layer F.Cu) (tedit 0)
    (at 115.914 101.485)
    (descr DNT0012B)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value FDC2212 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 13 smd rect (at 0 0) (size 2.7 3.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2 -1.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 11 smd rect (at 2 -0.75 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C7-Pad2)"))
    (pad 10 smd rect (at 2 -0.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 9 smd rect (at 2 0.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (pad 8 smd rect (at 2 0.75 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2 1.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 6 smd rect (at -2 1.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2 0.75 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /INTB))
    (pad 4 smd rect (at -2 0.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 3 smd rect (at -2 -0.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -2 -0.75 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA))
    (pad 1 smd rect (at -2 -1.25 90) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-12-1EP_4x4mm_P0.5mm_EP2.66x3.38mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-2012-15_AVX-P (layer F.Cu) (tedit 5B301BBE)
    (at 113.792 105.2195 90)
    (descr "Tantalum Capacitor SMD AVX-P (2012-15 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/40182/tmch.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C5 (at 0.889 -1.651 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.58 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8875 0 90) (size 1.125 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.238095)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.8875 0 90) (size 1.125 1.05) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.238095)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-2012-15_AVX-P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 5CFAC83C)
    (at 129.667 97.028 270)
    (descr "Terminal Block TE 282834-4, 4 pins, pitch 2.54mm, size 10.620000000000001x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-4 pitch 2.54mm size 10.620000000000001x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J2 (at 3.81 -4.37 270) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x04 (at 3.81 4.37 270) (layer F.Fab))
    (fp_text user %R (at 3.81 2 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.778 1.778) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(C6-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.778 1.778) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.778 1.778) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x04_P5.00mm_45-Degree.step
      (offset (xyz 7.62 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 108.204 96.774 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SCL))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 112.522 102.743 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.4605 0.127 270 unlocked) (layer F.SilkS))
    (fp_text value 0 (at 0 1.45 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 270) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /INTB))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 111.5695 105.4735)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0.0635 1.143 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 110.67034 105.4735 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 1.651 0 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_SMD_TXC_7C-4Pin_5.0x3.2mm (layer F.Cu) (tedit 58CD3345)
    (at 108.585 102.489)
    (descr "Miniature Crystal Clock Oscillator TXC 7C series, http://www.txccorp.com/download/products/osc/7C_o.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference X1 (at 0 0 270 unlocked) (layer F.SilkS))
    (fp_text value TXC-7C (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -1.27 -1.1) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at 1.27 -1.1) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at 1.27 1.1) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.27 1.1) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(X1-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_EuroQuartz_MT-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.92 103.378 90)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at -2.921 0 180) (layer F.SilkS))
    (fp_text value 18uH (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(C6-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.92 98.552 90)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value 18uH (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(C7-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.586 106.299)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 1.778 0.254) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 125.349 103.378 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -1.9558 0 180) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C6-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 125.349 98.552 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.032 0) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.586 105.156)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 1.778 0.254) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.586 104.013)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 1.778 0.254) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.95 99.695)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -1.651 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 126.111 95.123) (end 132.334 95.123) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.111 107.315) (end 132.334 107.315) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.587 95.123) (end 123.063 95.123) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.587 107.315) (end 126.111 107.315) (angle -180) (layer Edge.Cuts) (width 0.05))
  (dimension 27.559 (width 0.15) (layer Dwgs.User)
    (gr_text "27.559 mm" (at 119.1895 92.172) (layer Dwgs.User))
    (feature1 (pts (xy 132.969 95.758) (xy 132.969 92.885579)))
    (feature2 (pts (xy 105.41 95.758) (xy 105.41 92.885579)))
    (crossbar (pts (xy 105.41 93.472) (xy 132.969 93.472)))
    (arrow1a (pts (xy 132.969 93.472) (xy 131.842496 94.058421)))
    (arrow1b (pts (xy 132.969 93.472) (xy 131.842496 92.885579)))
    (arrow2a (pts (xy 105.41 93.472) (xy 106.536504 94.058421)))
    (arrow2b (pts (xy 105.41 93.472) (xy 106.536504 92.885579)))
  )
  (dimension 12.192 (width 0.15) (layer Dwgs.User)
    (gr_text "12.192 mm" (at 137.19 101.219 270) (layer Dwgs.User))
    (feature1 (pts (xy 132.334 107.315) (xy 136.476421 107.315)))
    (feature2 (pts (xy 132.334 95.123) (xy 136.476421 95.123)))
    (crossbar (pts (xy 135.89 95.123) (xy 135.89 107.315)))
    (arrow1a (pts (xy 135.89 107.315) (xy 135.303579 106.188496)))
    (arrow1b (pts (xy 135.89 107.315) (xy 136.476421 106.188496)))
    (arrow2a (pts (xy 135.89 95.123) (xy 135.303579 96.249504)))
    (arrow2b (pts (xy 135.89 95.123) (xy 136.476421 96.249504)))
  )
  (gr_text CAP-10 (at 107.188 105.2195) (layer F.Mask))
  (gr_text Holliday (at 107.188 105.9815) (layer F.Mask))
  (gr_text SCL (at 113.284 99.695 270) (layer B.SilkS))
  (gr_text SDA (at 110.617 99.695 270) (layer B.SilkS))
  (gr_text GND (at 108.204 99.695 270) (layer B.SilkS))
  (gr_text 3.3V (at 115.824 99.695 270) (layer B.SilkS))
  (gr_text CH1 (at 132.3975 98.425 90) (layer B.SilkS))
  (gr_text CH0 (at 132.3975 103.251 90) (layer B.SilkS))
  (gr_text CH1 (at 123.952 98.552 270) (layer F.SilkS))
  (gr_text CH0 (at 123.952 103.378 270) (layer F.SilkS))
  (gr_text CH0 (at 119.761 103.378 270) (layer F.SilkS))
  (gr_text CH1 (at 119.761 98.552 270) (layer F.SilkS))
  (gr_arc (start 106.045 95.758) (end 106.045 95.123) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 106.045 106.68) (end 105.41 106.68) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 132.334 106.68) (end 132.334 107.315) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 132.334 95.758) (end 132.969 95.758) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text SCL (at 112.649 99.314 270) (layer F.SilkS))
  (gr_text SDA (at 111.379 99.314 270) (layer F.SilkS))
  (gr_text GND (at 106.045 96.901 270) (layer F.SilkS))
  (gr_text 3.3V (at 118.11 96.901 270) (layer F.SilkS))
  (gr_text 0x2B (at 109.5375 106.4895) (layer B.SilkS))
  (gr_text 0x2A (at 112.3315 106.4895) (layer B.SilkS))
  (gr_line (start 105.41 106.68) (end 105.41 95.758) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.063 107.315) (end 106.045 107.315) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.969 95.758) (end 132.969 106.68) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.045 95.123) (end 123.063 95.123) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 105.41 95.123) (xy 117.348 95.123) (xy 117.348 101.981) (xy 118.491 101.981) (xy 118.491 107.315)
        (xy 117.348 107.315) (xy 105.41 107.315)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 105.41 95.123) (xy 117.348 95.123) (xy 117.348 101.981) (xy 118.491 101.981) (xy 118.491 107.315)
        (xy 105.41 107.315)
      )
    )
  )
)
