(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 401)
    (zones 0)
    (modules 57)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.27 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.56 0.65)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D2-Pad1)")
  (net 3 "Net-(D3-Pad1)")
  (net 4 "Net-(D4-Pad1)")
  (net 5 "Net-(D5-Pad1)")
  (net 6 "Net-(D6-Pad1)")
  (net 7 "Net-(D8-Pad1)")
  (net 8 +BATT)
  (net 9 +3V0)
  (net 10 AIN3_BATT)
  (net 11 +15V)
  (net 12 PA7_PROBE_OUT)
  (net 13 PA5_ENA_PROX)
  (net 14 PB0_LED_R)
  (net 15 PB1_LED_G)
  (net 16 PB2_LED_B)
  (net 17 PA6_PROBE_IN)
  (net 18 PA0_UPDI)
  (net 19 PA4_PROX_IN)
  (net 20 GND)
  (net 21 /Prox_Out)
  (net 22 "Net-(D8-Pad2)")
  (net 23 PA1_TxD2)
  (net 24 PA2_RxD2)
  (net 25 PB3)
  (net 26 /Q2BD)
  (net 27 /RED)
  (net 28 /GRN)
  (net 29 /BLU)
  (net 30 /UPDI)
  (net 31 /Q1BG)
  (net 32 /Q1AG)
  (net 33 /VIN)
  (net 34 /PA6B)
  (net 35 /TP1)
  (net 36 /TP2)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net +15V)
    (add_net +3V0)
    (add_net +BATT)
    (add_net /BLU)
    (add_net /GRN)
    (add_net /PA6B)
    (add_net /Prox_Out)
    (add_net /Q1AG)
    (add_net /Q1BG)
    (add_net /Q2BD)
    (add_net /RED)
    (add_net /TP1)
    (add_net /TP2)
    (add_net /UPDI)
    (add_net /VIN)
    (add_net AIN3_BATT)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net PA0_UPDI)
    (add_net PA1_TxD2)
    (add_net PA2_RxD2)
    (add_net PA4_PROX_IN)
    (add_net PA5_ENA_PROX)
    (add_net PA6_PROBE_IN)
    (add_net PA7_PROBE_OUT)
    (add_net PB0_LED_R)
    (add_net PB1_LED_G)
    (add_net PB2_LED_B)
    (add_net PB3)
  )
  (net_class Minimum ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class Power ""
    (clearance 0.635)
    (trace_width 0.635)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.635)
    (diff_pair_gap 0.635)
  )
  (module Boeing_6652:1946_or_S70-332 locked (layer F.Cu) (tedit 5E9F6F3D)
    (at 164.2364 115.062)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (fp_text reference TP2 (at 0 3.302) (layer F.SilkS))
    (fp_text value Probe_GND (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1) (layers F.Cu F.Mask)
      (net 36 /TP2))
    (pad 1 thru_hole circle (at 0 0) (size 2.25 2.25) (drill 1) (layers B.Cu B.Mask)
      (net 36 /TP2))
  )
  (module Boeing_6652:1946_or_S70-332 locked (layer F.Cu) (tedit 5E9F6F01)
    (at 164.2364 88.138)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (fp_text reference TP1 (at -0.0254 -3.048) (layer F.SilkS))
    (fp_text value Probe_Sig (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1) (layers F.Cu F.Mask)
      (net 35 /TP1))
    (pad 1 thru_hole circle (at 0 0) (size 2.25 2.25) (drill 1) (layers B.Cu B.Mask)
      (net 35 /TP1))
  )
  (module RA_LED:SOIC-14_3.9x8.7mm_P1.27mm_Handsoldering (layer F.Cu) (tedit 5E90E1C0)
    (at 152.4 101.6)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at -3.81 -6.604) (layer F.SilkS))
    (fp_text value ATtiny1614-SSN (at 0 5.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd roundrect (at 2.675 -3.81) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 GND))
    (pad 13 smd roundrect (at 2.675 -2.54) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 AIN3_BATT))
    (pad 12 smd roundrect (at 2.675 -1.27) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 PA2_RxD2))
    (pad 11 smd roundrect (at 2.675 0) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 PA1_TxD2))
    (pad 10 smd roundrect (at 2.675 1.27) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 PA0_UPDI))
    (pad 9 smd roundrect (at 2.675 2.54) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 PB0_LED_R))
    (pad 8 smd roundrect (at 2.675 3.81) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 PB1_LED_G))
    (pad 7 smd roundrect (at -2.675 3.81) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 PB2_LED_B))
    (pad 6 smd roundrect (at -2.675 2.54) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 PB3))
    (pad 5 smd roundrect (at -2.675 1.27) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 PA7_PROBE_OUT))
    (pad 4 smd roundrect (at -2.675 0) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 PA6_PROBE_IN))
    (pad 3 smd roundrect (at -2.675 -1.27) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 PA5_ENA_PROX))
    (pad 2 smd roundrect (at -2.675 -2.54) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 PA4_PROX_IN))
    (pad 1 smd roundrect (at -2.675 -3.81) (size 2.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +3V0))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 152.4 101.6)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 2.54) (layer B.SilkS))
    (fp_text value PB3 (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask)
      (net 25 PB3))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.636 104.648 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at -3.556 0 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 36 /TP2))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5E9F69E5)
    (at 140.97 95.25)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS))
    (fp_text value TPS709 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 +3V0))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 167.4876 114.2492 50)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D9 (at 0 -1.8 50) (layer B.SilkS))
    (fp_text value LED (at 0 -3 50) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 50) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 50) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D8-Pad2)"))
    (pad 2 smd roundrect (at 1.5 0 50) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /Prox_Out))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 155.829 120.9802 10)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D8 (at 0 -1.8 10) (layer B.SilkS))
    (fp_text value LED (at -0.000001 -3 10) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 10) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 10) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D8-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 10) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D8-Pad2)"))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 167.4876 88.9508 130)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D6 (at 0 -1.8 130) (layer B.SilkS))
    (fp_text value LED (at 0 -3 130) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 130) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 130) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D6-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 130) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D5-Pad1)"))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 155.829 82.2198 170)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D5 (at -4.294935 -0.222777 170) (layer B.SilkS))
    (fp_text value LED (at 0.000001 -3 170) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 170) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 170) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 170) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D4-Pad1)"))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 142.5702 84.5566 210)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D4 (at 0 -1.8 30) (layer B.SilkS))
    (fp_text value LED (at 0 -3 30) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 30) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 210) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 210) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D3-Pad1)"))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 133.9088 94.869 250)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D3 (at 0 -1.8 70) (layer B.SilkS))
    (fp_text value LED (at 0 -3 70) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 70) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 250) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D3-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 250) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 133.9088 108.331 290)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D2 (at 0 -1.8 110) (layer B.SilkS))
    (fp_text value LED (at 0 -3 110) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 110) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 290) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 290) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652_IPSS_Upper_043016:LED_Kingbright_APDA3020LSECK_J3-PF_3x2mm_Horizontal locked (layer B.Cu) (tedit 5E9F2399)
    (at 142.5702 118.6434 330)
    (descr "3.0 x 2.0 x 2.0 mm Right Angle SMD LED, 10 degree viewing angle, APDA3020LSECK/J3-PF, http://www.kingbrightusa.com/images/catalog/SPEC/APDA3020LSECK-J3-PF.pdf")
    (tags "LED RA APDA3020LSECK KINGBRIGHT 3x2mm")
    (attr smd)
    (fp_text reference D1 (at 0 -1.8 150) (layer B.SilkS))
    (fp_text value LED (at 0 -3 150) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 150) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -1.5 0 330) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 330) (size 2 1) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /Prox_Out))
    (model ${KIPRJMOD}/RA_LED.pretty/APDA3020.STEP
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 146.685 117.348 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at -2.794 0 180) (layer F.SilkS))
    (fp_text value "100 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 PA7_PROBE_OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 157.48 101.6)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 2.54) (layer B.SilkS))
    (fp_text value RxD (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask)
      (net 24 PA2_RxD2))
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 147.32 101.6)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 2.54) (layer B.SilkS))
    (fp_text value TxD (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask)
      (net 23 PA1_TxD2))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 143.764 104.648 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 3.429 -0.127 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 /PA6B))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 PA6_PROBE_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 locked (layer B.Cu) (tedit 5E9886D3)
    (at 155.575 85.725)
    (fp_text reference J4 (at -1.905 -1.905) (layer B.SilkS))
    (fp_text value GND (at -0.1 -3.1) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 locked (layer B.Cu) (tedit 5E9886D3)
    (at 149.225 85.725)
    (fp_text reference J3 (at -1.905 -1.905) (layer B.SilkS))
    (fp_text value Prox_Out (at -0.1 -3.1) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 21 /Prox_Out))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 locked (layer B.Cu) (tedit 5E9886D3)
    (at 149.225 92.075)
    (fp_text reference J2 (at -1.905 -1.905) (layer B.SilkS))
    (fp_text value V_Prox (at -0.1 -3.1) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 11 +15V))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 locked (layer B.Cu) (tedit 5E9886D3)
    (at 155.575 92.075)
    (fp_text reference J1 (at -1.905 -1.905) (layer B.SilkS))
    (fp_text value VBATT (at -0.1 -3.1) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 33 /VIN))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 144.526 115.316 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -2.794 0 180) (layer F.SilkS))
    (fp_text value "100 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 PA5_ENA_PROX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 142.748 101.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.651) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 PA6_PROBE_IN))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.636 100.33 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value "4.7 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 PA4_PROX_IN))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 141.732 104.648 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 3.556 0 270) (layer F.SilkS))
    (fp_text value NC (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 /PA6B))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 149.86 106.045)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 3.175) (layer B.SilkS))
    (fp_text value Probe_Out (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask)
      (net 12 PA7_PROBE_OUT))
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 149.86 97.155)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at -2.54 1.905) (layer B.SilkS))
    (fp_text value Probe_In (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask)
      (net 17 PA6_PROBE_IN))
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 154.94 106.045)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 2.667) (layer B.SilkS))
    (fp_text value UPDI (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask)
      (net 30 /UPDI))
  )
  (module TestPoint:TestPoint_Pad_D2.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 154.94 97.155)
    (descr "SMD pad as test Point, diameter 2.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at 2.54 1.905) (layer B.SilkS))
    (fp_text value ENA_PROX (at 0 -2.25) (layer B.Fab))
    (fp_text user %R (at 0 2.15) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 2.5 2.5) (layers B.Cu B.Mask)
      (net 13 PA5_ENA_PROX))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 161.036 104.14 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.54 0.254 180) (layer F.SilkS))
    (fp_text value "33 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 +3V0))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 /UPDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.668 104.648 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 3.556 0 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 35 /TP1))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 /Q2BD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 159.004 104.14 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at 2.54 0.381) (layer F.SilkS))
    (fp_text value "4.7 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 /UPDI))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 PA0_UPDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 139.7 104.648 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -3.556 0.127 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 /Q2BD))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 /PA6B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 160.528 96.52 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value "20 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 AIN3_BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 162.56 96.52 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value "180 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 AIN3_BATT))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 +15V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 157.226 110.998)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 /Q1BG))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 +BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 158.496 113.538)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 1.778) (layer F.SilkS))
    (fp_text value 100k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 32 /Q1AG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TSOT-23-6_HandSoldering (layer F.Cu) (tedit 5A02FF57)
    (at 151.13 116.205)
    (descr "6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf")
    (tags "TSOT-23-6 MK06A TSOT-6 Hand-soldering")
    (attr smd)
    (fp_text reference Q2 (at 0 2.667) (layer F.SilkS))
    (fp_text value DMN2215UDM (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at 1.71 -0.95) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 /Q1BG))
    (pad 5 smd rect (at 1.71 0) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 4 smd rect (at 1.71 0.95) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 /Q2BD))
    (pad 3 smd rect (at -1.71 0.95) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 PA7_PROBE_OUT))
    (pad 2 smd rect (at -1.71 0) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 1 smd rect (at -1.71 -0.95) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 PA5_ENA_PROX))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TSOT-23-6_HandSoldering (layer F.Cu) (tedit 5A02FF57)
    (at 151.257 112.522 180)
    (descr "6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf")
    (tags "TSOT-23-6 MK06A TSOT-6 Hand-soldering")
    (attr smd)
    (fp_text reference Q1 (at -0.254 2.794) (layer F.SilkS))
    (fp_text value FDC6506P (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at 1.71 -0.95 180) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT))
    (pad 5 smd rect (at 1.71 0 180) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 /VIN))
    (pad 4 smd rect (at 1.71 0.95 180) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 +15V))
    (pad 3 smd rect (at -1.71 0.95 180) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 /Q1BG))
    (pad 2 smd rect (at -1.71 0 180) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 +BATT))
    (pad 1 smd rect (at -1.71 -0.95 180) (size 2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 /Q1AG))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.4 95.885 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 +3V0))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 152.4 93.98 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.175 0) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 +3V0))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 158.496 96.52 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value "100 nF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 AIN3_BATT))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 145.415 95.25 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 9 +3V0))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.16 95.25 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 +BATT))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 134.62 95.25 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value "10 uF" (at 0 2.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 +BATT))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 167.132 93.98)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 167.132 109.22)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 138.43 114.3)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 138.43 88.9)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.668 100.33 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -2.032 180) (layer F.SilkS))
    (fp_text value "1.2 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 PA4_PROX_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 166.1922 101.6)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference H5 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value "Poka Yoke Dowel" (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 167.132 97.536)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 3.048 -1.27) (layer F.SilkS))
    (fp_text value 180 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 29 /BLU))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 PB0_LED_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 171.45 104.648 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 1.016 4.318 180) (layer F.SilkS))
    (fp_text value 180 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 27 /RED))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 PB2_LED_B))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 171.45 98.552)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -0.889 7.874) (layer F.SilkS))
    (fp_text value 180 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 PB1_LED_G))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 28 /GRN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 162.56 91.948 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 1.016 1.651) (layer F.SilkS))
    (fp_text value "2.7 k" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at -0.97 0.745) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0926-1-15-20-75-14-11-0:LED_Kingbright_APFA2507_2.5x0.7mm_Horizontal locked (layer B.Cu) (tedit 5E98C459)
    (at 172.72 101.6 90)
    (descr "LED RGB, APFA2507, http://www.kingbrightusa.com/images/catalog/SPEC/APFA2507LQBDSEEZGKC.pdf")
    (tags "LED RGB APFA2507 KINGBRIGHT 2.5x0.7mm")
    (attr smd)
    (fp_text reference D7 (at 0 -2.54) (layer B.SilkS))
    (fp_text value APFA2507LQBDSEEZGKC (at 0 -3 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0 90) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 27 /RED))
    (pad 2 smd rect (at 1.5 0 90) (size 1 0.9) (layers B.Cu B.Paste B.Mask)
      (net 28 /GRN))
    (pad 4 smd rect (at -0.4 -0.45 90) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 +3V0))
    (pad 3 smd rect (at 0.4 -0.45 90) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 /BLU))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Kingbright_APFA3010_3x1.5mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/APFA2507.STEP
      (offset (xyz -1.25 0.25 -0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "043016 A\nCriterion MS\n6652 2020 04" (at 142.875 99.695) (layer B.SilkS))
  (gr_circle (center 152.4 101.6) (end 174.625 101.6) (layer Edge.Cuts) (width 0.254))
  (zone (net 20) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.54 78.74) (xy 129.54 124.46) (xy 175.26 124.46) (xy 175.26 78.74)
      )
    )
  )
  (zone (net 20) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 76.2) (xy 127 127) (xy 177.8 127) (xy 177.8 76.2)
      )
    )
  )
  (zone (net 9) (net_name +3V0) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.97 93.345) (xy 142.24 92.075) (xy 151.13 92.075) (xy 151.765 92.075) (xy 152.4 92.71)
        (xy 152.4 97.155) (xy 151.13 98.425) (xy 147.955 98.425) (xy 147.32 97.79) (xy 147.32 95.885)
        (xy 146.685 95.25) (xy 144.78 95.25) (xy 144.145 94.615) (xy 140.97 94.615)
      )
    )
  )
)
