(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 69)
    (zones 0)
    (modules 13)
    (nets 10)
  )
  (page A4)
  (title_block
    (date 2019-02-09)
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.4)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(J2-Pad3)")
  (net 4 "Net-(J2-Pad4)")
  (net 5 "Net-(J2-Pad2)")
  (net 6 +5V)
  (net 7 +3V3)
  (net 8 /Vout1)
  (net 9 /Vout2)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /Vout1)
    (add_net /Vout2)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.5 70.4 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -2.925 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 +5V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 131.5 70.4 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -2.825 -0.1 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 +3V3))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 163.225 64.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -2.525 0.25 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /Vout1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.675 64.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -2.475 0.25 90) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 /Vout2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 149.8 73.7 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 4.6 -0.1 90) (layer F.SilkS))
    (fp_text value LED_ALT (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical locked (layer B.Cu) (tedit 59FED5CC)
    (at 162 63 270)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J1 (at 5.25 -1.25) (layer B.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 1.27 -4.87 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -1.27 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Vout1))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Vout1))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical locked (layer B.Cu) (tedit 5C760175)
    (at 117.46 63 270)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J3 (at 5 -1.54 180) (layer B.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 1.27 -4.87 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -1.27 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Vout2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Vout2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 145.4 71.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0.1 -1.7) (layer F.SilkS))
    (fp_text value 330 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 +3V3))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5C75FDE4)
    (at 137 71.6)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 3.1 -3.1) (layer F.SilkS))
    (fp_text value " AZ1117CH-3.3TRG1" (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:USB_Micro_B_Female_10118194-0001LF (layer F.Cu) (tedit 5B07215D)
    (at 119.75 71.65 270)
    (descr http://portal.fciconnect.com/Comergent//fci/drawing/10118194.pdf)
    (fp_text reference J2 (at 3.75 -1.55 270) (layer F.SilkS))
    (fp_text value 10118194-0001LF (at 0 7 270) (layer F.Fab))
    (fp_text user %R (at 0 2.84 270) (layer F.Fab))
    (pad 3 smd rect (at 0 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at 0.65 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at 1.3 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.65 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -1.3 0 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad SH thru_hole oval (at 2.5 0 270) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole oval (at -2.5 0 270) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole oval (at -3.5 2.7 270) (size 1 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole oval (at 3.5 2.7 270) (size 1 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 156.7 74 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at -2.1 6.2 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Vout1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 125.5 74 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at -2.05 6.3 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Vout2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 162.4 70.5 90)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 90) (layer F.Fab) hide)
  )
  (gr_text 5V (at 123 73.7 180) (layer F.SilkS))
  (gr_text 3.3V (at 122.1 69 180) (layer F.SilkS))
  (gr_text 3.3V (at 153.4 68.9 180) (layer F.SilkS))
  (gr_text 5V (at 154.3 73.6 180) (layer F.SilkS))
  (gr_text + (at 161.9 61.5 90) (layer F.SilkS))
  (gr_text - (at 164.4 61.5 90) (layer F.SilkS))
  (gr_text - (at 119.9 61.5 90) (layer F.SilkS))
  (gr_text + (at 117.4 61.5 90) (layer F.SilkS))
  (gr_text "Copyright (C) 2019 John Winans\nhttps://github.com/johnwinans/2044-breadboard-power" (at 154.9 69.1) (layer B.SilkS))
  (gr_arc (start 123.5 65) (end 122 65) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 120.5 62.5) (end 122 62.5) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 117 62.5) (end 117 61) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 117 75) (end 115.5 75) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 165 75) (end 165 76.5) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 158.5 65) (end 158.5 66.5) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 165 62.5) (end 166.5 62.5) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_arc (start 161.5 62.5) (end 161.5 61) (angle -90) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 160 65) (end 160 62.5) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 123.5 66.5) (end 158.5 66.5) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 122 62.5) (end 122 65) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 120.5 61) (end 117 61) (layer Edge.Cuts) (width 0.4))
  (dimension 51 (width 0.3) (layer Dwgs.User)
    (gr_text "51.000 mm" (at 141 82.2) (layer Dwgs.User))
    (feature1 (pts (xy 115.5 76.714063) (xy 115.5 80.686421)))
    (feature2 (pts (xy 166.5 76.714063) (xy 166.5 80.686421)))
    (crossbar (pts (xy 166.5 80.1) (xy 115.5 80.1)))
    (arrow1a (pts (xy 115.5 80.1) (xy 116.626504 79.513579)))
    (arrow1b (pts (xy 115.5 80.1) (xy 116.626504 80.686421)))
    (arrow2a (pts (xy 166.5 80.1) (xy 165.373496 79.513579)))
    (arrow2b (pts (xy 166.5 80.1) (xy 165.373496 80.686421)))
  )
  (dimension 15.5 (width 0.3) (layer Dwgs.User)
    (gr_text "15.500 mm" (at 178.1 68.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 166.5 76.5) (xy 176.586421 76.5)))
    (feature2 (pts (xy 166.5 61) (xy 176.586421 61)))
    (crossbar (pts (xy 176 61) (xy 176 76.5)))
    (arrow1a (pts (xy 176 76.5) (xy 175.413579 75.373496)))
    (arrow1b (pts (xy 176 76.5) (xy 176.586421 75.373496)))
    (arrow2a (pts (xy 176 61) (xy 175.413579 62.126504)))
    (arrow2b (pts (xy 176 61) (xy 176.586421 62.126504)))
  )
  (gr_text "Copyright (C) 2019 John Winans" (at 143.6 75.6) (layer F.SilkS))
  (gr_text "2044-breadboard-power V3" (at 127.2 75.6) (layer F.SilkS))
  (gr_line (start 115.5 75) (end 115.5 62.5) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 165 76.5) (end 117 76.5) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 166.5 62.5) (end 166.5 75) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 161.5 61) (end 165 61) (layer Edge.Cuts) (width 0.4))
  (dimension 42 (width 0.3) (layer Dwgs.User)
    (gr_text "42.000 mm" (at 141 55.8) (layer Dwgs.User))
    (feature1 (pts (xy 162 60) (xy 162 57.313579)))
    (feature2 (pts (xy 120 60) (xy 120 57.313579)))
    (crossbar (pts (xy 120 57.9) (xy 162 57.9)))
    (arrow1a (pts (xy 162 57.9) (xy 160.873496 58.486421)))
    (arrow1b (pts (xy 162 57.9) (xy 160.873496 57.313579)))
    (arrow2a (pts (xy 120 57.9) (xy 121.126504 58.486421)))
    (arrow2b (pts (xy 120 57.9) (xy 121.126504 57.313579)))
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.75))
    (polygon
      (pts
        (xy 114.75 60.25) (xy 167.75 60) (xy 167.75 84.75) (xy 113.75 84)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.75))
    (polygon
      (pts
        (xy 167 60.6) (xy 115.2 60.4) (xy 114.5 77.8) (xy 167.3 77.6)
      )
    )
  )
)
