<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="102.87" y2="0" width="0" layer="20"/>
<wire x1="102.87" y1="0" x2="102.87" y2="22.86" width="0" layer="20"/>
<wire x1="102.87" y1="22.86" x2="0" y2="22.86" width="0" layer="20"/>
<wire x1="0" y1="22.86" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="con-conrad">
<description>&lt;b&gt;Conrad Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="736880-49">
<description>&lt;b&gt;Cinch Einbauprintbuchse&lt;/b&gt;, ( RCA Jack ) RM 7.5 x 10 mm&lt;p&gt;
Artikel-Nr.: 736880 - 49&lt;br&gt;
Source: http://www.produktinfo.conrad.com/datenblaetter/725000-749999/736880-da-01-de-Cinch-Einbaubuchse.pdf</description>
</package>
</packages>
</library>
<library name="fifo">
<description>&lt;b&gt;First In First Out Memories&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="1206">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="MINI-DIN6">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED-TRICOLOR-THROUGHHOLE">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microchip-new">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ASF">
<description>&lt;b&gt;CRYSTAL CLOCK OSCILLATORS&lt;/b&gt;&lt;p&gt;
5.0 Vdc or 3.3 Vdc - LOW PROFILE ULTRA MINIATURE CERAMIC SURFACE MOUNT&lt;br&gt;
Source: http://www.abracon.com/Oscillators/asf1-L-L1.pdf</description>
</package>
</packages>
</library>
<library name="memory-sst">
<description>SST Memory Devices</description>
<packages>
<package name="SO08-S2A">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
200 MIL BODY WIDTH (5.2MM X 8MM)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="DIL40" value="MEGA323-P">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="VIDEO" library="con-conrad" package="736880-49" value="736880-49"/>
<element name="IC4" library="fifo" package="DIL16" value="74232B">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R2" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R3" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R4" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R5" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R6" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R7" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="T1" library="transistor" package="TO92" value="2N3904"/>
<element name="T2" library="transistor" package="TO92" value="2N3904"/>
<element name="T3" library="transistor" package="TO92" value="2N3904"/>
<element name="T4" library="transistor" package="TO92" value="2N3904"/>
<element name="IC2" library="microchip-new" package="DIL14" value="PIC16F676P"/>
<element name="R8" library="SparkFun" package="1206" value=""/>
<element name="IC3" library="burr-brown" package="SOT223" value="REG1117-1V8">
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MPN" value="REG1117"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1097566"/>
</element>
<element name="C1" library="SparkFun" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="IC5" library="burr-brown" package="SOT223" value="REG1117-5V0">
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MPN" value="REG1117"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1097566"/>
</element>
<element name="C2" library="SparkFun" package="CPOL-RADIAL-100UF-25V" value=""/>
<element name="Q1" library="crystal" package="ASF" value="ASF1">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$1" library="SparkFun" package="MINI-DIN6" value="MINI-DIN6PTH"/>
<element name="LED1" library="SparkFun" package="LED3MM" value=""/>
<element name="R9" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="Q2" library="crystal" package="ASF" value="ASF1">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$2" library="SparkFun" package="LED-TRICOLOR-THROUGHHOLE" value="LED-TRICOLOR-THROUGHHOLE"/>
<element name="R10" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="S1" library="SparkFun" package="TACTILE-PTH" value=""/>
<element name="R11" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="U1" library="memory-sst" package="SO08-S2A" value="SST25VF064C-S3"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="11"/>
<contactref element="IC4" pad="8"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="VIDEO" pad="2"/>
<contactref element="IC2" pad="14"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="31"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="10"/>
<contactref element="IC4" pad="16"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="30"/>
<contactref element="IC5" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="4"/>
<contactref element="R9" pad="P$2"/>
<contactref element="Q2" pad="4"/>
<contactref element="Q2" pad="4"/>
<contactref element="U$1" pad="4"/>
<contactref element="R10" pad="P$1"/>
<contactref element="R11" pad="P$1"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R6" pad="P$1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="P$2"/>
<contactref element="R5" pad="P$1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$1"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$1"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$1"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="P$1"/>
<contactref element="T3" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="P$1"/>
<contactref element="T4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="IC4" pad="10"/>
<contactref element="T4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC4" pad="11"/>
<contactref element="T3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC4" pad="12"/>
<contactref element="T2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC4" pad="13"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="T4" pad="1"/>
<contactref element="T3" pad="1"/>
<contactref element="T2" pad="1"/>
<contactref element="T1" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="7"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="IC4" pad="5"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="IC4" pad="6"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$16">
<contactref element="IC4" pad="7"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="R8" pad="2"/>
<contactref element="VIDEO" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="IC4" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="IC4" pad="3"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="IC4" pad="15"/>
<contactref element="Q1" pad="3"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="IC2" pad="10"/>
<contactref element="IC4" pad="9"/>
</signal>
<signal name="N$20">
<contactref element="IC2" pad="12"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="N$22">
<contactref element="IC2" pad="11"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="N$24">
<contactref element="IC4" pad="14"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$25">
<contactref element="LED1" pad="A"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="N$28">
<contactref element="IC1" pad="28"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$30">
<contactref element="Q2" pad="3"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$31">
<contactref element="IC1" pad="18"/>
<contactref element="U$2" pad="GRN"/>
</signal>
<signal name="N$32">
<contactref element="IC1" pad="19"/>
<contactref element="U$2" pad="BLU"/>
</signal>
<signal name="N$33">
<contactref element="IC1" pad="20"/>
<contactref element="U$2" pad="RED"/>
</signal>
<signal name="N$34">
<contactref element="U$2" pad="GND"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="5"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="N$36">
<contactref element="IC1" pad="37"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="S1" pad="3"/>
<contactref element="R11" pad="P$2"/>
<contactref element="IC1" pad="9"/>
<contactref element="S1" pad="4"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="IC1" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$35">
<contactref element="IC1" pad="3"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$38">
<contactref element="IC1" pad="4"/>
<contactref element="U1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
