(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-2")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 81)
    (zones 0)
    (modules 4)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.8 0.65)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-PadA2)")
  (net 3 "Net-(J1-PadA3)")
  (net 4 "Net-(J1-PadA4)")
  (net 5 "Net-(J1-PadA5)")
  (net 6 "Net-(J1-PadA6)")
  (net 7 "Net-(J1-PadA7)")
  (net 8 "Net-(J1-PadA10)")
  (net 9 "Net-(J1-PadA8)")
  (net 10 "Net-(J1-PadA11)")
  (net 11 "Net-(J1-PadB2)")
  (net 12 "Net-(J1-PadB3)")
  (net 13 "Net-(J1-PadB5)")
  (net 14 "Net-(J1-PadB8)")
  (net 15 "Net-(J1-PadB10)")
  (net 16 "Net-(J1-PadB11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-PadA10)")
    (add_net "Net-(J1-PadA11)")
    (add_net "Net-(J1-PadA2)")
    (add_net "Net-(J1-PadA3)")
    (add_net "Net-(J1-PadA4)")
    (add_net "Net-(J1-PadA5)")
    (add_net "Net-(J1-PadA6)")
    (add_net "Net-(J1-PadA7)")
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB10)")
    (add_net "Net-(J1-PadB11)")
    (add_net "Net-(J1-PadB2)")
    (add_net "Net-(J1-PadB3)")
    (add_net "Net-(J1-PadB5)")
    (add_net "Net-(J1-PadB8)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 125.25 81 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x04_Female (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-PadA4)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-PadA7)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-PadA6)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.25 84)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-PadA5)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 132 84.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 5.1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J1-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module misc_footprints:E8124-010-01 (layer F.Cu) (tedit 5CD38F4A)
    (at 129.07 88.9)
    (descr E8124-010-01)
    (tags E8124-010-01)
    (attr smd)
    (fp_text reference J1 (at 0 3.3274) (layer F.SilkS))
    (fp_text value USB_C_Receptacle (at 0 8) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -3.6 0) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad A1 smd rect (at -2.75 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A2 smd rect (at -2.25 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-PadA2)"))
    (pad A3 smd rect (at -1.75 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-PadA3)"))
    (pad A4 smd rect (at -1.25 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadA4)"))
    (pad A5 smd rect (at -0.75 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-PadA5)"))
    (pad A6 smd rect (at -0.25 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-PadA6)"))
    (pad A7 smd rect (at 0.25 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-PadA7)"))
    (pad A8 smd rect (at 0.75 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-PadA8)"))
    (pad A9 smd rect (at 1.25 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadA4)"))
    (pad A10 smd rect (at 1.75 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-PadA10)"))
    (pad A11 smd rect (at 2.25 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-PadA11)"))
    (pad A12 smd rect (at 2.75 -1.91) (size 0.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B1 thru_hole circle (at 2.8 -0.7) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B2 thru_hole circle (at 2.4 0) (size 0.65 0.65) (drill 0.4) (layers *.Cu)
      (net 11 "Net-(J1-PadB2)"))
    (pad B3 thru_hole circle (at 1.6 0) (size 0.65 0.65) (drill 0.4) (layers *.Cu)
      (net 12 "Net-(J1-PadB3)"))
    (pad B4 thru_hole circle (at 1.2 -0.7) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-PadA4)"))
    (pad B5 thru_hole circle (at 0.8 0) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-PadB5)"))
    (pad B6 thru_hole circle (at 0.4 -0.7) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-PadA6)"))
    (pad B7 thru_hole circle (at -0.4 -0.7) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-PadA7)"))
    (pad B8 thru_hole circle (at -0.8 0) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-PadB8)"))
    (pad B9 thru_hole circle (at -1.2 -0.7) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-PadA4)"))
    (pad B10 thru_hole circle (at -1.6 0) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-PadB10)"))
    (pad B11 thru_hole circle (at -2.4 0) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-PadB11)"))
    (pad B12 thru_hole circle (at -2.8 -0.7) (size 0.65 0.65) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.27 -1.2) (size 0.9 1.8) (drill oval 0.5 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.27 -1.2) (size 0.9 1.8) (drill oval 0.5 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -6.125 4.85) (size 0.9 1.8) (drill oval 0.5 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 6.125 4.85) (size 0.9 1.8) (drill oval 0.5 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole oval (at 3.6 0) (size 0.8 0.65) (drill oval 0.8 0.65) (layers *.Cu))
    (model :3d:E8124-010-01.stp
      (offset (xyz 0 -3.269999950889528 0.8499999872342808))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_arc (start 135.2 79.9) (end 135.7 79.9) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 122.9 79.9) (end 122.9 79.4) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 122.9 94.7) (end 122.4 94.7) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.9 90.2) (end 124.9 89.7) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 133.3 90.2) (end 133.8 90.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 135.2 94.6) (end 135.2 95.1) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.4 95.2) (end 122.9 95.2) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 124.4 90.2) (end 124.4 95.2) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.3 89.7) (end 124.9 89.7) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.8 95.1) (end 133.8 90.2) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 135.2 95.1) (end 133.8 95.1) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 135.7 79.9) (end 135.7 94.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 122.9 79.4) (end 135.2 79.4) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 122.4 94.7) (end 122.4 79.9) (layer Edge.Cuts) (width 0.2))
  (gr_text CC2 (at 132 85.5) (layer F.SilkS))
  (gr_text CC1 (at 126 85.5) (layer F.SilkS))
  (gr_text "G + - V" (at 129 83.5) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.2 79.2) (xy 135.8 79.2) (xy 135.9 95.4) (xy 122.2 95.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.1 79.2) (xy 135.9 79.3) (xy 136 95.4) (xy 122.2 95.3)
      )
    )
  )
)
