(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 44)
    (zones 0)
    (modules 12)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D3-Pad2)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D5-Pad1)")
  (net 6 /A)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D5-Pad1)")
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 82.55 78.1625 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer B.Fab))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 6 /A))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 97.6122 78.16 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer B.Fab))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 4 "Net-(D3-Pad1)"))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 5 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 90.056 78.16 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer B.Fab))
    (fp_text value R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.222222)
      (net 3 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AlexGlobal:PowerPad (layer F.Cu) (tedit 5F5F1632)
    (at 98.2 79.7)
    (fp_text reference U3 (at 0 0.5) (layer F.Fab))
    (fp_text value SolderPad (at 0 -0.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 1 4) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 4) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1 2) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 2) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 3) (size 1.524 1.524) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
  )
  (module AlexGlobal:PowerPad (layer F.Cu) (tedit 5F5F1632)
    (at 90.6 79.7)
    (fp_text reference U2 (at 0 0.5) (layer B.Fab))
    (fp_text value SolderPad (at 0 -0.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 1 4) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 4) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1 2) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 2) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 3) (size 1.524 1.524) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module AlexGlobal:PowerPad (layer F.Cu) (tedit 5F5F1632)
    (at 83.1 79.7)
    (fp_text reference U1 (at 0 0.5) (layer B.Fab))
    (fp_text value SolderPad (at 0 -0.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 1 4) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 4) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1 2) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 2) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 3) (size 1.524 1.524) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 /A))
  )
  (module LED_SMD:LED_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 101.37 78.82 180)
    (descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D6 (at 0 -2.28) (layer B.Fab))
    (fp_text value LED (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(D5-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 /A))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 101.4 75.2)
    (descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D5 (at 0 -2.28) (layer B.Fab))
    (fp_text value LED (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 /A))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 93.81 75.2)
    (descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0 -2.28) (layer B.Fab))
    (fp_text value LED (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 "Net-(D3-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 93.7895 78.82 180)
    (descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at 0 -2.28) (layer B.Fab))
    (fp_text value LED (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 86.258 78.8225 180)
    (descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -2.28) (layer B.Fab))
    (fp_text value LED (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 86.3 75.2)
    (descr "LED SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -2.28) (layer B.Fab))
    (fp_text value LED (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text v1.1 (at 84.7344 79.6036) (layer B.SilkS))
  (gr_text "& t.smeekes" (at 88.9 74.93) (layer B.SilkS))
  (gr_text a.fedorov (at 97.79 74.93) (layer B.SilkS))
  (gr_text "ESC Tester" (at 92.6 78.1) (layer B.SilkS))
  (gr_line (start 80.7 72.6) (end 80.7 72.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.2 72.6) (end 80.7 72.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.2 84.7) (end 104.2 72.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 80.7 84.7) (end 104.2 84.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 80.7 72.9) (end 80.7 84.7) (layer Edge.Cuts) (width 0.05))
  (gr_text C (at 101.5 82.8) (layer F.SilkS))
  (gr_text B (at 93.810714 82.8) (layer F.SilkS))
  (gr_text A (at 86.3 82.8) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.9 85.3) (xy 80.2 85.3) (xy 80.2 72.1) (xy 104.9 72.1)
      )
    )
  )
)
