<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="3.81" y1="11.43" x2="100" y2="11.43" width="0" layer="20"/>
<wire x1="100" y1="11.43" x2="100" y2="71.11" width="0" layer="20"/>
<wire x1="100" y1="71.11" x2="3.81" y2="71.11" width="0" layer="20"/>
<wire x1="3.81" y1="71.11" x2="3.81" y2="11.43" width="0" layer="20"/>
<text>5V Regulator
(PDQ30-Q24-S5-D)</text>
<text>LED Driver
( RCD-24-1.00)</text>
<text>BAT+</text>
<text>BAT-</text>
<text>BAT-</text>
<text>BAT+</text>
<text>5V+</text>
<text>0V-</text>
<text>DIM</text>
<text>TRM</text>
<text>REM</text>
<text>PWM</text>
<text>JCK</text>
<text>D3</text>
<text>LED+</text>
<text>LED+</text>
<text>LED-</text>
<text>LED-</text>
<text>5V</text>
<text>5V</text>
<text>0V</text>
<text>0V</text>
<text>B+</text>
<text>B+</text>
<text>B-</text>
<text>B-</text>
<text>0V</text>
<text>5V</text>
<text>0V</text>
<text>5V</text>
<text>B-</text>
<text>B+</text>
<text>B-</text>
<text>B+</text>
<text>5V+</text>
<text>5V+</text>
<text>0V</text>
<text>0V</text>
<text>LED-</text>
<text>LED-</text>
<text>LED+</text>
<text>LED+</text>
<text>5V Regulator
(PDQ30-Q24-S5-D)</text>
<text>  1 
+Vin</text>
<text>  2 
-Vin</text>
<text>     6 
Remote</text>
<text>     3 
+Vout</text>
<text>     5 
-Vout</text>
<text>   4 
Trim</text>
<text>LED Driver
( RCD-24-1.00)</text>
<text>+Vin</text>
<text>-Vin</text>
<text>DIM</text>
<text>PWM</text>
<text>+Vout</text>
<text>-Vout</text>
<text>BAT+</text>
<text>BAT-</text>
<text>BAT+</text>
<text>BAT-</text>
<text>DIM</text>
<text>TRM</text>
<text>REM</text>
<text>PWM</text>
<text>JCK</text>
<text>0V-</text>
<text>5V+</text>
<text>BAT+</text>
<text>BAT-</text>
<text>D3</text>
<hole x="6.35" y="13.97" drill="2.2"/>
<hole x="6.35" y="68.58" drill="2.2"/>
<hole x="97.79" y="68.58" drill="2.2"/>
<hole x="97.79" y="13.97" drill="2.2"/>
</plain>
<libraries>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DCJ0303">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt; Pad shape changed to LONG 2007.07.26&lt;p&gt;
Source: DCJ0303.pdf</description>
</package>
</packages>
</library>
<library name="con-jst-vh">
<description>&lt;b&gt;JST Connectors&lt;/b&gt; - VH 3.96 MM Series&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2016, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="B2P-VH">
<description>&lt;b&gt;HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-termi-block">
<description>&lt;b&gt;AMP/Tyco TERMI-BLOCK Connectors, 5mm&lt;/b&gt;&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="796644-2">
<description>&lt;b&gt;Connector Right Angle&lt;/b&gt;&lt;p&gt; 
pitch 5 mm</description>
</package>
</packages>
</library>
<library name="recom-international">
<description>&lt;b&gt;RECOM POWER SOLUTIONS&lt;/b&gt;&lt;p&gt;
Constant Current Output, Power LED Driver&lt;br&gt;
http://www.recom-international.com&lt;p&gt;
&lt;author&gt;Autor librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RCD-24/W/X3">
<description>&lt;b&gt;DC/DC Converter&lt;/b&gt; RCD.24 Series /W/X3&lt;p&gt;
Source: http://www.recom-international.com/pdf/Innoline-2008/RCD-24.pdf</description>
</package>
</packages>
</library>
<library name="con-headers-jp">
<description>&lt;b&gt;Male(J), Female(P) and Pin Headers&lt;/b&gt;&lt;p&gt;Version 1.02 - 03/10/2009&lt;p&gt;
This library is a collection of various pin headers and AMP, Molex and 3M board-to-board connectors. 
This library assumes the notion of JACKS(male) and PLUGS(female) as represented by the J and P symbols.
Standard male/female pin header types are available in common 0.1" and 2 mm pitch types with alternate mirrored footprints as well.
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="DIL-100-2X16_M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - MIRRORED 0.1"</description>
</package>
</packages>
</library>
<library name="PDQ30-Q24-S5-D">
<packages>
<package name="PDQ30-Q24-S5-D">
</package>
</packages>
</library>
<library name="con-amp">
<description>&lt;b&gt;AMP Connectors&lt;/b&gt;&lt;p&gt;
RJ45 Jack connectors&lt;br&gt;
 Based on the previous libraris:
 &lt;ul&gt;
 &lt;li&gt;amp.lbr
 &lt;li&gt;amp-j.lbr
 &lt;li&gt;amp-mta.lbr
 &lt;li&gt;amp-nlok.lbr
 &lt;li&gt;amp-sim.lbr
 &lt;li&gt;amp-micro-match.lbr
 &lt;/ul&gt;
 Sources :
 &lt;ul&gt;
 &lt;li&gt;Catalog 82066 Revised 11-95 
 &lt;li&gt;Product Guide 296785 Rev. 8-99
 &lt;li&gt;Product Guide CD-ROM 1999
 &lt;li&gt;www.amp.com
 &lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="USB">
<description>&lt;b&gt;USB connector&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="16.8V-2.1MM" library="con-jack" package="DCJ0303" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="BATT-PACK" library="con-jst-vh" package="B2P-VH" value="B2P-VH">
<attribute name="LABEL" value=""/>
</element>
<element name="LED" library="con-amp-termi-block" package="796644-2" value="796644-2"/>
<element name="LED-DRIVER" library="recom-international" package="RCD-24/W/X3" value="RCD-24-0.30/W/X3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="LED2" library="con-amp-termi-block" package="796644-2" value="796644-2"/>
<element name="P1" library="con-headers-jp" package="DIL-100-2X16_M" value="M-2X16-DIL-100_M"/>
<element name="PWR-16.8V" library="con-amp-termi-block" package="796644-2" value="796644-2"/>
<element name="PWR1-5V" library="con-amp-termi-block" package="796644-2" value="796644-2"/>
<element name="PWR2-16.8V1" library="con-amp-termi-block" package="796644-2" value="796644-2"/>
<element name="PWR2-5V" library="con-amp-termi-block" package="796644-2" value="796644-2"/>
<element name="RASPI-5V-REG" library="PDQ30-Q24-S5-D" package="PDQ30-Q24-S5-D" value="PDQ30-Q24-S5-D"/>
<element name="X1" library="con-amp" package="USB" value=""/>
<element name="X2" library="con-amp" package="USB" value=""/>
</elements>
<signals>
<signal name="BAT+">
<contactref element="16.8V-2.1MM" pad="3"/>
<contactref element="BATT-PACK" pad="1"/>
<contactref element="RASPI-5V-REG" pad="+VIN"/>
<contactref element="PWR2-16.8V1" pad="1"/>
<contactref element="PWR-16.8V" pad="1"/>
<contactref element="LED-DRIVER" pad="1"/>
<contactref element="P1" pad="7"/>
<contactref element="P1" pad="8"/>
<contactref element="P1" pad="9"/>
<contactref element="P1" pad="10"/>
</signal>
<signal name="BAT-">
<contactref element="16.8V-2.1MM" pad="1"/>
<contactref element="BATT-PACK" pad="2"/>
<contactref element="PWR2-16.8V1" pad="2"/>
<contactref element="PWR-16.8V" pad="2"/>
<contactref element="LED-DRIVER" pad="4"/>
<contactref element="RASPI-5V-REG" pad="-VIN"/>
<contactref element="P1" pad="1"/>
<contactref element="P1" pad="2"/>
<contactref element="P1" pad="4"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="LED+">
<contactref element="LED-DRIVER" pad="6"/>
<contactref element="LED" pad="1"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="LED-">
<contactref element="LED-DRIVER" pad="5"/>
<contactref element="LED" pad="2"/>
<contactref element="LED2" pad="2"/>
</signal>
<signal name="5VOUT+">
<contactref element="RASPI-5V-REG" pad="+VOUT"/>
<contactref element="PWR2-5V" pad="1"/>
<contactref element="PWR1-5V" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="P1" pad="13"/>
<contactref element="P1" pad="14"/>
<contactref element="P1" pad="15"/>
<contactref element="P1" pad="16"/>
</signal>
<signal name="5VOUT-">
<contactref element="X1" pad="4"/>
<contactref element="RASPI-5V-REG" pad="-VOUT"/>
<contactref element="X2" pad="4"/>
<contactref element="PWR1-5V" pad="2"/>
<contactref element="PWR2-5V" pad="2"/>
<contactref element="P1" pad="19"/>
<contactref element="P1" pad="20"/>
<contactref element="P1" pad="22"/>
<contactref element="P1" pad="21"/>
</signal>
<signal name="TRIM">
<contactref element="P1" pad="31"/>
<contactref element="RASPI-5V-REG" pad="TRIM"/>
</signal>
<signal name="REMOTE">
<contactref element="RASPI-5V-REG" pad="REMOTE"/>
<contactref element="P1" pad="32"/>
</signal>
<signal name="DIM">
<contactref element="LED-DRIVER" pad="2"/>
<contactref element="P1" pad="29"/>
</signal>
<signal name="PWM">
<contactref element="LED-DRIVER" pad="3"/>
<contactref element="P1" pad="30"/>
</signal>
<signal name="N$13">
<contactref element="P1" pad="11"/>
<contactref element="P1" pad="12"/>
</signal>
<signal name="N$16">
<contactref element="P1" pad="17"/>
<contactref element="P1" pad="18"/>
</signal>
<signal name="N$1">
<contactref element="P1" pad="23"/>
<contactref element="P1" pad="24"/>
</signal>
<signal name="N$2">
<contactref element="P1" pad="5"/>
<contactref element="P1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="P1" pad="25"/>
<contactref element="P1" pad="26"/>
<contactref element="16.8V-2.1MM" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="P1" pad="27"/>
<contactref element="P1" pad="28"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
