(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 235)
    (zones 0)
    (modules 31)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (trace_clearance 0.1778)
    (zone_clearance 0.4572)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8128 0.4064)
    (user_via 1.016 0.508)
    (user_via 1.651 1.016)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4732 2.10058)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 125.73 116.84)
    (grid_origin 125.73 116.84)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5.0V)
  (net 3 /TOP_SDA)
  (net 4 /TOP_SCL)
  (net 5 /XRES)
  (net 6 /DEBUG_TX)
  (net 7 /DEBUG_RX)
  (net 8 /SWD_DATA)
  (net 9 /SWD_CLK)
  (net 10 +3.3V)
  (net 11 "Net-(C1-Pad1)")
  (net 12 "Net-(C2-Pad1)")
  (net 13 "Net-(D1-Pad2)")
  (net 14 "Net-(FB1-Pad1)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 "Net-(J1-Pad3)")
  (net 17 "Net-(J1-Pad2)")
  (net 18 "Net-(J1-Pad6)")
  (net 19 "Net-(P2-Pad1)")
  (net 20 "Net-(R1-Pad2)")
  (net 21 "Net-(R2-Pad2)")
  (net 22 "Net-(P4-Pad4)")
  (net 23 "Net-(P4-Pad2)")
  (net 24 "Net-(TP6-Pad1)")
  (net 25 "Net-(TP7-Pad1)")
  (net 26 "Net-(TP8-Pad1)")
  (net 27 "Net-(TP9-Pad1)")
  (net 28 "Net-(TP10-Pad1)")
  (net 29 "Net-(TP11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.2032)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net +5.0V)
    (add_net /DEBUG_RX)
    (add_net /DEBUG_TX)
    (add_net /SWD_CLK)
    (add_net /SWD_DATA)
    (add_net /TOP_SCL)
    (add_net /TOP_SDA)
    (add_net /XRES)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(FB1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(TP10-Pad1)")
    (add_net "Net-(TP11-Pad1)")
    (add_net "Net-(TP6-Pad1)")
    (add_net "Net-(TP7-Pad1)")
    (add_net "Net-(TP8-Pad1)")
    (add_net "Net-(TP9-Pad1)")
  )
  (module t_logos:Thales_15x2_SLK (layer B.Cu) (tedit 0)
    (at 135.382 106.934 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 131.445 104.775)
    (fp_text reference TP12 (at 0 1.651) (layer F.SilkS) hide)
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 154.305 95.25)
    (fp_text reference TP11 (at -2.413 0.635) (layer F.SilkS))
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(TP11-Pad1)"))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 142.875 104.775)
    (fp_text reference TP10 (at -0.508 2.54 90) (layer F.SilkS))
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "Net-(TP10-Pad1)"))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 150.495 104.775)
    (fp_text reference TP9 (at 0.127 2.159 90) (layer F.SilkS))
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(TP9-Pad1)"))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 147.955 104.775)
    (fp_text reference TP8 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "Net-(TP8-Pad1)"))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 140.335 104.775)
    (fp_text reference TP7 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "Net-(TP7-Pad1)"))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 154.305 97.79)
    (fp_text reference TP6 (at 2.286 0.254) (layer F.SilkS))
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "Net-(TP6-Pad1)"))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 154.305 100.33)
    (fp_text reference TP5 (at 0 1.651) (layer F.SilkS) hide)
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 145.415 104.775)
    (fp_text reference TP4 (at 0 2.286 90) (layer F.SilkS) hide)
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 157.734 105.41)
    (fp_text reference TP3 (at 0 1.651) (layer F.SilkS) hide)
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 +5.0V))
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 137.795 104.775)
    (fp_text reference TP2 (at 0.127 2.667 90) (layer F.SilkS) hide)
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 +3.3V))
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 161.29 99.187 90)
    (descr "SMT resistor, 0603")
    (fp_text reference R5 (at 0 -1.651 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P4-Pad2)"))
    (pad 1 smd rect (at 0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /TOP_SDA))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 163.83 99.187 90)
    (descr "SMT resistor, 0603")
    (fp_text reference R4 (at -0.127 1.651 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P4-Pad4)"))
    (pad 1 smd rect (at 0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /TOP_SCL))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 128.905 86.36 90)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (fp_text reference P6 (at -2.159 -2.032 180) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 4.385 12.43 90) (layer F.Fab))
    (fp_text user %R (at 2.77 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SWD_DATA))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /SWD_CLK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /XRES))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +3.3V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 158.75 86.36 90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference P5 (at 0.127 -3.175 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 4.385 9.89 90) (layer F.Fab))
    (fp_text user %R (at 2.77 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /TOP_SCL))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /TOP_SDA))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 161.29 105.41 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference P4 (at -2.667 1.27 180) (layer F.SilkS))
    (fp_text value 4x4_header (at 1.27 4.87 90) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27) (layer F.Fab))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P4-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5.0V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5.0V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_qfn:QFN-16_4mm (layer F.Cu) (tedit 5F7C7D7C)
    (at 149.225 99.695 180)
    (attr smd)
    (fp_text reference U1 (at -3.175 -3.556 180) (layer F.SilkS))
    (fp_text value FT230X (at -0.635 0) (layer F.SilkS) hide)
    (pad 17 smd rect (at 0 0 180) (size 2.4 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.975 -2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(TP9-Pad1)"))
    (pad 15 smd rect (at -0.325 -2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /DEBUG_RX))
    (pad 14 smd rect (at 0.325 -2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(TP8-Pad1)"))
    (pad 13 smd rect (at 0.975 -2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 2.1 -0.975 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(TP10-Pad1)"))
    (pad 11 smd rect (at 2.1 -0.325 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(TP7-Pad1)"))
    (pad 10 smd rect (at 2.1 0.325 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C2-Pad1)"))
    (pad 9 smd rect (at 2.1 0.975 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (pad 8 smd rect (at 0.975 2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 0.325 2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R1-Pad2)"))
    (pad 6 smd rect (at -0.325 2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R2-Pad2)"))
    (pad 5 smd rect (at -0.975 2.1 180) (size 0.35 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(TP11-Pad1)"))
    (pad 4 smd rect (at -2.1 0.975 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(TP6-Pad1)"))
    (pad 3 smd rect (at -2.1 0.325 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.1 -0.325 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 /DEBUG_TX))
    (pad 1 smd rect (at -2.1 -0.975 180) (size 0.8 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (model "${MY_LIBS}/Sketchup Models/3d/QFN-16_4mm.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_misc:TP50 (layer F.Cu) (tedit 5BAD3C95)
    (at 154.305 92.71)
    (fp_text reference TP1 (at 0 -1.524) (layer F.SilkS))
    (fp_text value TEST_POINT (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad1)"))
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 144.145 86.36 90)
    (descr "SMT resistor, 0603")
    (fp_text reference R3 (at -0.254 -1.651 180) (layer F.SilkS))
    (fp_text value "0 Ohm" (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 149.987 93.599 90)
    (descr "SMT resistor, 0603")
    (fp_text reference R2 (at 0 1.651 180) (layer F.SilkS))
    (fp_text value 27 (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R2-Pad2)"))
    (pad 1 smd rect (at 0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad3)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0603 (layer F.Cu) (tedit 5BB76B6F)
    (at 148.59 93.599 90)
    (descr "SMT resistor, 0603")
    (fp_text reference R1 (at 0 -1.651 180) (layer F.SilkS))
    (fp_text value 27 (at 0 0.9652 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at 0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_connectors:Header5_254 (layer F.Cu) (tedit 5F63AC0B)
    (at 128.905 92.71)
    (fp_text reference P3 (at -1.778 4.572) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -0.5) (layer F.Fab))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /SWD_DATA))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /SWD_CLK))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /XRES))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 +3.3V))
    (model ${T_LIBS}/3d/t_connectors/022112052.stp
      (offset (xyz 5.08 0 1.6256))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module t_connectors:Header4_254 (layer F.Cu) (tedit 5F63AD14)
    (at 158.75 92.71)
    (fp_text reference P2 (at -3.048 -3.429) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -0.5) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /TOP_SCL))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /TOP_SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad1)"))
    (model ${T_LIBS}/3d/t_connectors/022112042.stp
      (offset (xyz 3.81 0 1.651))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module t_USB:conn_usb_B_micro_smd (layer B.Cu) (tedit 6050B333)
    (at 149.225 85.725)
    (descr "USB B micro SMD connector, Molex P/N 47346-0001")
    (fp_text reference J1 (at 5.334 1.143) (layer B.SilkS))
    (fp_text value USB_micro-B (at 0 4.0005) (layer B.SilkS) hide)
    (pad 5 smd rect (at 1.30048 2.65938) (size 0.44958 1.37922) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65024 2.65938) (size 0.44958 1.37922) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 2.65938) (size 0.44958 1.37922) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.65024 2.65938) (size 0.44958 1.37922) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.30048 2.65938) (size 0.44958 1.37922) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(FB1-Pad1)"))
    (pad "" smd rect (at -2.46126 2.2987) (size 1.4732 2.10058) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 2.46126 2.2987) (size 1.4732 2.10058) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -2.91338 0) (size 2.3749 1.89738) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 2.91338 0) (size 2.3749 1.89738) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 0.8382 0) (size 1.17348 1.89738) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -0.8382 0) (size 1.17348 1.89738) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (model ${T_LIBS}/3d/t_USB/10118192-002lfc.stp
      (offset (xyz -98 3 -0.4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_passive_smd:fb_0805 (layer F.Cu) (tedit 5C1562BE)
    (at 145.034 91.186)
    (descr "SMT capacitor, 0805")
    (fp_text reference FB1 (at -2.921 0) (layer F.SilkS))
    (fp_text value Ferrite_Bead1 (at 0 1.3462) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0) (layer F.Fab))
    (fp_text user %R (at -0.315 0.1) (layer F.CrtYd))
    (pad 2 smd rect (at -0.95 0) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 0.95 0) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(FB1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/FB_0805.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_so:SOD-123 (layer F.Cu) (tedit 5C1BD3D0)
    (at 144.145 95.25 90)
    (fp_text reference D1 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value BAV3004 (at 0.0635 1.8415 90) (layer F.Fab))
    (fp_text user %R (at 0.4445 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at 2.025 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2.025 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C2-Pad1)"))
    (model ${T_LIBS}/3d/t_sot/D_SOD-123.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_1210 (layer F.Cu) (tedit 5C1BCADF)
    (at 140.97 99.695 180)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at 0.762 -2.413) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C2-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/C_1210.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 144.78 100.33 90)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C2 (at -2.413 -0.889 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C2-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0603 (layer F.Cu) (tedit 5CF041F7)
    (at 146.05 95.885 270)
    (descr "SMT resistor, 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.016 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0.0635 90) (layer F.Fab))
    (pad 2 smd rect (at -0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.75 0 270) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0603.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_connectors:FPC_CONN_20_52893-2095 (layer F.Cu) (tedit 540EF72C)
    (at 149.225 113.03)
    (fp_text reference P1 (at 9.779 0) (layer F.SilkS))
    (fp_text value CONN_FFC_20 (at 0.5 1.4) (layer F.SilkS) hide)
    (pad 22 smd rect (at 7.4 0) (size 1.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at -7.4 0) (size 1.6 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 4.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5.0V))
    (pad 19 smd rect (at 4.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5.0V))
    (pad 18 smd rect (at 3.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 3.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 2.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /TOP_SDA))
    (pad 15 smd rect (at 2.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /TOP_SCL))
    (pad 14 smd rect (at 1.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 1.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /XRES))
    (pad 12 smd rect (at 0.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /DEBUG_TX))
    (pad 11 smd rect (at 0.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /DEBUG_RX))
    (pad 10 smd rect (at -0.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /SWD_DATA))
    (pad 9 smd rect (at -0.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /SWD_CLK))
    (pad 8 smd rect (at -1.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -1.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 +3.3V))
    (pad 6 smd rect (at -2.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 +3.3V))
    (pad 5 smd rect (at -2.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -3.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.25 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.75 -3.15) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${T_LIBS}/3d/t_connectors/52893-2095.wrl
      (offset (xyz 0 2.285999965667724 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (dimension 33.02 (width 0.15) (layer Dwgs.User)
    (gr_text "1.3000 in" (at 119.35 100.33 90) (layer Dwgs.User))
    (feature1 (pts (xy 125.73 83.82) (xy 120.063579 83.82)))
    (feature2 (pts (xy 125.73 116.84) (xy 120.063579 116.84)))
    (crossbar (pts (xy 120.65 116.84) (xy 120.65 83.82)))
    (arrow1a (pts (xy 120.65 83.82) (xy 121.236421 84.946504)))
    (arrow1b (pts (xy 120.65 83.82) (xy 120.063579 84.946504)))
    (arrow2a (pts (xy 120.65 116.84) (xy 121.236421 115.713496)))
    (arrow2b (pts (xy 120.65 116.84) (xy 120.063579 115.713496)))
  )
  (dimension 44.45 (width 0.15) (layer Dwgs.User)
    (gr_text "1.7500 in" (at 147.955 122.585) (layer Dwgs.User))
    (feature1 (pts (xy 170.18 116.84) (xy 170.18 121.871421)))
    (feature2 (pts (xy 125.73 116.84) (xy 125.73 121.871421)))
    (crossbar (pts (xy 125.73 121.285) (xy 170.18 121.285)))
    (arrow1a (pts (xy 170.18 121.285) (xy 169.053496 121.871421)))
    (arrow1b (pts (xy 170.18 121.285) (xy 169.053496 120.698579)))
    (arrow2a (pts (xy 125.73 121.285) (xy 126.856504 121.871421)))
    (arrow2b (pts (xy 125.73 121.285) (xy 126.856504 120.698579)))
  )
  (gr_text "Battery Adapter \nProgramming \nHeader" (at 127.635 112.776) (layer F.SilkS))
  (gr_text "Battery Adapter \nProgramming Header" (at 135.001 109.728) (layer B.SilkS))
  (gr_text DRM (at 138.303 112.268) (layer B.SilkS))
  (gr_text 03/16/2021 (at 135.001 113.919) (layer B.SilkS))
  (gr_text "SCL\n" (at 164.084 97.028) (layer F.SilkS))
  (gr_text "SDA\n" (at 160.782 97.028) (layer F.SilkS))
  (gr_text VTARG (at 129.032 98.679 90) (layer F.SilkS))
  (gr_text GND (at 131.445 98.044 90) (layer F.SilkS))
  (gr_text DATA (at 138.049 98.298 90) (layer F.SilkS))
  (gr_text "CLK\n" (at 136.144 97.917 90) (layer F.SilkS))
  (gr_text XRES (at 133.985 98.298 90) (layer F.SilkS))
  (gr_text +5V (at 157.607 107.315) (layer F.SilkS))
  (gr_text +3.3V (at 137.795 107.95 90) (layer F.SilkS))
  (gr_text GND (at 131.445 106.553) (layer F.SilkS))
  (gr_text GND (at 145.415 107.315 90) (layer F.SilkS))
  (gr_text GND (at 156.718 100.33) (layer F.SilkS))
  (gr_line (start 125.73 116.84) (end 125.73 83.82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.18 116.84) (end 125.73 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.18 83.82) (end 170.18 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 83.82) (end 170.18 83.82) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.545 116.205) (xy 126.365 116.205) (xy 126.365 84.455) (xy 169.545 84.455)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 10)
    (connect_pads yes (clearance 0.4572))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.545 116.205) (xy 126.365 116.205) (xy 126.365 84.455) (xy 169.545 84.455)
      )
    )
  )
  (zone (net 18) (net_name "Net-(J1-Pad6)") (layer B.Cu) (hatch edge 0.508)
    (priority 20)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.21 88.9) (xy 141.605 88.9) (xy 141.605 84.455) (xy 156.21 84.455)
      )
    )
  )
)
