(kicad_pcb (version 20171130) (host pcbnew "(6.0.0-rc1-dev-1614-ge850a482d)")
  (general
    (thickness 1.6)
    (drawings 126)
    (tracks 942)
    (zones 0)
    (modules 54)
    (nets 97)
  )
  (page A4)
  (layers
    (0 Top signal)
    (1 GND power hide)
    (2 PWR power hide)
    (31 Bottom signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (trace_clearance 0.1524)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.1)
    (edge_width 0.508)
    (segment_width 0.1778)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.635 0.635)
    (mod_text_width 0.127)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 /USB-)
  (net 2 /USB+)
  (net 3 "Net-(J1-Pad4)")
  (net 4 GND)
  (net 5 +3V3)
  (net 6 VBAT)
  (net 7 /~RESET)
  (net 8 /LED1)
  (net 9 /SWCLK)
  (net 10 /XTAL1)
  (net 11 /XTAL2)
  (net 12 /AREF)
  (net 13 "Net-(J3-Pad1)")
  (net 14 SD_CS)
  (net 15 MOSI)
  (net 16 SCK)
  (net 17 MISO)
  (net 18 "Net-(J3-Pad8)")
  (net 19 "Net-(J3-PadSW_T)")
  (net 20 "Net-(J3-PadDET_T)")
  (net 21 /DTR)
  (net 22 /SWDIO)
  (net 23 DAC0)
  (net 24 AIN6)
  (net 25 AIN7)
  (net 26 AIN8)
  (net 27 AIN9)
  (net 28 SCL)
  (net 29 DAC1)
  (net 30 SDA)
  (net 31 D19)
  (net 32 D20)
  (net 33 D31)
  (net 34 D35)
  (net 35 D36)
  (net 36 D37)
  (net 37 D38)
  (net 38 D41)
  (net 39 D42)
  (net 40 D43)
  (net 41 D44)
  (net 42 D49)
  (net 43 D50)
  (net 44 D59)
  (net 45 D60)
  (net 46 D64)
  (net 47 "Net-(U3-Pad17)")
  (net 48 "Net-(U3-Pad18)")
  (net 49 "Net-(U3-Pad19)")
  (net 50 "Net-(U3-Pad20)")
  (net 51 "Net-(U3-Pad21)")
  (net 52 "Net-(U3-Pad22)")
  (net 53 IO15)
  (net 54 "Net-(U3-Pad24)")
  (net 55 IO34)
  (net 56 IO35)
  (net 57 IO32)
  (net 58 IO33)
  (net 59 IO25)
  (net 60 IO26)
  (net 61 IO27)
  (net 62 IO21)
  (net 63 IO17)
  (net 64 IO16)
  (net 65 IO4)
  (net 66 "Net-(U5-Pad4)")
  (net 67 /EN)
  (net 68 IO39)
  (net 69 IO36)
  (net 70 VUSB)
  (net 71 /VBAT_MES)
  (net 72 /PROG)
  (net 73 ~)
  (net 74 "Net-(R7-Pad1)")
  (net 75 "Net-(R15-Pad2)")
  (net 76 "Net-(R16-Pad2)")
  (net 77 "Net-(R17-Pad2)")
  (net 78 "Net-(C11-Pad1)")
  (net 79 "Net-(CHRG1-Pad2)")
  (net 80 "Net-(L1-Pad2)")
  (net 81 "Net-(U2-Pad40)")
  (net 82 "Net-(D2-Pad2)")
  (net 83 "Net-(GRN1-Pad1)")
  (net 84 "Net-(R11-Pad2)")
  (net 85 "Net-(R12-Pad2)")
  (net 86 "Net-(R1-Pad2)")
  (net 87 "Net-(D2-Pad4)")
  (net 88 /~RTS)
  (net 89 /VIN)
  (net 90 "Net-(U2-Pad28)")
  (net 91 D16)
  (net 92 RX)
  (net 93 TX)
  (net 94 TCK)
  (net 95 TDI)
  (net 96 TMS)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net +3V3)
    (add_net /AREF)
    (add_net /DTR)
    (add_net /EN)
    (add_net /LED1)
    (add_net /PROG)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /USB+)
    (add_net /USB-)
    (add_net /VBAT_MES)
    (add_net /VIN)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net /~RESET)
    (add_net /~RTS)
    (add_net AIN6)
    (add_net AIN7)
    (add_net AIN8)
    (add_net AIN9)
    (add_net D16)
    (add_net D19)
    (add_net D20)
    (add_net D31)
    (add_net D35)
    (add_net D36)
    (add_net D37)
    (add_net D38)
    (add_net D41)
    (add_net D42)
    (add_net D43)
    (add_net D44)
    (add_net D49)
    (add_net D50)
    (add_net D59)
    (add_net D60)
    (add_net D64)
    (add_net DAC0)
    (add_net DAC1)
    (add_net GND)
    (add_net IO15)
    (add_net IO16)
    (add_net IO17)
    (add_net IO21)
    (add_net IO25)
    (add_net IO26)
    (add_net IO27)
    (add_net IO32)
    (add_net IO33)
    (add_net IO34)
    (add_net IO35)
    (add_net IO36)
    (add_net IO39)
    (add_net IO4)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(CHRG1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(GRN1-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-PadDET_T)")
    (add_net "Net-(J3-PadSW_T)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad24)")
    (add_net "Net-(U5-Pad4)")
    (add_net RX)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net SD_CS)
    (add_net TCK)
    (add_net TDI)
    (add_net TMS)
    (add_net TX)
    (add_net VBAT)
    (add_net VUSB)
    (add_net ~)
  )
  (module 503182-1853:MOLEX_503182-1853 (layer Bottom) (tedit 5BD74303)
    (at 94.8055 99.2505 90)
    (attr smd)
    (fp_text reference J3 (at -6.17463 8.60672 90) (layer B.SilkS) hide)
    (fp_text value 5031821852 (at 0.127 -3.556 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.9 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at -1.8 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 14 SD_CS))
    (pad 3 smd rect (at -0.7 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 15 MOSI))
    (pad 4 smd rect (at 0.4 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 5 smd rect (at 1.5 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 16 SCK))
    (pad 6 smd rect (at 2.6 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad 7 smd rect (at 3.7 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 17 MISO))
    (pad 8 smd rect (at 4.8 5.605) (size 1.24 0.8) (layers Bottom B.Paste B.Mask)
      (net 18 "Net-(J3-Pad8)"))
    (pad SH1 smd rect (at -7.245 4.975) (size 2.5 0.95) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad SH2 smd rect (at 7.145 5.125) (size 2.2 1.15) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad SW_T smd rect (at 6.74 2.975) (size 1.25 1.16) (layers Bottom B.Paste B.Mask)
      (net 19 "Net-(J3-PadSW_T)"))
    (pad DET_T smd rect (at 6.74 -6.025) (size 1.2 1.16) (layers Bottom B.Paste B.Mask)
      (net 20 "Net-(J3-PadDET_T)"))
    (pad SH5 smd rect (at -7.145 -6.355) (size 2.2 1.15) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad SH4 smd rect (at -2.84 -7.15 270) (size 1.5 1.15) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad SH3 smd rect (at 4.94 -7.15 270) (size 1.5 1.15) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/5031821852.STEP
      (offset (xyz 0 -7.493 1.524))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 84.45 104.59 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 2.535 -0.312 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 SDA))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 84.42 106.09)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -2.505 -0.172) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 SCL))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Top) (tedit 5B301BBD)
    (at 74.2315 103.8225 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 0.8255 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /VBAT_MES))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 79.255 93.28)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -1.912 0.065 -180) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(R17-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 96 TMS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 81.985 93.16)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0.565 -0.831) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R16-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 94 TCK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 79.2515 92.08)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -1.9085 -0.005) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R15-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 95 TDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 78.49 104.56)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -1.83896 0.05166) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /DTR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 78.486 105.99)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -1.86182 0.11684) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 /~RTS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 69.6595 91.821)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 1.84404 0.33528) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /SWCLK))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 61.722 94.20352)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -1.73228 0.00762) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /~RESET))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 58.537 101.289)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 1.27746 0.0062 90) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 ~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Top) (tedit 5B301BBD)
    (at 71.5264 104.267 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0.2286 -0.88646 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(CHRG1-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Top) (tedit 5B301BBD)
    (at 74.2315 101.6 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1.11506 0.15748 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /PROG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 78.49 103.45 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.62706 -0.03214 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SC-80 (layer Top) (tedit 58A3074E)
    (at 67.64 98.66 180)
    (descr "JEITA SC-80")
    (tags SC-80)
    (attr smd)
    (fp_text reference D1 (at -1.702 0.0064 180) (layer F.SilkS))
    (fp_text value MBR120 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 180) (layer F.Fab))
    (pad 1 smd rect (at -0.725 0 180) (size 0.35 0.35) (layers Top F.Paste F.Mask)
      (net 89 /VIN))
    (pad 2 smd rect (at 0.725 0 180) (size 0.35 0.35) (layers Top F.Paste F.Mask)
      (net 70 VUSB))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SC-80.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-footprints:LED3535 (layer Top) (tedit 5C46A6B7)
    (at 63.77 104.39)
    (attr smd)
    (fp_text reference D2 (at -4.04 -0.87 -210) (layer F.SilkS) hide)
    (fp_text value WS2812B (at -1.778 2.54 -210) (layer F.Fab))
    (pad 3 smd rect (at 1.749999 0.875 90) (size 0.85 1) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.75 0.875 90) (size 0.85 1) (layers Top F.Paste F.Mask)
      (net 82 "Net-(D2-Pad2)") (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 1.75 -0.875 90) (size 0.85 1) (layers Top F.Paste F.Mask)
      (net 87 "Net-(D2-Pad4)") (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -1.749999 -0.875 90) (size 0.85 1) (layers Top F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (model "${CUSTOM_FOOTPRINT_DIR}/3d/SMD WS2812B Mini.step"
      (offset (xyz 0 0 1.8796))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer Top) (tedit 5C27FA59)
    (at 64.7192 92.1512 180)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J4 (at 0 -5.8 180) (layer F.SilkS) hide)
    (fp_text value B2B-PH-SM4-TB (at 0 5.8 180) (layer F.Fab))
    (fp_text user %R (at 0 1.5 180) (layer F.Fab))
    (pad MP smd roundrect (at 3.35 2.75 180) (size 1.5 3.1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.167))
    (pad MP smd roundrect (at -3.35 2.75 180) (size 1.5 3.1) (layers Top F.Paste F.Mask) (roundrect_rratio 0.167))
    (pad 2 smd roundrect (at 1 -2.85 180) (size 0.8 3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -1 -2.85 180) (size 0.8 3) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VBAT))
    (model "${CUSTOM_FOOTPRINT_DIR}/3d/S2B-PH-SM4-TB(LF)(SN)--3DModel-STEP-56544.STEP"
      (offset (xyz 0 -4.419599999999999 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer Top) (tedit 5C0CA70F)
    (at 70.0532 104.4956 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference CHRG1 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "ORANGE LED" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(CHRG1-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 VUSB))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer Top) (tedit 5C0C9AA4)
    (at 69.977 91.78544)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value TESTPOINTPAD2MM (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 9 /SWCLK))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer Top) (tedit 5C0C9A7E)
    (at 72.517 91.78544)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 0 -1.648) (layer F.SilkS) hide)
    (fp_text value TESTPOINTPAD2MM (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers Top F.Mask)
      (net 22 /SWDIO))
  )
  (module custom-footprints:10118194-0001LF locked (layer Top) (tedit 5C0C9521)
    (at 58.16092 99.40544 270)
    (attr smd)
    (fp_text reference J1 (at -5.13988 -1.64156) (layer F.SilkS) hide)
    (fp_text value 10118194-0001LF (at 5.26692 -3.27619) (layer F.SilkS) hide)
    (fp_text user PCB~Edge (at 4.25835 1.50295 270) (layer F.SilkS) hide)
    (pad 13 smd rect (at 3.05 0 270) (size 1.5 1.55) (layers Top F.Paste F.Mask))
    (pad 12 smd rect (at -3.05 0 270) (size 1.5 1.55) (layers Top F.Paste F.Mask))
    (pad 11 smd rect (at 1 0 270) (size 1.5 1.55) (layers Top F.Paste F.Mask))
    (pad 10 smd rect (at -1 0 270) (size 1.5 1.55) (layers Top F.Paste F.Mask))
    (pad 9 thru_hole circle (at 3.5 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 73 ~))
    (pad 8 thru_hole circle (at -3.5 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 73 ~))
    (pad 7 thru_hole circle (at 2.5 -2.7 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -2.5 -2.7 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 smd rect (at 1.3 -2.675 90) (size 0.45 1.35) (layers Top F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at 0.65 -2.675 90) (size 0.45 1.35) (layers Top F.Paste F.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -2.675 90) (size 0.45 1.35) (layers Top F.Paste F.Mask)
      (net 2 /USB+))
    (pad 2 smd rect (at -0.65 -2.675 90) (size 0.45 1.35) (layers Top F.Paste F.Mask)
      (net 1 /USB-))
    (pad 1 smd rect (at -1.3 -2.675 90) (size 0.45 1.35) (layers Top F.Paste F.Mask)
      (net 70 VUSB))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/10118194.STEP
      (offset (xyz 0 3.2004 -0.4318))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer Top) (tedit 5B301BBE)
    (at 59.0296 93.7558 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference GRN1 (at 6.9596 4.6736 180) (layer F.SilkS) hide)
    (fp_text value "GREEN LED" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(GRN1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Bottom) (tedit 5B301BBD)
    (at 61.6458 92.837)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1.651 0.2794 -180) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /LED1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(GRN1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Top) (tedit 5B301BBD)
    (at 71.4732 100.0506)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -1.4986 -0.0762) (layer F.SilkS))
    (fp_text value 100K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /VBAT_MES))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VBAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5B301BBE)
    (at 68.5292 103.9622 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -0.0127 0.79502 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 VBAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Adafruit Feather M4 Express:BTN_KMR2_4.6X2.8" (layer Top) (tedit 0)
    (at 64.2 99.75 270)
    (attr smd)
    (fp_text reference SW1 (at -2.032 -1.778 270) (layer F.SilkS) hide)
    (fp_text value "KMR231NG LFS" (at -2.032 2.159 270) (layer F.Fab) hide)
    (pad A smd rect (at 2.05 -0.8 270) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 7 /~RESET) (solder_mask_margin 0.0508))
    (pad B smd rect (at 2.05 0.8 270) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad B' smd rect (at -2.05 0.8 270) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad A' smd rect (at -2.05 -0.8 270) (size 0.9 0.9) (layers Top F.Paste F.Mask)
      (net 7 /~RESET) (solder_mask_margin 0.0508))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/KMR221GLF.STEP
      (offset (xyz 0 0 1.3716))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Bottom) (tedit 5B301BBE)
    (at 64.5795 91.059)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at -2.5781 -0.254) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(C11-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5B301BBE)
    (at 73.212196 99.36998 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -0.05598 -1.336804 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5B301BBE)
    (at 69.82968 96.79432 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 1.29032 0.02032) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5B301BBE)
    (at 67.88902 95.9612)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -1.26482 -0.0762 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer Top) (tedit 5B301BBD)
    (at 72.7202 94.1324 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -1.4898 -0.6576) (layer F.SilkS))
    (fp_text value 10K (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 /VIN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /EN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-footprints:NPPC_0.100in_headers_2ROW (layer Top) (tedit 5BD526DB)
    (at 78.8035 99.5045 90)
    (attr smd)
    (fp_text reference J5 (at -3.683 0 90) (layer F.SilkS))
    (fp_text value NPTC072KFMS-RC (at 0 5.334 90) (layer F.Fab))
    (pad 14 smd rect (at 7.62 2.889 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 94 TCK))
    (pad 13 smd rect (at 5.08 2.889 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 59 IO25))
    (pad 12 smd rect (at 2.54 2.889 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 56 IO35))
    (pad 11 smd rect (at 0 2.889 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 68 IO39))
    (pad 10 smd rect (at -2.54 2.889 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 69 IO36))
    (pad 9 smd rect (at -5.08 2.889 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 62 IO21))
    (pad 8 smd rect (at -7.62 2.889 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 65 IO4))
    (pad 7 smd rect (at 7.62 -2.921 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 95 TDI))
    (pad 6 smd rect (at 5.08 -2.921 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 96 TMS))
    (pad 5 smd rect (at 2.54 -2.921 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 60 IO26))
    (pad 4 smd rect (at 0 -2.921 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 55 IO34))
    (pad 3 smd rect (at -2.54 -2.921 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 53 IO15))
    (pad 2 smd rect (at -5.08 -2.921 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 63 IO17))
    (pad 1 smd rect (at -7.62 -2.921 90) (size 1 1.56) (layers Top F.Paste F.Mask)
      (net 64 IO16))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x07_P2.54mm_Vertical_SMD.step
      (at (xyz 0 0 0))
      (scale (xyz 0.9 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x17_P2.54mm_Vertical (layer Top) (tedit 5BD524CA)
    (at 62.357 109.56544 90)
    (descr "Through hole straight socket strip, 1x17, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x17 2.54mm single row")
    (fp_text reference J7 (at -0.48006 -1.4605 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x17 (at 0 43.41 90) (layer F.Fab))
    (fp_text user %R (at -3.84556 20.066 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5748 1.5748) (drill 1) (layers *.Cu *.Mask)
      (net 41 D44))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 D43))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 D42))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 D41))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 D37))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 D36))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 D35))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 D31))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 SCK))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 MOSI))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 MISO))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 RX))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 93 TX))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 1.5748 1.5748) (drill 0.9) (layers *.Cu *.Mask)
      (net 91 D16))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer Top) (tedit 5C0C9B65)
    (at 69.977 89.24544 90)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J2 (at 0.40894 -3.6195 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x14 (at 0 35.35 90) (layer F.Fab))
    (fp_text user %R (at 0 16.51 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VBAT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 D49))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /VIN))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 DAC1))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 D59))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 D60))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 D64))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 DAC0))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 AIN6))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 AIN7))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 AIN8))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 AIN9))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 SCL))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 SDA))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5BD51ACE)
    (at 71.7296 99.06)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -1.2192 -0.3556 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Adafruit Feather M4 Express:SOT23-5" (layer Top) (tedit 0)
    (at 72.644 96.647 90)
    (descr "<b>Small Outline Transistor</b> - 5 Pin")
    (attr smd)
    (fp_text reference U5 (at -0.6985 -1.4605 270) (layer F.SilkS))
    (fp_text value AP2112K-3.3TRG1 (at 1.978 0.635 90) (layer F.Fab))
    (pad 5 smd rect (at -0.95 -1.3001 90) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 0.95 -1.3001 90) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 66 "Net-(U5-Pad4)") (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 0.95 1.3001 90) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 67 /EN) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at 0 1.3001 90) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -0.95 1.3001 90) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 89 /VIN) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5BD519E7)
    (at 70.1953 94.1324 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -1.3057 -0.0762 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Adafruit Feather M4 Express:SOT23-R" (layer Top) (tedit 0)
    (at 67.7672 101.1174)
    (descr "<b>SOT23</b> - Reflow soldering")
    (attr smd)
    (fp_text reference Q3 (at -0.762 0.4318) (layer F.SilkS))
    (fp_text value DMG341 (at 1.778 0.635) (layer F.Fab))
    (pad 3 smd rect (at 0 -1) (size 0.635 1.016) (layers Top F.Paste F.Mask)
      (net 6 VBAT) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at 0.95 1) (size 0.635 1.016) (layers Top F.Paste F.Mask)
      (net 89 /VIN) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -0.95 1) (size 0.635 1.016) (layers Top F.Paste F.Mask)
      (net 70 VUSB) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Bottom) (tedit 5BD51BB5)
    (at 64.5795 92.2655 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.7051 0.3683 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module QFP50P1200X1200X120-64N (layer Bottom) (tedit 0)
    (at 69.5325 99.441 180)
    (attr smd)
    (fp_text reference U2 (at -5.842 6.0325 180) (layer B.SilkS))
    (fp_text value ATSAMD51J20A-AU (at 1.7145 -0.254 270) (layer B.SilkS))
    (pad 1 smd rect (at -5.67 3.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 10 /XTAL1))
    (pad 2 smd rect (at -5.67 3.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 11 /XTAL2))
    (pad 3 smd rect (at -5.67 2.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 23 DAC0))
    (pad 4 smd rect (at -5.67 2.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 12 /AREF))
    (pad 5 smd rect (at -5.67 1.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 24 AIN6))
    (pad 6 smd rect (at -5.67 1.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 25 AIN7))
    (pad 7 smd rect (at -5.67 0.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad 8 smd rect (at -5.67 0.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 9 smd rect (at -5.67 -0.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 26 AIN8))
    (pad 10 smd rect (at -5.67 -0.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 27 AIN9))
    (pad 11 smd rect (at -5.67 -1.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 68 IO39))
    (pad 12 smd rect (at -5.67 -1.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 69 IO36))
    (pad 13 smd rect (at -5.67 -2.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 14 SD_CS))
    (pad 14 smd rect (at -5.67 -2.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 29 DAC1))
    (pad 15 smd rect (at -5.67 -3.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 71 /VBAT_MES))
    (pad 16 smd rect (at -5.67 -3.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 91 D16))
    (pad 17 smd rect (at -3.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 30 SDA))
    (pad 18 smd rect (at -3.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 28 SCL))
    (pad 19 smd rect (at -2.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 31 D19))
    (pad 20 smd rect (at -2.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 32 D20))
    (pad 21 smd rect (at -1.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 22 smd rect (at -1.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad 23 smd rect (at -0.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 88 /~RTS))
    (pad 24 smd rect (at -0.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 21 /DTR))
    (pad 25 smd rect (at 0.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 15 MOSI))
    (pad 26 smd rect (at 0.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 16 SCK))
    (pad 27 smd rect (at 1.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 17 MISO))
    (pad 28 smd rect (at 1.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 90 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at 2.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 93 TX))
    (pad 30 smd rect (at 2.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 92 RX))
    (pad 31 smd rect (at 3.25 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 33 D31))
    (pad 32 smd rect (at 3.75 -5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 87 "Net-(D2-Pad4)"))
    (pad 33 smd rect (at 5.67 -3.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad 34 smd rect (at 5.67 -3.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 35 smd rect (at 5.67 -2.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 34 D35))
    (pad 36 smd rect (at 5.67 -2.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 35 D36))
    (pad 37 smd rect (at 5.67 -1.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 36 D37))
    (pad 38 smd rect (at 5.67 -1.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 37 D38))
    (pad 39 smd rect (at 5.67 -0.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 86 "Net-(R1-Pad2)"))
    (pad 40 smd rect (at 5.67 -0.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 81 "Net-(U2-Pad40)"))
    (pad 41 smd rect (at 5.67 0.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 38 D41))
    (pad 42 smd rect (at 5.67 0.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 39 D42))
    (pad 43 smd rect (at 5.67 1.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 40 D43))
    (pad 44 smd rect (at 5.67 1.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 41 D44))
    (pad 45 smd rect (at 5.67 2.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 1 /USB-))
    (pad 46 smd rect (at 5.67 2.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 2 /USB+))
    (pad 47 smd rect (at 5.67 3.25 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad 48 smd rect (at 5.67 3.75 90) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 49 smd rect (at 3.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 42 D49))
    (pad 50 smd rect (at 3.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 43 D50))
    (pad 51 smd rect (at 2.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 8 /LED1))
    (pad 52 smd rect (at 2.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 7 /~RESET))
    (pad 53 smd rect (at 1.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 78 "Net-(C11-Pad1)"))
    (pad 54 smd rect (at 1.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 4 GND))
    (pad 55 smd rect (at 0.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 80 "Net-(L1-Pad2)"))
    (pad 56 smd rect (at 0.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 57 smd rect (at -0.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 9 /SWCLK))
    (pad 58 smd rect (at -0.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 22 /SWDIO))
    (pad 59 smd rect (at -1.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 44 D59))
    (pad 60 smd rect (at -1.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 45 D60))
    (pad 61 smd rect (at -2.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 96 TMS))
    (pad 62 smd rect (at -2.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 94 TCK))
    (pad 63 smd rect (at -3.25 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 95 TDI))
    (pad 64 smd rect (at -3.75 5.67) (size 0.28 1.47) (layers Bottom B.Paste B.Mask)
      (net 46 D64))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-64_10x10mm_P0.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Adafruit Feather M4 Express:SOT23-5" (layer Top) (tedit 0)
    (at 71.501 102.0445 270)
    (descr "<b>Small Outline Transistor</b> - 5 Pin")
    (attr smd)
    (fp_text reference U4 (at 0.7355 -1.939 270) (layer F.SilkS))
    (fp_text value MCP73831T-2ACI/OT (at 1.978 0.635 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.3001 270) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 74 "Net-(R7-Pad1)") (solder_mask_margin 0.0508))
    (pad 2 smd rect (at 0 1.3001 270) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 0.95 1.3001 270) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 6 VBAT) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 0.95 -1.3001 270) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 70 VUSB) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -0.95 -1.3001 270) (size 0.55 1.2) (layers Top F.Paste F.Mask)
      (net 72 /PROG) (solder_mask_margin 0.0508))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Adafruit HUZZAH32 ESP32 Feather:WROOM32_SKINNY" (layer Top) (tedit 0)
    (at 96.74606 99.40544 270)
    (attr smd)
    (fp_text reference U3 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value ESP32_WROOM32_SKINNY (at 0 0 270) (layer F.SilkS) hide)
    (pad P$1 smd rect (at 0.34 2.7 270) (size 6 6) (layers Top F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad 38 smd rect (at 8.5 -5 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad 37 smd rect (at 8.5 -3.73 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 30 SDA) (solder_mask_margin 0.0508))
    (pad 36 smd rect (at 8.5 -2.46 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 28 SCL) (solder_mask_margin 0.0508))
    (pad 35 smd rect (at 8.5 -1.19 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 81 "Net-(U2-Pad40)") (solder_mask_margin 0.0508))
    (pad 34 smd rect (at 8.5 0.08 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 86 "Net-(R1-Pad2)") (solder_mask_margin 0.0508))
    (pad 33 smd rect (at 8.5 1.35 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 62 IO21) (solder_mask_margin 0.0508))
    (pad 32 smd rect (at 8.5 2.62 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (solder_mask_margin 0.0508))
    (pad 31 smd rect (at 8.5 3.89 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 17 MISO) (solder_mask_margin 0.0508))
    (pad 30 smd rect (at 8.5 5.16 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 15 MOSI) (solder_mask_margin 0.0508))
    (pad 29 smd rect (at 8.5 6.43 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 16 SCK) (solder_mask_margin 0.0508))
    (pad 28 smd rect (at 8.5 7.7 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 63 IO17) (solder_mask_margin 0.0508))
    (pad 27 smd rect (at 8.5 8.97 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 64 IO16) (solder_mask_margin 0.0508))
    (pad 26 smd rect (at 8.5 10.24 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 65 IO4) (solder_mask_margin 0.0508))
    (pad 25 smd rect (at 8.5 11.51 270) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 84 "Net-(R11-Pad2)") (solder_mask_margin 0.0508))
    (pad 24 smd rect (at 5.73 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 54 "Net-(U3-Pad24)") (solder_mask_margin 0.0508))
    (pad 23 smd rect (at 4.46 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 53 IO15) (solder_mask_margin 0.0508))
    (pad 22 smd rect (at 3.19 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 52 "Net-(U3-Pad22)") (solder_mask_margin 0.0508))
    (pad 21 smd rect (at 1.92 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 51 "Net-(U3-Pad21)") (solder_mask_margin 0.0508))
    (pad 20 smd rect (at 0.65 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 50 "Net-(U3-Pad20)") (solder_mask_margin 0.0508))
    (pad 19 smd rect (at -0.62 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 49 "Net-(U3-Pad19)") (solder_mask_margin 0.0508))
    (pad 18 smd rect (at -1.89 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 48 "Net-(U3-Pad18)") (solder_mask_margin 0.0508))
    (pad 17 smd rect (at -3.16 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 47 "Net-(U3-Pad17)") (solder_mask_margin 0.0508))
    (pad 16 smd rect (at -4.43 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 76 "Net-(R16-Pad2)") (solder_mask_margin 0.0508))
    (pad 15 smd rect (at -5.7 12.9 180) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -8.5 11.51 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 75 "Net-(R15-Pad2)") (solder_mask_margin 0.0508))
    (pad 13 smd rect (at -8.5 10.24 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 77 "Net-(R17-Pad2)") (solder_mask_margin 0.0508))
    (pad 12 smd rect (at -8.5 8.97 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 61 IO27) (solder_mask_margin 0.0508))
    (pad 11 smd rect (at -8.5 7.7 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 60 IO26) (solder_mask_margin 0.0508))
    (pad 10 smd rect (at -8.5 6.43 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 59 IO25) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at -8.5 5.16 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 58 IO33) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at -8.5 3.89 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 57 IO32) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at -8.5 2.62 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 56 IO35) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at -8.5 1.35 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 55 IO34) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -8.5 0.08 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 68 IO39) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -8.5 -1.19 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 69 IO36) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -8.5 -2.46 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 85 "Net-(R12-Pad2)") (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -8.5 -3.73 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 5 +3V3) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -8.5 -5 90) (size 1.2 0.9) (layers Top F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/KiCAD-ESP-WROOM-32.step
      (offset (xyz 0 -0.2794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Bottom) (tedit 5BD51C11)
    (at 79.7115 95.294 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.044 -0.9335 270) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /XTAL1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Bottom) (tedit 5BD51C16)
    (at 79.7115 97.6945 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -0.0315 -1 270) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /XTAL2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5BD519A0)
    (at 67.8688 97.01784 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.4224 -0.36576) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /AREF))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Bottom) (tedit 5BD51B69)
    (at 63.69304 94.16288 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.39624 0.89408 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /~RESET))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Bottom) (tedit 5BD51B77)
    (at 63.18 105.03 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0.0254 -0.9398 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Top) (tedit 5BD51C77)
    (at 72.9615 105.7275)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -0.0635 -0.8509 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Top F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0806_2016Metric (layer Bottom) (tedit 5BD5FCE8)
    (at 66.9925 92.202 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 2.54 -0.0635 180) (layer B.SilkS))
    (fp_text value 10uH (at 0.762 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0.762 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0 90) (size 0.5 1.6) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 1.5 0 90) (size 0.5 1.6) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(L1-Pad2)"))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/Inductor0806.step
      (offset (xyz 0.7619999885559082 0 0))
      (scale (xyz 0.9 0.9 0.9))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer Bottom) (tedit 5BD51B3D)
    (at 58.537 100.2095)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.0254 -1.0287 180) (layer B.SilkS))
    (fp_text value "4.5 nF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 ~))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers Bottom B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_MicroCrystal_CC7V-T1A-2Pin_3.2x1.5mm (layer Bottom) (tedit 5A0FD1B2)
    (at 77.851 96.012 90)
    (descr "SMD Crystal MicroCrystal CC7V-T1A/CM7V-T1A series http://www.microcrystal.com/images/_Product-Documentation/01_TF_ceramic_Packages/01_Datasheet/CC1V-T1A.pdf, 3.2x1.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at -2.794 0.127 90) (layer B.SilkS))
    (fp_text value ST3215SB (at 0 -1.95 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1.8) (layers Bottom B.Paste B.Mask)
      (net 11 /XTAL2))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1.8) (layers Bottom B.Paste B.Mask)
      (net 10 /XTAL1))
    (model ${CUSTOM_FOOTPRINT_DIR}/3d/SMD2_Crystal.STEP
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz -90 0 0))
    )
  )
  (module "Adafruit HUZZAH32 ESP32 Feather:MOUNTINGHOLE_2.5_PLATED" (layer Top) (tedit 0)
    (at 58.42 108.204)
    (fp_text reference J96 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTINGHOLE2.5 (at 0 0) (layer F.SilkS) hide)
    (pad P$1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (module "Adafruit HUZZAH32 ESP32 Feather:MOUNTINGHOLE_2.5_PLATED" (layer Top) (tedit 0)
    (at 58.42 90.4875)
    (fp_text reference J97 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MOUNTINGHOLE2.5 (at 0 0) (layer F.SilkS) hide)
    (pad P$1 thru_hole circle (at 0 0) (size 3.2 3.2) (drill 2.5) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0508))
  )
  (gr_text D16 (at 104.32 110.28 30) (layer F.SilkS))
  (gr_text D42 (at 73.64476 107.696) (layer B.SilkS))
  (gr_text D41 (at 76.09078 107.696) (layer B.SilkS))
  (gr_text D35 (at 83.82 107.696) (layer B.SilkS))
  (gr_text D31 (at 86.106 107.696) (layer B.SilkS))
  (gr_text GND (at 101.58222 110.34014 30) (layer F.SilkS))
  (gr_text D41 (at 75.07986 108.204) (layer F.SilkS))
  (gr_text D43 (at 67.46748 107.696) (layer F.SilkS))
  (gr_text TX (at 99.04476 110.40872 30) (layer F.SilkS))
  (gr_text RX (at 96.47744 110.38662 30) (layer F.SilkS))
  (gr_text TMS (at 74.61 93.37) (layer F.SilkS))
  (gr_text RX (at 96.17 107.696) (layer B.SilkS))
  (gr_text D16 (at 103.886 107.696) (layer B.SilkS))
  (gr_text TX (at 98.48 107.696) (layer B.SilkS))
  (gr_text - (at 63.754 96.901 180) (layer F.SilkS))
  (gr_text + (at 65.659 96.901 90) (layer F.SilkS))
  (gr_text HOLLIDAY (at 57.086 101.743 270) (layer B.Mask))
  (gr_text HOLLIDAY (at 57.086 101.743 270) (layer Bottom))
  (gr_text SAM32 (at 56.388 105.029) (layer F.Mask))
  (gr_line (start 109.19206 106.94508) (end 109.19206 108.49864) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 106.65206 108.49864) (end 109.19206 108.49864) (angle 90) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 103.755076 102.181768) (end 109.19206 106.94508) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 55.85206 96.296067) (end 56.3 96.74) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 103.758052 96.469398) (end 109.220013 91.69) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 103.918511 96.711167) (end 103.628512 96.721166) (angle 58.4) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 103.915535 101.939999) (end 103.625536 101.93) (angle -58.4) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 103.625536 101.93) (end 103.628512 96.721166) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 55.85206 102.438136) (end 56.3 101.994203) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 56.071489 101.815368) (end 56.361488 101.805369) (angle 40.02178601) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 56.071489 96.918835) (end 56.361488 96.928834) (angle -40.02178601) (layer Edge.Cuts) (width 0.508))
  (gr_text uSD (at 103.12 104.16 90) (layer B.SilkS))
  (gr_text v22 (at 82.677 100.584 90) (layer B.SilkS))
  (gr_text LED (at 57.14 93.67 270) (layer F.SilkS))
  (gr_text CHRG (at 69.17 105.94) (layer F.SilkS))
  (gr_text RST (at 62.04 99.65 270) (layer F.SilkS))
  (gr_text SDA (at 101.87432 88.31326 210) (layer F.SilkS))
  (gr_text SCL (at 99.30384 88.34374 210) (layer F.SilkS))
  (gr_text MISO (at 93.84284 110.36808 30) (layer F.SilkS))
  (gr_text MOSI (at 91.3892 110.36046 30) (layer F.SilkS))
  (gr_text SCK (at 88.90762 110.3122 30) (layer F.SilkS))
  (gr_text D64 (at 84.2645 90.932 180) (layer B.SilkS))
  (gr_text AIN7 (at 91.8845 90.932 180) (layer B.SilkS))
  (gr_text SDA (at 102.0445 90.932 180) (layer B.SilkS))
  (gr_text D60 (at 81.7245 90.932 180) (layer B.SilkS))
  (gr_text AIN8 (at 94.4245 90.932 180) (layer B.SilkS))
  (gr_text DAC0 (at 86.614 90.932 180) (layer B.SilkS))
  (gr_text SCL (at 99.5045 90.932 180) (layer B.SilkS))
  (gr_text D59 (at 79.1845 90.932 180) (layer B.SilkS))
  (gr_text DAC1 (at 76.327 90.932 180) (layer B.SilkS))
  (gr_text VBAT (at 68.58 90.932 180) (layer B.SilkS))
  (gr_text D49 (at 71.5645 90.932 180) (layer B.SilkS))
  (gr_text USB (at 74.1045 90.932 180) (layer B.SilkS))
  (gr_text AIN6 (at 89.3445 90.932 180) (layer B.SilkS))
  (gr_text AIN9 (at 96.9645 90.932 180) (layer B.SilkS))
  (gr_text GND (at 101.55 107.696) (layer B.SilkS))
  (gr_text MISO (at 93.98 107.696) (layer B.SilkS))
  (gr_text MOSI (at 91.44 107.696) (layer B.SilkS))
  (gr_text SCK (at 88.66378 107.696) (layer B.SilkS))
  (gr_text D36 (at 81.28 107.696) (layer B.SilkS))
  (gr_text D37 (at 78.74 107.696) (layer B.SilkS))
  (gr_text GND (at 71.12 107.696) (layer B.SilkS))
  (gr_text D43 (at 68.58 107.696) (layer B.SilkS))
  (gr_text 3.3V (at 66.04 107.696) (layer B.SilkS))
  (gr_text D44 (at 63.5 107.696) (layer B.SilkS))
  (gr_text "3.7/4.2V LiPo" (at 64.02 88.65) (layer B.SilkS))
  (gr_text C+M (at 75.057 104.521 90) (layer B.SilkS))
  (gr_circle (center 106.553 90.61572) (end 108.205221 90.61572) (layer Edge.Cuts) (width 0.508))
  (gr_circle (center 106.553 108.20522) (end 108.205221 108.20522) (layer Edge.Cuts) (width 0.508))
  (gr_text "BEGIN WIFI ANTENNA" (at 102.616 99.3775 90) (layer F.SilkS))
  (gr_text "ESP32-WROOM-32\n**OPTIONAL**" (at 87.122 98.2345 90) (layer F.SilkS))
  (gr_text "ESP32 I/O" (at 78.74 98.8695 90) (layer F.SilkS))
  (gr_text SAM32 (at 82.68 95.01 90) (layer B.SilkS))
  (gr_text SAM32 (at 56.388 105.029) (layer Top))
  (gr_text github/maholli (at 84.7725 93.853 90) (layer B.SilkS))
  (gr_text TCK (at 83.6295 91.948) (layer F.SilkS))
  (gr_text TDI (at 74.168 91.8845) (layer F.SilkS))
  (gr_text IO25 (at 82.042 93.345) (layer F.SilkS))
  (gr_text IO26 (at 75.6285 95.631) (layer F.SilkS))
  (gr_text IO35 (at 82.042 95.6945) (layer F.SilkS))
  (gr_text IO17 (at 75.692 103.378) (layer F.SilkS))
  (gr_text IO34 (at 75.6285 98.171) (layer F.SilkS))
  (gr_text IO15 (at 75.819 100.7745) (layer F.SilkS))
  (gr_text IO16 (at 75.6666 105.918) (layer F.SilkS))
  (gr_text IO39 (at 82.042 98.2345) (layer F.SilkS))
  (gr_text IO36 (at 82.042 100.838) (layer F.SilkS))
  (gr_text IO21 (at 81.9785 103.3145) (layer F.SilkS))
  (gr_text IO04 (at 81.9785 105.918) (layer F.SilkS))
  (gr_text DIO (at 72.517 93.1164) (layer F.SilkS))
  (gr_text D36 (at 79.756 107.696) (layer F.SilkS))
  (gr_text D35 (at 82.677 108.204) (layer F.SilkS))
  (gr_text D37 (at 77.724 107.696) (layer F.SilkS))
  (gr_text GND (at 69.977 107.696) (layer F.SilkS))
  (gr_text D42 (at 72.517 107.696) (layer F.SilkS))
  (gr_text 3.3V (at 65.024 107.696) (layer F.SilkS))
  (gr_text D44 (at 62.4205 107.696) (layer F.SilkS))
  (gr_text D60 (at 82.677 90.805) (layer F.SilkS))
  (gr_text D59 (at 80.137 90.805) (layer F.SilkS))
  (gr_text DAC1 (at 77.597 90.805) (layer F.SilkS))
  (gr_text USB (at 75.0316 90.805) (layer F.SilkS))
  (gr_text D49 (at 72.4916 90.678) (layer F.SilkS))
  (gr_text VBAT (at 70.104 90.678) (layer F.SilkS))
  (gr_text CLK (at 70.0278 93.091) (layer F.SilkS))
  (gr_line (start 109.220013 90.13644) (end 109.220013 91.69) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 55.85206 90.13644) (end 55.85206 96.296067) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 106.680013 90.13644) (end 109.220013 90.13644) (angle -90) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 55.85206 102.438136) (end 55.85206 108.49864) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 106.680013 87.59644) (end 58.39206 87.59644) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 58.39206 111.03864) (end 106.65206 111.03864) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 58.39206 90.13644) (end 58.39206 87.59644) (angle -90) (layer Edge.Cuts) (width 0.508))
  (gr_line (start 56.361488 96.928834) (end 56.361488 101.805369) (layer Edge.Cuts) (width 0.508))
  (gr_arc (start 58.39206 108.49864) (end 55.85206 108.49864) (angle -90) (layer Edge.Cuts) (width 0.508))
  (zone (net 4) (net_name GND) (layer GND) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 55.85206 87.59) (xy 55.85206 111.05) (xy 103.25 111.05) (xy 103.25 87.59)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer PWR) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.2032) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 55.8546 111.091501) (xy 103.25 111.04955) (xy 103.25 87.583047) (xy 55.8546 87.6381)
      )
    )
  )
)
