(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 239)
    (tracks 317)
    (zones 0)
    (modules 33)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.127)
    (segment_width 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 165.735 75.184)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad18)")
  (net 2 "Net-(U1-Pad19)")
  (net 3 +3V3)
  (net 4 GND)
  (net 5 "Net-(C3-Pad1)")
  (net 6 RESET)
  (net 7 TX)
  (net 8 RX)
  (net 9 VIN)
  (net 10 TEST)
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(JP1-Pad1)")
  (net 13 P2.2)
  (net 14 P2.1)
  (net 15 RF|SEL)
  (net 16 SCK)
  (net 17 P1.4)
  (net 18 MOSI)
  (net 19 P1.3)
  (net 20 MISO)
  (net 21 P2.5)
  (net 22 P2.4)
  (net 23 P1.0)
  (net 24 P2.3)
  (net 25 "Net-(U2-Pad4)")
  (net 26 "Net-(U2-Pad9)")
  (net 27 "Net-(U2-Pad10)")
  (net 28 "Net-(U2-Pad11)")
  (net 29 "Net-(U2-Pad12)")
  (net 30 "Net-(U2-Pad13)")
  (net 31 "Net-(J7-Pad1)")
  (net 32 "Net-(J8-Pad1)")
  (net 33 "Net-(J9-Pad1)")
  (net 34 "Net-(J10-Pad1)")
  (net 35 "Net-(J13-Pad1)")
  (net 36 "Net-(J14-Pad1)")
  (net 37 "Net-(J15-Pad1)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad9)")
    (add_net P1.0)
    (add_net P1.3)
    (add_net P1.4)
    (add_net P2.1)
    (add_net P2.2)
    (add_net P2.3)
    (add_net P2.4)
    (add_net P2.5)
    (add_net RESET)
    (add_net RF|SEL)
    (add_net RX)
    (add_net SCK)
    (add_net TEST)
    (add_net TX)
    (add_net VIN)
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 176.657 80.645 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module flabbergast:IC_LOGO (layer B.Cu) (tedit 572485E7)
    (at 192.913 73.406)
    (fp_text reference IC_LOGO (at 0 -2.286) (layer Cmts.User) hide)
    (fp_text value IC_LOGO (at 0 2.159) (layer Cmts.User) hide)
  )
  (module flabbergast:IC_LOGO (layer F.Cu) (tedit 572485E7)
    (at 175.006 89.789)
    (fp_text reference IC_LOGO (at 0 2.286) (layer Cmts.User) hide)
    (fp_text value IC_LOGO (at 0 -2.159) (layer Cmts.User) hide)
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391EB7)
    (at 182.245 75.565 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.8 90) (layer B.SilkS) hide)
    (fp_text value byp (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 9 VIN))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy -0.55 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 5 "Net-(C3-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 187.34 81.915 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8) (layer B.SilkS) hide)
    (fp_text value pwr (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 12 "Net-(JP1-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 5A0AB76C)
    (at 187.071 77.597 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at -0.127 0 90) (layer B.SilkS))
    (fp_text value MCP1703A-3302_SOT23 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(JP1-Pad1)"))
    (pad 1 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_C26-LF_D2.1mm_L6.5mm_Horizontal_1EP_style1 (layer F.Cu) (tedit 5A0FD1B2)
    (at 161.0868 83.2866 270)
    (descr "Crystal THT C26-LF 6.5mm length 2.06mm diameter")
    (tags ['C26-LF'])
    (fp_text reference Y1 (at -0.9906 7.1628) (layer F.SilkS) hide)
    (fp_text value 32768kHz (at 3.57 1.75) (layer F.Fab))
    (fp_text user %R (at 1 5.75) (layer F.Fab))
    (pad 3 smd rect (at 0.95 5.75 270) (size 2.2 6.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.9 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad19)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad18)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_C26-LF_D2.1mm_L6.5mm_Horizontal_1EP_style1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 171.45 88.265 180)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at 3.81 22.987) (layer F.SilkS) hide)
    (fp_text value MSP430G2553IN20 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 P2.2))
    (pad 19 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad19)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 P2.1))
    (pad 18 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad18)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 RF|SEL))
    (pad 17 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 TEST))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 SCK))
    (pad 16 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 RESET))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 P1.4))
    (pad 15 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 MOSI))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 P1.3))
    (pad 14 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 MISO))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 TX))
    (pad 13 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 P2.5))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 RX))
    (pad 12 thru_hole oval (at 7.62 20.32 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 P2.4))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 P1.0))
    (pad 11 thru_hole oval (at 7.62 22.86 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 P2.3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:M03_NOSILK_SMALLER (layer F.Cu) (tedit 5D0A8C2D)
    (at 157.48 73.025 90)
    (fp_text reference J5 (at 1.27 0 90) (layer Cmts.User) hide)
    (fp_text value SPI (at 1.27 0 90) (layer Eco1.User) hide)
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 18 MOSI))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 16 SCK))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 20 MISO))
  )
  (module flabbergast:M03_NOSILK_SMALLER (layer F.Cu) (tedit 5D0A8C2D)
    (at 160.02 73.025 90)
    (fp_text reference J4 (at 1.27 0 90) (layer Cmts.User) hide)
    (fp_text value P1 (at 1.27 0 90) (layer Eco1.User) hide)
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 23 P1.0))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 19 P1.3))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 17 P1.4))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 152.4 70.485)
    (fp_text reference J15 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 37 "Net-(J15-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 37 "Net-(J15-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 37 "Net-(J15-Pad1)"))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 152.4 73.025)
    (fp_text reference J14 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 36 "Net-(J14-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 36 "Net-(J14-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 36 "Net-(J14-Pad1)"))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 152.4 65.405)
    (fp_text reference J13 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 35 "Net-(J13-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 35 "Net-(J13-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 35 "Net-(J13-Pad1)"))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 157.48 80.645)
    (fp_text reference J12 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 157.48 78.105)
    (fp_text reference J11 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 +3V3))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 152.4 75.565)
    (fp_text reference J10 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 34 "Net-(J10-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 34 "Net-(J10-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 34 "Net-(J10-Pad1)"))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 152.4 67.945)
    (fp_text reference J9 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 33 "Net-(J9-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 33 "Net-(J9-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 33 "Net-(J9-Pad1)"))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 152.4 80.645)
    (fp_text reference J8 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 32 "Net-(J8-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 32 "Net-(J8-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 32 "Net-(J8-Pad1)"))
  )
  (module flabbergast:M02_CONNECTED_SMALLER (layer F.Cu) (tedit 5D0A8BC6)
    (at 152.4 78.105)
    (fp_text reference J7 (at 3.81 0) (layer Cmts.User) hide)
    (fp_text value proto_pair (at 3.81 0) (layer Eco1.User) hide)
    (pad 1 connect rect (at 1.27 0) (size 1.6 0.5) (layers F.Cu F.Mask)
      (net 31 "Net-(J7-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 31 "Net-(J7-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.85) (layers *.Cu *.Mask)
      (net 31 "Net-(J7-Pad1)"))
  )
  (module flabbergast:M06_NOSILK (layer F.Cu) (tedit 0)
    (at 149.86 84.455 90)
    (fp_text reference J1 (at 0 0 90) (layer Cmts.User) hide)
    (fp_text value serplus (at 0 0 90) (layer Eco1.User) hide)
    (pad 6 thru_hole oval (at 6.35 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 RESET))
    (pad 5 thru_hole oval (at 3.81 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 TX))
    (pad 4 thru_hole oval (at 1.27 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 RX))
    (pad 3 thru_hole oval (at -1.27 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 VIN))
    (pad 2 thru_hole oval (at -3.81 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 TEST))
    (pad 1 thru_hole oval (at -6.35 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module flabbergast:HOLE_CIRC_25 (layer F.Cu) (tedit 5D033C27)
    (at 179.2478 89.7382)
    (fp_text reference HOLE (at 0 2.286) (layer Dwgs.User) hide)
    (fp_text value 2.5MM (at 0 4.064) (layer Dwgs.User) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu))
  )
  (module flabbergast:HOLE_CIRC_25 (layer F.Cu) (tedit 5D033C27)
    (at 159.2326 66.2432)
    (fp_text reference HOLE (at 0 2.286) (layer Dwgs.User) hide)
    (fp_text value 2.5MM (at 0 4.064) (layer Dwgs.User) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu))
  )
  (module flabbergast:M05_NOSILK (layer F.Cu) (tedit 569F9C30)
    (at 149.86 70.485 270)
    (fp_text reference J6 (at 1.27 0 90) (layer Cmts.User) hide)
    (fp_text value P2 (at 1.27 0 90) (layer Eco1.User) hide)
    (pad 5 thru_hole oval (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 P2.5))
    (pad 4 thru_hole oval (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 P2.4))
    (pad 3 thru_hole oval (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 P2.3))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 P2.2))
    (pad 1 thru_hole oval (at -5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 P2.1))
  )
  (module flabbergast:CR2032_shorter (layer F.Cu) (tedit 5D03462B)
    (at 184.658 68.326 90)
    (fp_text reference BT1 (at -12.7 -12.7 90) (layer F.SilkS) hide)
    (fp_text value CR2032 (at -12.7 12.7 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.29 2.29) (drill 1.41) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at -19.05 0 90) (size 2.29 2.29) (drill 1.41) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 176.9364 64.8208 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at -1.6256 0.0508 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.05) (layer F.Fab))
    (fp_text user %R (at 1.2954 -0.0762) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 168.87 90.932 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 4.151 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.05) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 187.08 73.66)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -0.009 -1.524) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 182.88 81.035 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 1.524 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.3mm_L11.0mm (layer F.Cu) (tedit 5A1DC085)
    (at 194.056 90.17)
    (descr "solder Pin_ diameter 1.3mm, hole diameter 1.3mm, length 11.0mm")
    (tags "solder Pin_ pressfit")
    (fp_text reference J2 (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.3mm_L11.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal (layer B.Cu) (tedit 5B7745C6)
    (at 177.927 67.945 180)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J3 (at 1 2.55) (layer B.SilkS) hide)
    (fp_text value JST_power (at 1 -7.45) (layer B.Fab))
    (fp_text user %R (at 1 -2.5) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 9 VIN))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 160.02 90.932 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 47kR (at 3.81 0) (layer F.SilkS))
    (fp_text value 100kR (at 3.81 1.92) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 RESET))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:TACTILE-SWITCH-THT-6x3.5mm (layer F.Cu) (tedit 5D095972)
    (at 156.21 87.884)
    (descr "tactile switch SPST right angle, PTS645VL31-2 LFS")
    (tags "tactile switch SPST angled PTS645VL31-2 LFS C&K Button")
    (fp_text reference SW1 (at 0.381 -2.667) (layer F.SilkS) hide)
    (fp_text value Reset (at 0.254 2.7305) (layer F.Fab))
    (fp_text user %R (at 0.381 -2.667) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.708 0) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 RESET))
    (pad 1 thru_hole circle (at -3.302 0) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_Tactile_SPST_Angled_PTS645Vx31-2LFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module flabbergast:RFM12B (layer F.Cu) (tedit 59DBE374)
    (at 185.166 77.724 180)
    (fp_text reference U2 (at 0 5.334) (layer F.SilkS) hide)
    (fp_text value RFM69CW (at 0 -6.985) (layer F.SilkS))
    (pad 4 smd rect (at -8.001 0 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad4)") (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -8.001 -5.99948 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad1)") (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -8.001 -4.0005 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -8.001 -1.99898 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -8.001 1.99898 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 18 MOSI) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at -8.001 4.0005 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 16 SCK) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at -8.001 5.99948 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 15 RF|SEL) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at 8.001 5.99948 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 20 MISO) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at 8.001 4.0005 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad9)") (solder_mask_margin 0.0508))
    (pad 10 smd rect (at 8.001 1.99898 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad10)") (solder_mask_margin 0.0508))
    (pad 11 smd rect (at 8.001 0 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad11)") (solder_mask_margin 0.0508))
    (pad 12 smd rect (at 8.001 -1.99898 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad12)") (solder_mask_margin 0.0508))
    (pad 13 smd rect (at 8.001 -4.0005 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad13)") (solder_mask_margin 0.0508))
    (pad 14 smd rect (at 8.001 -5.99948 180) (size 2.49936 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 4 GND) (solder_mask_margin 0.0508))
  )
  (gr_line (start 195.58 92.329) (end 196.215 91.694) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.59 92.329) (end 148.59 88.138) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 195.58 92.329) (end 148.59 92.329) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 147.447 63.627) (end 147.447 86.868) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 189.865 63.627) (end 147.447 63.627) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 189.865 67.945) (end 189.865 63.627) (layer Edge.Cuts) (width 0.127))
  (gr_text vdd (at 169.799 88.265 270) (layer B.SilkS))
  (gr_text 1.0 (at 169.799 85.725 270) (layer B.SilkS))
  (gr_text "1.1\nrx" (at 169.164 83.185 270) (layer B.SilkS))
  (gr_text "1.2\ntx" (at 169.164 80.645 270) (layer B.SilkS))
  (gr_text 1.3 (at 169.799 78.105 270) (layer B.SilkS))
  (gr_text 1.4 (at 169.799 75.565 270) (layer B.SilkS))
  (gr_text "1.5\nsck" (at 169.164 73.025 270) (layer B.SilkS))
  (gr_text 2.0 (at 169.799 70.485 270) (layer B.SilkS))
  (gr_text 2.1 (at 169.799 67.945 270) (layer B.SilkS))
  (gr_text 2.2 (at 169.799 65.405 270) (layer B.SilkS))
  (gr_text 2.3 (at 165.481 65.405 90) (layer B.SilkS))
  (gr_text 2.4 (at 165.481 67.945 90) (layer B.SilkS))
  (gr_text 2.5 (at 165.481 70.485 90) (layer B.SilkS))
  (gr_text "1.6\nmiso" (at 166.116 73.025 90) (layer B.SilkS))
  (gr_text "1.7\nmosi" (at 166.116 75.565 90) (layer B.SilkS))
  (gr_text rst (at 165.481 78.105 90) (layer B.SilkS))
  (gr_text test (at 165.481 80.645 90) (layer B.SilkS))
  (gr_text "2.7\nxout" (at 166.116 83.185 90) (layer B.SilkS))
  (gr_text "2.6\nxin" (at 166.116 85.725 90) (layer B.SilkS))
  (gr_text gnd (at 165.608 88.265 90) (layer B.SilkS))
  (gr_text "(c)flabbergast" (at 155.956 84.201) (layer B.SilkS))
  (gr_text "msp430g2553\nsensor board\nrev1 2019.06" (at 193.04 81.915 90) (layer B.SilkS))
  (gr_text "ant\n1" (at 191.516 83.82) (layer F.SilkS))
  (gr_text vin (at 177.927 69.342) (layer B.SilkS))
  (gr_text gnd (at 175.895 69.342) (layer B.SilkS))
  (gr_text gnd (at 184.658 85.09) (layer B.SilkS))
  (gr_text vdd (at 184.658 70.485) (layer B.SilkS))
  (gr_text MSP430G2553 (at 167.64 76.835 90) (layer F.SilkS))
  (gr_line (start 147.447 86.868) (end 148.59 88.011) (layer Edge.Cuts) (width 0.127))
  (gr_text vin (at 180.594 75.565 90) (layer B.SilkS))
  (gr_text reg.i (at 182.245 72.644) (layer B.SilkS))
  (gr_text vdd (at 182.245 78.232 180) (layer B.SilkS))
  (gr_text reg.o (at 189.611 81.915 270) (layer B.SilkS))
  (gr_text vdd (at 185.293 81.915 90) (layer B.SilkS))
  (gr_text reset (at 161.544 87.884 270) (layer F.SilkS))
  (gr_text "C1,C2:0.1uF\nC3,C4:1-22uF\n 0805\nU3:MCP1703T\n SOT-23A\ncrystal:\n 32768kHz" (at 181.1274 76.962) (layer F.SilkS))
  (gr_text ant (at 191.643 90.17 90) (layer B.SilkS))
  (gr_text gnd (at 161.544 80.645 270) (layer F.SilkS))
  (gr_text gnd (at 161.544 80.645 270) (layer B.SilkS))
  (gr_text vdd (at 161.544 78.105 270) (layer B.SilkS))
  (gr_text vdd (at 161.544 78.105 270) (layer F.SilkS))
  (gr_text 1.0 (at 161.417 75.565 270) (layer B.SilkS))
  (gr_text 1.3 (at 161.417 73.025 270) (layer B.SilkS))
  (gr_text 1.4 (at 161.417 70.485 270) (layer B.SilkS))
  (gr_text 1.7 (at 158.496 74.295) (layer B.SilkS))
  (gr_text 1.5 (at 158.496 71.755) (layer B.SilkS))
  (gr_text 1.6 (at 158.496 69.088) (layer B.SilkS))
  (gr_text 2.1 (at 148.209 65.405 90) (layer B.SilkS))
  (gr_text 2.2 (at 148.209 67.945 90) (layer B.SilkS))
  (gr_text 2.3 (at 148.209 70.485 90) (layer B.SilkS))
  (gr_text 2.4 (at 148.209 73.025 90) (layer B.SilkS))
  (gr_text 2.5 (at 148.209 75.565 90) (layer B.SilkS))
  (gr_text rst (at 148.209 78.105 90) (layer B.SilkS))
  (gr_text 1.2 (at 148.209 80.645 90) (layer B.SilkS))
  (gr_text vin (at 148.209 85.725 90) (layer B.SilkS))
  (gr_text 1.1 (at 148.209 83.185 90) (layer B.SilkS))
  (gr_text 2.1 (at 148.209 65.405 90) (layer F.SilkS))
  (gr_text 2.2 (at 148.209 67.945 90) (layer F.SilkS))
  (gr_text 2.3 (at 148.209 70.485 90) (layer F.SilkS))
  (gr_text 2.4 (at 148.209 73.025 90) (layer F.SilkS))
  (gr_text 2.5 (at 148.209 75.565 90) (layer F.SilkS))
  (gr_text rst (at 148.209 78.105 90) (layer F.SilkS))
  (gr_text tx (at 148.209 80.645 90) (layer F.SilkS))
  (gr_text rx (at 148.209 83.185 90) (layer F.SilkS))
  (gr_text vin (at 148.209 85.725 90) (layer F.SilkS))
  (gr_text mos (at 158.496 74.295) (layer F.SilkS))
  (gr_text sck (at 158.496 71.755) (layer F.SilkS))
  (gr_text mis (at 158.496 69.088) (layer F.SilkS))
  (gr_text 1.4 (at 161.417 70.485 270) (layer F.SilkS))
  (gr_text 1.3 (at 161.417 73.025 270) (layer F.SilkS))
  (gr_text 1.0 (at 161.417 75.565 270) (layer F.SilkS))
  (gr_line (start 148.59 88.138) (end 148.59 88.011) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 196.215 91.44) (end 196.215 91.694) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 196.215 69.85) (end 196.215 91.44) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 191.77 69.85) (end 196.215 69.85) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 189.865 67.945) (end 191.77 69.85) (layer Edge.Cuts) (width 0.127))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.8 87.2744) (xy 180.594 87.2744) (xy 181.864 88.5444) (xy 181.864 90.8304) (xy 180.594 92.1004)
        (xy 177.8 92.1004) (xy 176.53 90.8304) (xy 176.53 88.5444)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 195.58 92.075) (xy 195.58 70.485) (xy 173.99 70.485) (xy 173.99 92.075)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.3))
    (polygon
      (pts
        (xy 195.58 92.075) (xy 195.58 70.485) (xy 173.99 70.485) (xy 173.99 92.075)
      )
    )
  )
)
