(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 101)
    (zones 0)
    (modules 47)
    (nets 18)
  )
  (page USLetter)
  (title_block
    (title "Dyna ST-70 Power Board")
    (date "March 9, 2018")
    (rev A)
    (company "SDS Labs")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (user_trace_width 1.905)
    (user_trace_width 2.54)
    (user_trace_width 3.175)
    (user_trace_width 3.81)
    (user_trace_width 4.445)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 76.2 152.4)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(B+1-Pad1)")
  (net 2 "Net-(B+2-Pad1)")
  (net 3 "Net-(BiasIn1-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C1-Pad2)")
  (net 6 "Net-(C2-Pad2)")
  (net 7 "Net-(C3-Pad1)")
  (net 8 "Net-(C4-Pad1)")
  (net 9 "Net-(C5-Pad2)")
  (net 10 "Net-(C5-Pad1)")
  (net 11 "Net-(C7-Pad2)")
  (net 12 "Net-(C7-Pad1)")
  (net 13 "Net-(C10-Pad1)")
  (net 14 "Net-(C9-Pad1)")
  (net 15 "Net-(C11-Pad2)")
  (net 16 "Net-(C11-Pad1)")
  (net 17 "Net-(FromBiasPots1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(B+1-Pad1)")
    (add_net "Net-(B+2-Pad1)")
    (add_net "Net-(BiasIn1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(FromBiasPots1-Pad1)")
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B6D)
    (at 137.16 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference B+1 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 1 "Net-(B+1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B71)
    (at 144.145 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference B+2 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 2 "Net-(B+2-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842A6B)
    (at 97.79 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference BiasIn (at 3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 3 "Net-(BiasIn1-Pad1)"))
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5C842A0E)
    (at 93.98 46.99)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0 2.54) (layer F.SilkS))
    (fp_text value "100uf 100v" (at 1.905 0 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5C842A28)
    (at 88.265 46.99 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value "100uf 100v" (at 1.905 0 270) (layer F.SilkS))
    (fp_text user %R (at 1.27 0.635 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4 (layer F.Cu) (tedit 5C842C39)
    (at 160.775 59.69)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (fp_text reference C3 (at 3.75 -1.27) (layer F.SilkS))
    (fp_text value "0.022uf 400v" (at 3.69 1.905) (layer F.SilkS))
    (fp_text user %R (at 3.75 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4 (layer F.Cu) (tedit 5C842C41)
    (at 179.705 59.69 180)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 5mm Capacitor")
    (fp_text reference C4 (at 3.81 1.27 180) (layer F.SilkS))
    (fp_text value "0.022uf 400v" (at 3.75 -1.905 180) (layer F.SilkS))
    (fp_text user %R (at 3.75 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W5.0mm_P7.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842CEF)
    (at 167.64 80.645)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C5 (at 3.175 -13.335) (layer F.SilkS))
    (fp_text value "82uf 400v" (at 5 16.25) (layer F.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "Net-(C5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842CE6)
    (at 177.8 111.76 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C6 (at 3.175 13.335 180) (layer F.SilkS))
    (fp_text value "82uf 400v" (at -0.635 4.445 180) (layer F.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 9 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842CDD)
    (at 140.97 96.52)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C7 (at 3.175 -13.335) (layer F.SilkS))
    (fp_text value "56uf 400v" (at 0 4.445) (layer F.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842CD4)
    (at 151.13 127.635 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C8 (at 3.175 13.335 180) (layer F.SilkS))
    (fp_text value "56uf 400v" (at 0 3.81 180) (layer F.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842CC5)
    (at 113.665 81.28)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C9 (at 3.175 -12.7) (layer F.SilkS))
    (fp_text value "56uf 400v" (at 0 4.445) (layer F.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 13 "Net-(C10-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842CB6)
    (at 123.825 112.395 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C10 (at 2.54 12.7 180) (layer F.SilkS))
    (fp_text value "56uf 400v" (at 0 4.445 180) (layer F.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 13 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842CA2)
    (at 86.36 97.155)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C11 (at 3.175 -13.335) (layer F.SilkS))
    (fp_text value "56uf 400v" (at 0 4.445) (layer F.SilkS))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D30.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5C842C94)
    (at 96.52 128.27 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=30mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 30mm Electrolytic Capacitor")
    (fp_text reference C12 (at 2.54 13.335 180) (layer F.SilkS))
    (fp_text value "56uf 400v" (at 0 3.81 180) (layer F.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 15 "Net-(C11-Pad2)"))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5C8429CB)
    (at 103.505 53.975 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.08 -2.54 180) (layer F.SilkS))
    (fp_text user %R (at 5.47 0 180) (layer F.Fab))
    (fp_text user K (at 0 -2.1 180) (layer F.Fab))
    (fp_text user K (at 0 -2.1 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(BiasIn1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5C842BF6)
    (at 137.16 61.595 90)
    (descr "Diode, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "Diode DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 10.795 -1.27 90) (layer F.SilkS))
    (fp_text value 1N5408 (at 8.255 1.27 90) (layer F.SilkS))
    (fp_text user K (at 0 -2.6 90) (layer F.SilkS) hide)
    (fp_text user K (at 0 -2.6 90) (layer F.Fab))
    (fp_text user %R (at 8.3325 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(B+1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5C842BFA)
    (at 144.145 61.595 90)
    (descr "Diode, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "Diode DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D3 (at 10.795 -1.27 90) (layer F.SilkS))
    (fp_text value 1N5408 (at 8.255 1.27 90) (layer F.SilkS))
    (fp_text user %R (at 8.3325 0 90) (layer F.Fab))
    (fp_text user K (at 0 -2.6 90) (layer F.Fab))
    (fp_text user K (at 0 -2.6 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 "Net-(B+2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842AF4)
    (at 108.585 50.165)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference eye19 (at -3.175 -11.43 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 16 "Net-(C11-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842AB2)
    (at 108.585 44.45)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference eye19-2 (at 0 -10.16) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 16 "Net-(C11-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842AF0)
    (at 108.585 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference eye19-3 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 16 "Net-(C11-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B04)
    (at 115.57 50.165)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference eye20 (at -3.175 -11.43 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B19)
    (at 115.57 44.45)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference eye20-2 (at 0 -10.16) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B16)
    (at 115.57 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference eye20-3 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842C1A)
    (at 184.785 59.69)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference FilCT1 (at 0 3.81) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 8 "Net-(C4-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842C1F)
    (at 155.575 59.69)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference FilCT2 (at 0 3.81) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 7 "Net-(C3-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842A9D)
    (at 82.55 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference FrmPots (at 3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 17 "Net-(FromBiasPots1-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B5F)
    (at 129.54 44.45)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference Cath (at -3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842BA9)
    (at 122.555 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference frmInd (at -3.175 0.635 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842C83)
    (at 184.658 96.012)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference GND (at 0.762 -3.302) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B28)
    (at 122.555 50.165)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference Out1 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad1)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B34)
    (at 122.555 44.45)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference Out2 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad1)"))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C8429A1)
    (at 80.645 53.975)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0) (layer F.SilkS))
    (fp_text value "10K 0.25w" (at 5.08 2.37) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C8428ED)
    (at 78.105 40.386 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value "10K 0.25w" (at 16.129 0 270) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(FromBiasPots1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5C84296D)
    (at 109.855 61.468)
    (descr "Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=20.32mm, 1.5W, length*diameter=14.3*5.7mm^2")
    (tags "Resistor Axial_DIN0614 series Axial Horizontal pin pitch 20.32mm 1.5W length 14.3mm diameter 5.7mm")
    (fp_text reference R3 (at 4.445 2.032) (layer F.SilkS))
    (fp_text value "6.8k 2w" (at 10.795 2.032) (layer F.SilkS))
    (fp_text user %R (at 10.16 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 20.32 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 12 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5C842951)
    (at 85.09 61.468)
    (descr "Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=20.32mm, 1.5W, length*diameter=14.3*5.7mm^2")
    (tags "Resistor Axial_DIN0614 series Axial Horizontal pin pitch 20.32mm 1.5W length 14.3mm diameter 5.7mm")
    (fp_text reference R4 (at 4.445 2.032) (layer F.SilkS))
    (fp_text value "22k 2w" (at 10.795 2.032) (layer F.SilkS))
    (fp_text user %R (at 10.16 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842EAB)
    (at 172.5325 86.36)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 2.62) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 9 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842EB4)
    (at 172.72 105.41 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 2.62 180) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 9 "Net-(C5-Pad2)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842E9F)
    (at 146.05 102.235)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 2.62) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 11 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 12 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842EA5)
    (at 146.2375 121.285 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 2.62 180) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 11 "Net-(C7-Pad2)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842E8A)
    (at 118.5575 86.995)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 2.62) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 13 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 14 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842E99)
    (at 118.8115 106.426 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 2.62 180) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 13 "Net-(C10-Pad1)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842E84)
    (at 91.2525 102.87)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 2.62) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62) (layer B.SilkS))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 15 "Net-(C11-Pad2)"))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 16 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5C842E93)
    (at 91.694 122.555 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 2.62 180) (layer B.SilkS))
    (fp_text value "470k 1w" (at 0 -2.62 180) (layer B.SilkS))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 15 "Net-(C11-Pad2)"))
    (pad 2 smd roundrect (at 2.9875 0 180) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842A85)
    (at 90.17 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference ToPots (at 3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 6 "Net-(C2-Pad2)"))
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5C842B51)
    (at 129.54 38.735)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference toInd (at -3.175 0 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
  )
  (module sdsLogos:sdsLabs-large-fSilk (layer F.Cu) (tedit 5C842E4B)
    (at 120.65 137.16)
    (fp_text reference G*** (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -5.08) (layer F.SilkS) hide)
  )
  (gr_text "Dyna ST-70 Power Board" (at 118.745 143.51) (layer F.SilkS))
  (gr_circle (center 146.05 74.295) (end 148.4376 74.295) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 88.9 74.295) (end 91.2876 74.295) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 146.05 147.955) (end 148.4376 147.955) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 88.9 147.955) (end 91.2876 147.955) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 152.4) (end 76.2 152.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.56 127) (end 162.56 152.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 127) (end 162.56 127) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 55.88) (end 187.96 127) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 55.88) (end 187.96 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 35.56) (end 147.32 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 35.56) (end 147.32 35.56) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.2 152.4) (end 76.2 35.56) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.105 57.15) (xy 80.645 57.15) (xy 80.645 121.285) (xy 88.9 121.285) (xy 88.9 135.255)
        (xy 104.775 135.255) (xy 104.775 105.41) (xy 116.205 105.41) (xy 116.205 118.11) (xy 143.51 118.11)
        (xy 143.51 135.255) (xy 157.48 135.255) (xy 157.48 104.14) (xy 170.18 104.14) (xy 170.18 118.11)
        (xy 181.61 118.11) (xy 181.61 67.31) (xy 187.96 67.31) (xy 187.96 127) (xy 162.56 127)
        (xy 162.56 152.4) (xy 76.2 152.4) (xy 76.2 50.8) (xy 78.105 50.8)
      )
    )
  )
)
