(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-4")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 146)
    (zones 0)
    (modules 21)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 Isen)
  (net 3 GND)
  (net 4 RL4)
  (net 5 RL3)
  (net 6 RL2)
  (net 7 RL1)
  (net 8 B+4)
  (net 9 B+3)
  (net 10 B+2)
  (net 11 B+1)
  (net 12 Supply)
  (net 13 Vin)
  (net 14 BV1)
  (net 15 BV2)
  (net 16 BV3)
  (net 17 BV4)
  (net 18 Vs)
  (net 19 Vss)
  (net 20 "Net-(uC1-Pad1)")
  (net 21 "Net-(uC1-Pad37)")
  (net 22 "Net-(uC1-Pad2)")
  (net 23 "Net-(uC1-Pad36)")
  (net 24 "Net-(uC1-Pad3)")
  (net 25 "Net-(uC1-Pad35)")
  (net 26 "Net-(uC1-Pad4)")
  (net 27 "Net-(uC1-Pad5)")
  (net 28 "Net-(uC1-Pad6)")
  (net 29 "Net-(uC1-Pad7)")
  (net 30 "Net-(uC1-Pad8)")
  (net 31 "Net-(uC1-Pad9)")
  (net 32 "Net-(uC1-Pad10)")
  (net 33 "Net-(uC1-Pad11)")
  (net 34 "Net-(uC1-Pad12)")
  (net 35 "Net-(uC1-Pad14)")
  (net 36 "Net-(uC1-Pad15)")
  (net 37 "Net-(uC1-Pad16)")
  (net 38 "Net-(uC1-Pad17)")
  (net 39 "Net-(uC1-Pad21)")
  (net 40 "Net-(uC1-Pad18)")
  (net 41 "Net-(uC1-Pad20)")
  (net 42 "Net-(J6-Pad4)")
  (net 43 "Net-(uC1-Pad34)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net B+1)
    (add_net B+2)
    (add_net B+3)
    (add_net B+4)
    (add_net BV1)
    (add_net BV2)
    (add_net BV3)
    (add_net BV4)
    (add_net GND)
    (add_net Isen)
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(uC1-Pad1)")
    (add_net "Net-(uC1-Pad10)")
    (add_net "Net-(uC1-Pad11)")
    (add_net "Net-(uC1-Pad12)")
    (add_net "Net-(uC1-Pad14)")
    (add_net "Net-(uC1-Pad15)")
    (add_net "Net-(uC1-Pad16)")
    (add_net "Net-(uC1-Pad17)")
    (add_net "Net-(uC1-Pad18)")
    (add_net "Net-(uC1-Pad2)")
    (add_net "Net-(uC1-Pad20)")
    (add_net "Net-(uC1-Pad21)")
    (add_net "Net-(uC1-Pad3)")
    (add_net "Net-(uC1-Pad34)")
    (add_net "Net-(uC1-Pad35)")
    (add_net "Net-(uC1-Pad36)")
    (add_net "Net-(uC1-Pad37)")
    (add_net "Net-(uC1-Pad4)")
    (add_net "Net-(uC1-Pad5)")
    (add_net "Net-(uC1-Pad6)")
    (add_net "Net-(uC1-Pad7)")
    (add_net "Net-(uC1-Pad8)")
    (add_net "Net-(uC1-Pad9)")
    (add_net RL1)
    (add_net RL2)
    (add_net RL3)
    (add_net RL4)
    (add_net Supply)
    (add_net Vin)
    (add_net Vs)
    (add_net Vss)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 114.173 79.121 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Isense (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Isen))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127.762 79.121 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "Quad Relay Pack" (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 RL4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 RL3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 RL2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 RL1))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 148.819381 84.159491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 33k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 B+1))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 BV1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 148.819381 87.729491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 BV1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 151.359381 84.145491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.397 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 B+2))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 BV2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 151.359381 87.729491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -0.141 -1.397 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 BV2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 153.899381 84.145491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0.141 -1.27 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 B+3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 BV3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 153.899381 87.715491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -3.062 0 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 BV3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 156.439381 84.159491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 B+4))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 BV4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 156.439381 87.701491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 BV4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 146.279381 84.145491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Vin))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Vs))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 146.279381 87.729491 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Vs))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 127.762 103.138 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Supply))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 Vss))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 129.54 103.138 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.43 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 Vss))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FootPrints:ESP-32S (layer F.Cu) (tedit 5C802CE2)
    (at 135.330001 110.160001)
    (fp_text reference uC1 (at -17.78 0 90) (layer F.SilkS))
    (fp_text value ESP-32S (at 0 0) (layer F.Fab))
    (fp_text user GND (at 10.287 8.89 90) (layer F.SilkS))
    (fp_text user GND (at -10.16 -8.763 90) (layer F.SilkS))
    (fp_text user GND (at 22.86 8.763 90) (layer F.SilkS))
    (fp_text user 3V3 (at 22.86 -8.89 90) (layer F.SilkS))
    (fp_text user Vin (at -22.987 -9.017 90) (layer F.SilkS))
    (fp_text user USB (at -21.844 0 90) (layer F.SilkS))
    (pad 38 thru_hole oval (at -22.86 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole oval (at -22.86 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(uC1-Pad1)"))
    (pad 37 thru_hole oval (at -20.32 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(uC1-Pad37)"))
    (pad 2 thru_hole oval (at -20.32 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(uC1-Pad2)"))
    (pad 36 thru_hole oval (at -17.78 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(uC1-Pad36)"))
    (pad 3 thru_hole oval (at -17.78 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(uC1-Pad3)"))
    (pad 35 thru_hole oval (at -15.24 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(uC1-Pad35)"))
    (pad 4 thru_hole oval (at -15.24 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(uC1-Pad4)"))
    (pad 34 thru_hole oval (at -12.7 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(uC1-Pad34)"))
    (pad 5 thru_hole oval (at -12.7 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(uC1-Pad5)"))
    (pad 33 thru_hole oval (at -10.16 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole oval (at -10.16 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(uC1-Pad6)"))
    (pad 32 thru_hole oval (at -7.62 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 Vss))
    (pad 7 thru_hole oval (at -7.62 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(uC1-Pad7)"))
    (pad 31 thru_hole oval (at -5.08 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 RL4))
    (pad 8 thru_hole oval (at -5.08 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(uC1-Pad8)"))
    (pad 30 thru_hole oval (at -2.54 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 RL3))
    (pad 9 thru_hole oval (at -2.54 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(uC1-Pad9)"))
    (pad 29 thru_hole oval (at 0 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 RL2))
    (pad 10 thru_hole oval (at 0 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(uC1-Pad10)"))
    (pad 28 thru_hole oval (at 2.54 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 RL1))
    (pad 11 thru_hole oval (at 2.54 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(uC1-Pad11)"))
    (pad 27 thru_hole oval (at 5.08 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Isen))
    (pad 12 thru_hole oval (at 5.08 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(uC1-Pad12)"))
    (pad 26 thru_hole oval (at 7.62 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 Vs))
    (pad 13 thru_hole oval (at 7.62 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 25 thru_hole oval (at 10.16 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 BV1))
    (pad 14 thru_hole oval (at 10.16 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(uC1-Pad14)"))
    (pad 24 thru_hole oval (at 12.7 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 BV2))
    (pad 15 thru_hole oval (at 12.7 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(uC1-Pad15)"))
    (pad 23 thru_hole oval (at 15.24 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 BV3))
    (pad 16 thru_hole oval (at 15.24 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(uC1-Pad16)"))
    (pad 22 thru_hole oval (at 17.78 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 BV4))
    (pad 17 thru_hole oval (at 17.78 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(uC1-Pad17)"))
    (pad 21 thru_hole oval (at 20.32 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(uC1-Pad21)"))
    (pad 18 thru_hole oval (at 20.32 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(uC1-Pad18)"))
    (pad 20 thru_hole oval (at 22.86 -11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(uC1-Pad20)"))
    (pad 19 thru_hole oval (at 22.86 11.43) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.871 93.726)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value GND (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.871 83.693)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Supply (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 Supply))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 117.475 110.49 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value Vreg (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 Supply))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J6-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D13.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 121.031 85.725 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=13mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 13mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -7.75 270) (layer F.SilkS))
    (fp_text value CP (at 2.5 7.75 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 Supply))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D13.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 146.304 79.121 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value voltages (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 Vin))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 B+1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 B+2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 B+3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 B+4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Axial_L18.0mm_D10.0mm_P25.00mm_Horizontal (layer F.Cu) (tedit 5AE50EF2)
    (at 130.175 114.3)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*10mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
    (tags "CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 12.5 -6.12) (layer F.SilkS))
    (fp_text value CP (at 12.5 6.12) (layer F.Fab))
    (fp_text user %R (at 12.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 25 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Axial_L18.0mm_D10.0mm_P25.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 159.385 123.19) (end 109.22 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 77.47) (end 159.385 77.47) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 77.47) (end 109.22 123.19) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.385 123.19) (end 159.385 77.47) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.22 77.47) (xy 159.385 77.47) (xy 159.385 123.19) (xy 109.22 123.19)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.385 123.19) (xy 159.385 77.47) (xy 109.22 77.47) (xy 109.22 123.19)
      )
    )
  )
)
