(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 12)
    (no_connects 0)
    (area 128.694999 85.649999 154.245001 100.887601)
    (thickness 1.6)
    (drawings 19)
    (tracks 24)
    (zones 0)
    (modules 8)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.16)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 1.524)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 130.04 88.9)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 0)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory G:/gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(P1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad2)")
  )
  (net_class POWER ""
    (clearance 0.16)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(P1-Pad2)")
  )
  (module switch (layer F.Cu) (tedit 5914D1B8)
    (at 134.358 98.298)
    (fp_text reference SW1 (at 3.048 -3.0988) (layer F.SilkS))
    (fp_text value SW_Push_SPDT (at 5 -5) (layer F.Fab))
    (pad 3 thru_hole oval (at 6 0) (size 2.5 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 3 0) (size 2.5 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 2.5 1.524) (drill oval 1) (layers *.Cu *.Mask))
  )
  (module multimeter:std_resistor (layer F.Cu) (tedit 5914D1E1)
    (at 144.272 94.996 90)
    (fp_text reference R1 (at 3.937 0.0174 90) (layer F.SilkS))
    (fp_text value 100R (at 4.6 -4.8 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
  )
  (module TO_SOT_Packages_THT:TO-220_Vertical (layer F.Cu) (tedit 5914D204)
    (at 134.62 88.9)
    (descr "TO-220, Vertical, RM 2.54mm")
    (tags "TO-220 Vertical RM 2.54mm")
    (fp_text reference U1 (at 2.6082 2.8702) (layer F.SilkS))
    (fp_text value LM7805 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module multimeter:std_cap (layer F.Cu) (tedit 5914D1FE)
    (at 142.1812 93.3704 180)
    (fp_text reference C2 (at 1.9558 -0.0254 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 5.08 -3.175 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module multimeter:std_cap (layer F.Cu) (tedit 5914D1F9)
    (at 132.453 93.3958)
    (fp_text reference C1 (at 1.9558 0.0508) (layer F.SilkS))
    (fp_text value 0.33uF (at 5.08 -3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module multimeter:std_wirepads (layer F.Cu) (tedit 591417F2)
    (at 130.048 91.44 90)
    (fp_text reference P1 (at -2.0574 0.1063 180) (layer F.SilkS) hide)
    (fp_text value INPUTV (at 1.27 1.27 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad2)"))
  )
  (module multimeter:std_wirepads (layer F.Cu) (tedit 591417F8)
    (at 152.9 88.9 270)
    (fp_text reference P2 (at 0 1.778 270) (layer F.SilkS) hide)
    (fp_text value OUTPUTV (at 1.905 -3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5914D1C8)
    (at 148.082 91.44 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at -1.905 -0.0588 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 142.359 98.806) (end 142.359 100.8126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.391 96.774) (end 142.359 98.806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.3514 100.8126) (end 142.359 100.8126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.3514 98.8314) (end 132.3514 100.8126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.3514 98.8314) (end 128.77 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 10 (width 0.3) (layer F.SilkS)
    (gr_text "10.000 mm" (at 136.04 77.9) (layer F.SilkS))
    (feature1 (pts (xy 139.04 83.9) (xy 139.04 79.2)))
    (feature2 (pts (xy 129.04 83.9) (xy 129.04 79.2)))
    (crossbar (pts (xy 129.04 81.9) (xy 139.04 81.9)))
    (arrow1a (pts (xy 139.04 81.9) (xy 137.913496 82.486421)))
    (arrow1b (pts (xy 139.04 81.9) (xy 137.913496 81.313579)))
    (arrow2a (pts (xy 129.04 81.9) (xy 130.166504 82.486421)))
    (arrow2b (pts (xy 129.04 81.9) (xy 130.166504 81.313579)))
  )
  (gr_text "Trevor van Ginkel" (at 137.1139 96.2406) (layer B.SilkS))
  (gr_text "LM78XX adapter board" (at 138.7522 91.4654) (layer B.SilkS))
  (gr_line (start 139.8571 98.298) (end 140.8604 98.298) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 136.8472 98.298) (end 137.8505 98.298) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 133.85 98.298) (end 134.866 98.298) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 144.391 96.774) (end 149.471 96.774) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.77 88.9) (end 128.77 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.17 85.725) (end 154.17 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.17 92.075) (end 149.471 96.774) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text VIN (at 130.421 86.868) (layer F.SilkS))
  (gr_text +5V (at 152.138 86.868) (layer F.SilkS))
  (gr_line (start 128.77 85.725) (end 154.17 85.725) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.77 88.9) (end 128.77 85.725) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.17 92.075) (xy 149.471 96.774) (xy 144.391 96.774) (xy 142.359 98.806) (xy 142.359 100.8126)
        (xy 132.3514 100.8126) (xy 132.3514 98.8314) (xy 128.77 95.25) (xy 128.77 85.725) (xy 154.17 85.725)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.17 92.075) (xy 149.471 96.774) (xy 144.391 96.774) (xy 142.359 98.806) (xy 142.359 100.8126)
        (xy 132.3514 100.8126) (xy 132.3514 98.8314) (xy 128.77 95.25) (xy 128.77 85.725) (xy 154.17 85.725)
      )
    )
  )
)
