(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 18)
    (no_connects 0)
    (area 133.63 54.024999 159.042002 161.075001)
    (thickness 1.6)
    (drawings 6)
    (tracks 298)
    (zones 0)
    (modules 4)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad5)")
  (net 2 "Net-(U1-Pad6)")
  (net 3 "Net-(U1-Pad7)")
  (net 4 "Net-(U1-Pad8)")
  (net 5 "Net-(U1-Pad9)")
  (net 6 "Net-(U1-Pad4)")
  (net 7 "Net-(U1-Pad3)")
  (net 8 "Net-(U1-Pad2)")
  (net 9 "Net-(U1-Pad1)")
  (net 10 "Net-(U2-Pad5)")
  (net 11 "Net-(U2-Pad6)")
  (net 12 "Net-(U2-Pad7)")
  (net 13 "Net-(U2-Pad8)")
  (net 14 "Net-(U2-Pad9)")
  (net 15 "Net-(U2-Pad4)")
  (net 16 "Net-(U2-Pad3)")
  (net 17 "Net-(U2-Pad2)")
  (net 18 "Net-(U2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
  )
  (module .pretty:usb3 (layer F.Cu) (tedit 5852EDAE)
    (at 145.43 86.9)
    (fp_text reference U1 (at -9.8 -6) (layer F.SilkS))
    (fp_text value usb3.0 (at -9.1 -7.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 10.7 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 5.8) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 10.7 5.8) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 1.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 3.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 5.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 7.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 9.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad9)"))
    (pad 4 thru_hole circle (at 1.83 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at 4.33 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at 6.33 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad2)"))
    (pad 1 thru_hole circle (at 8.83 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad1)"))
  )
  (module .pretty:usb3 (layer F.Cu) (tedit 5852EDAE)
    (at 145.43 98.14)
    (fp_text reference U2 (at -9.8 -6) (layer F.SilkS))
    (fp_text value usb3.0 (at -9.1 -7.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 10.7 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 5.8) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 10.7 5.8) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 1.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at 3.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at 5.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at 7.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad8)"))
    (pad 9 thru_hole circle (at 9.33 1.4) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad9)"))
    (pad 4 thru_hole circle (at 1.83 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad4)"))
    (pad 3 thru_hole circle (at 4.33 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad3)"))
    (pad 2 thru_hole circle (at 6.33 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad2)"))
    (pad 1 thru_hole circle (at 8.83 3.8) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(U2-Pad1)"))
  )
  (module .pretty:usb3reg (layer F.Cu) (tedit 5852ECF4)
    (at 155 128)
    (fp_text reference U3 (at -9.41 -6.17) (layer F.SilkS))
    (fp_text value usb3.0 (at -8.37 -7.62) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 13.4) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -3.5 2.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad9)"))
    (pad 8 thru_hole circle (at -3.5 4.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad8)"))
    (pad 7 thru_hole circle (at -3.5 6.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad7)"))
    (pad 6 thru_hole circle (at -3.5 8.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad6)"))
    (pad 5 thru_hole circle (at -3.5 10.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 1 thru_hole circle (at -2 3.07) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(U2-Pad1)"))
    (pad 2 thru_hole circle (at -2 5.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad2)"))
    (pad 3 thru_hole circle (at -2 7.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at -2 10.07) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad4)"))
  )
  (module .pretty:usb3reg (layer F.Cu) (tedit 5852ECF4)
    (at 155 110)
    (fp_text reference U4 (at -9.41 -6.17) (layer F.SilkS))
    (fp_text value usb3.0 (at -8.37 -7.62) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 13.4) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -3.5 2.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad9)"))
    (pad 8 thru_hole circle (at -3.5 4.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at -3.5 6.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad7)"))
    (pad 6 thru_hole circle (at -3.5 8.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at -3.5 10.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad5)"))
    (pad 1 thru_hole circle (at -2 3.07) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -2 5.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -2 7.57) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -2 10.07) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad4)"))
  )
  (gr_circle (center 142.65 157.15) (end 140.7 157.15) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 153.25 57.85) (end 153.25 55.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.8 54.1) (end 138.8 54.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.8 161) (end 158.8 54.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.8 161) (end 158.8 161) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.8 54.1) (end 138.8 161) (angle 90) (layer Edge.Cuts) (width 0.15))
)
