(kicad_pcb (version 20171130) (host pcbnew 5.1.4-e60b266~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 331)
    (zones 0)
    (modules 39)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 50.8 101.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 +5V)
  (net 4 VCC)
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(D1-Pad1)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 USB_D+)
  (net 10 USB_D-)
  (net 11 USB_VBUS)
  (net 12 "Net-(J2-Pad6)")
  (net 13 PS2_CLK)
  (net 14 "Net-(J2-Pad2)")
  (net 15 "Net-(J3-Pad15)")
  (net 16 VGA_VSYNCH)
  (net 17 VGA_HSYNCH)
  (net 18 "Net-(J3-Pad12)")
  (net 19 "Net-(J3-Pad11)")
  (net 20 "Net-(J3-Pad9)")
  (net 21 "Net-(J3-Pad4)")
  (net 22 "Net-(J3-Pad3)")
  (net 23 "Net-(J3-Pad2)")
  (net 24 "Net-(J3-Pad1)")
  (net 25 "Net-(J4-Pad3)")
  (net 26 COMPOSITE)
  (net 27 "Net-(J5-Pad3)")
  (net 28 SERIAL_TXD)
  (net 29 "Net-(J7-Pad6)")
  (net 30 ICSP_PCC)
  (net 31 ICSP_PGD)
  (net 32 ICSP_MCLR)
  (net 33 "Net-(JP1-Pad1)")
  (net 34 "Net-(JP6-Pad1)")
  (net 35 "Net-(JP7-Pad1)")
  (net 36 "Net-(R2-Pad1)")
  (net 37 SERIAL_RXD)
  (net 38 "Net-(R9-Pad1)")
  (net 39 "Net-(U1-Pad26)")
  (net 40 VGA_VIDEO)
  (net 41 PS2_DATA)
  (net 42 "Net-(R10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net COMPOSITE)
    (add_net GND)
    (add_net ICSP_MCLR)
    (add_net ICSP_PCC)
    (add_net ICSP_PGD)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP6-Pad1)")
    (add_net "Net-(JP7-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad26)")
    (add_net PS2_CLK)
    (add_net PS2_DATA)
    (add_net SERIAL_RXD)
    (add_net SERIAL_TXD)
    (add_net USB_D+)
    (add_net USB_D-)
    (add_net USB_VBUS)
    (add_net VCC)
    (add_net VGA_HSYNCH)
    (add_net VGA_VIDEO)
    (add_net VGA_VSYNCH)
  )
  (module terminal:CUI_MD-60SM locked (layer F.Cu) (tedit 5DB8B56F)
    (at 120.65 142.24 270)
    (fp_text reference J2 (at 5.588 7.62 90) (layer F.SilkS))
    (fp_text value PS2 (at -5.334 7.62 90) (layer F.SilkS))
    (fp_text user PANEL~FRONT (at -1.0923 -5.88804 90) (layer F.Cu) hide)
    (pad S3 thru_hole oval (at 6.75 -1) (size 3.4 1.7) (drill oval 2.2 0.7) (layers *.Cu *.Mask))
    (pad S2 thru_hole oval (at -6.75 -1) (size 3.4 1.7) (drill oval 2.2 0.7) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.4 4.5 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad6)"))
    (pad 5 thru_hole circle (at -3.4 4.5 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 PS2_CLK))
    (pad 4 thru_hole circle (at 3.4 2 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 1.3 2 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at -1.3 2 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 PS2_DATA))
    (pad 3 thru_hole circle (at -3.4 2 270) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 0 -1.8 270) (size 3.4 1.7) (drill oval 2.2 0.7) (layers *.Cu *.Mask))
  )
  (module terminal:SWITCHCRAFT_PJRAN1X1U01X locked (layer F.Cu) (tedit 5DB8B557)
    (at 67.31 155.956)
    (fp_text reference J4 (at -6.35 -4.826) (layer F.SilkS))
    (fp_text value Composite (at 1.524 -7.62) (layer F.SilkS))
    (fp_text user PCB~EDGE (at -3.75 2.37) (layer F.Cu) hide)
    (pad 1 thru_hole oval (at 0 0) (size 4 2) (drill oval 2.5 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 3.75 -3.7 90) (size 3.6 1.8) (drill oval 2.5 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at -3.75 -3.7 90) (size 3.6 1.8) (drill oval 2.5 1) (layers *.Cu *.Mask)
      (net 26 COMPOSITE))
  )
  (module terminal:TE_3-641215-2 locked (layer F.Cu) (tedit 5DA3559D)
    (at 111.76 106.68 180)
    (fp_text reference J6 (at -5.08 -0.508) (layer F.SilkS))
    (fp_text value "External 5V" (at -1.635 4.405) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module terminal:TE_3-641215-4 locked (layer F.Cu) (tedit 5DA355C8)
    (at 121.92 111.76 90)
    (fp_text reference J5 (at -9.906 0 180) (layer F.SilkS))
    (fp_text value Serial (at -6.715 4.405 90) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at -7.62 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad3)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 SERIAL_TXD))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Package_TO_SOT_THT:TO-92_HandSolder (layer F.Cu) (tedit 5A282C46)
    (at 64.135 105.41 180)
    (descr "TO-92 leads molded, narrow, drill 0.75mm, handsoldering variant with enlarged pads (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at 1.27 2.54) (layer F.SilkS))
    (fp_text value MCP1700-3302E_TO92 (at 1.27 2.79) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -4.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.1 1.8) (drill 0.75 (offset 0 0.4)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole roundrect (at 2.54 0 180) (size 1.1 1.8) (drill 0.75 (offset 0 0.4)) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 2 thru_hole roundrect (at 1.27 -1.27 180) (size 1.1 1.8) (drill 0.75 (offset 0 -0.4)) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 99.06 110.49)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 3.81 0) (layer F.SilkS))
    (fp_text value 82 (at 4.064 -2.286) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 80.645 135.255 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 3.81 0) (layer F.SilkS))
    (fp_text value 150 (at 3.81 2.54) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 COMPOSITE))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 80.645 140.335 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 3.81 0) (layer F.SilkS))
    (fp_text value 470 (at 3.81 2.54) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 COMPOSITE))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 VGA_HSYNCH))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 86.36 110.49 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.54) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 SERIAL_RXD))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 76.2 110.49 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 0) (layer F.SilkS))
    (fp_text value 100K (at 3.81 2.37) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 SERIAL_RXD))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 99.06 140.335 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 220 (at 3.81 -2.286 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 VGA_VIDEO))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 109.22 132.715 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.37 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 PS2_DATA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 104.14 132.715 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.37 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 PS2_CLK))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 106.68 105.41 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 4.7K (at 4.064 2.37) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 USB_VBUS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 96.52 110.49 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.54) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 ICSP_MCLR))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 123.444 105.41 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 54.61 105.41 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 54.356 156.464 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 56D1B4CB)
    (at 123.444 156.464 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 96.52 127.635)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 2.54 0) (layer F.SilkS))
    (fp_text value 27pF (at 2.5 -2.54) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 81.28 127.635 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.5 0) (layer F.SilkS))
    (fp_text value 27pF (at 2.5 2.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 111.76 127.635)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 2.54 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 -2.54) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 109.22 127.635 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.54 2.54) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_Tantal_D5.0mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 58.42 114.3 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 3.75) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_Tantal_D5.0mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 66.04 114.3 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C2 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 3.75) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_Tantal_D5.0mm_P5.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 124.46 127.635 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 3.81) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_HC49-U_Vertical placed (layer F.Cu) (tedit 5A1AD3B8)
    (at 91.44 128.905 180)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.44 0) (layer F.SilkS))
    (fp_text value 8MHz (at 2.44 3.525) (layer F.SilkS))
    (fp_text user %R (at 2.44 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 4.88 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W7.62mm_Socket placed (layer F.Cu) (tedit 5A02E8C5)
    (at 71.12 122.555 90)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at 3.81 16.51 180) (layer F.SilkS))
    (fp_text value PIC32MX250F128B-I_SP (at 3.556 27.686 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 16.51 180) (layer F.Fab))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R10-Pad1)"))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad26)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 VGA_VIDEO))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 VGA_HSYNCH))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(JP6-Pad1)"))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 VGA_VSYNCH))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 USB_D-))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 USB_D+))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(JP7-Pad1)"))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R9-Pad1)"))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 SERIAL_RXD))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 VGA_HSYNCH))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 SERIAL_TXD))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 PS2_CLK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 ICSP_PCC))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 PS2_DATA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 ICSP_PGD))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 ICSP_MCLR))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 88.9 137.795 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value B (at 0 4.87) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(JP7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 85.09 137.795 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP6 (at 0 -2.33) (layer F.SilkS))
    (fp_text value A (at 0 4.87) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(JP6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 92.71 137.795 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value C (at 0 4.87) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 ICSP_PCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 71.755 130.175 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "USB Power" (at 3.048 1.524 90) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 USB_VBUS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 63.246 140.97)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Blue (at 1.27 5.08) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad3)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 59.436 140.97)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Green (at 0 5.08) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(JP1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 55.626 140.97)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Red (at -1.016 5.08) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical locked (layer F.Cu) (tedit 59FED5CC)
    (at 69.215 105.41 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J7 (at 0 15.24 90) (layer F.SilkS))
    (fp_text value ICSP (at 2.54 6.985) (layer F.SilkS))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J7-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 ICSP_PCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 ICSP_PGD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 ICSP_MCLR))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module terminal:AMPHENOL_L77HDE15SD1CH4F locked (layer F.Cu) (tedit 0)
    (at 95.25 148.59)
    (fp_text reference J3 (at -2.54 -6.096) (layer F.SilkS))
    (fp_text value VGA (at 6.604 -6.096) (layer F.SilkS))
    (pad S2 thru_hole circle (at 12.495 0) (size 4.066 4.066) (drill 3.05) (layers *.Cu *.Mask))
    (pad S1 thru_hole circle (at -12.495 0) (size 4.066 4.066) (drill 3.05) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -4.83 2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad15)"))
    (pad 14 thru_hole circle (at -2.54 2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 16 VGA_VSYNCH))
    (pad 13 thru_hole circle (at -0.25 2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 17 VGA_HSYNCH))
    (pad 12 thru_hole circle (at 2.04 2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad12)"))
    (pad 11 thru_hole circle (at 4.33 2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad11)"))
    (pad 10 thru_hole circle (at -3.685 0) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -1.395 0) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad9)"))
    (pad 8 thru_hole circle (at 0.895 0) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 3.185 0) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 5.475 0) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -4.83 -2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -2.54 -2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad4)"))
    (pad 3 thru_hole circle (at -0.25 -2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 2.04 -2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 4.33 -2.54) (size 1.785 1.785) (drill 1.19) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)"))
  )
  (module terminal:OST_USB-B1HSB6 locked (layer F.Cu) (tedit 5D6166FB)
    (at 60.96 128.27 270)
    (fp_text reference J1 (at 7.112 -7.62) (layer F.SilkS))
    (fp_text value USB (at -8.89 2.54) (layer F.SilkS))
    (pad 5 thru_hole circle (at 6.02 0 270) (size 3.346 3.346) (drill 2.33) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 5 thru_hole circle (at -6.02 0 270) (size 3.346 3.346) (drill 2.33) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 4 thru_hole circle (at 1.25 -2.71 270) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -1.25 -2.71 270) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 9 USB_D+))
    (pad 2 thru_hole circle (at -1.25 -4.71 270) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 10 USB_D-))
    (pad 1 thru_hole rect (at 1.25 -4.71 270) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 11 USB_VBUS))
  )
  (module LED_THT:LED_D5.0mm locked (layer F.Cu) (tedit 5995936A)
    (at 114.3 115.57 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.524 -4.064) (layer F.SilkS))
    (fp_text value Status (at 1.27 3.96) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text VCC (at 125.984 120.396 90) (layer F.SilkS))
  (gr_text RX (at 125.984 116.84 90) (layer F.SilkS))
  (gr_text TX (at 125.984 114.3 90) (layer F.SilkS))
  (gr_text GND (at 125.984 110.744 90) (layer F.SilkS))
  (gr_text GND (at 115.316 102.87) (layer F.SilkS))
  (gr_text +5V (at 110.744 102.87) (layer F.SilkS))
  (gr_line (start 127 101.6) (end 127 160.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 101.6) (end 127 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 160.02) (end 50.8 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 160.02) (end 50.8 160.02) (layer Edge.Cuts) (width 0.05))
)
