(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 31)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 9)
    (tracks 79)
    (zones 0)
    (modules 17)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(M1-Pad1)")
  (net 5 "Net-(M2-Pad1)")
  (net 6 "Net-(M3-Pad1)")
  (net 7 GND)
  (net 8 "Net-(M4-Pad1)")
  (net 9 "Net-(Q1-Pad2)")
  (net 10 "Net-(Q2-Pad2)")
  (net 11 "Net-(R3-Pad2)")
  (net 12 "Net-(R4-Pad2)")
  (net 13 "Net-(SHIELD1-PadAD5)")
  (net 14 "Net-(SHIELD1-PadAD4)")
  (net 15 "Net-(SHIELD1-PadAD3)")
  (net 16 "Net-(SHIELD1-PadAD0)")
  (net 17 "Net-(SHIELD1-PadAD1)")
  (net 18 "Net-(SHIELD1-PadAD2)")
  (net 19 "Net-(SHIELD1-PadGND2)")
  (net 20 "Net-(SHIELD1-Pad3V3)")
  (net 21 "Net-(SHIELD1-PadRST)")
  (net 22 "Net-(SHIELD1-Pad4)")
  (net 23 "Net-(SHIELD1-Pad5)")
  (net 24 "Net-(SHIELD1-Pad6)")
  (net 25 "Net-(SHIELD1-Pad7)")
  (net 26 "Net-(SHIELD1-Pad8)")
  (net 27 "Net-(SHIELD1-Pad9)")
  (net 28 "Net-(SHIELD1-Pad10)")
  (net 29 "Net-(SHIELD1-Pad11)")
  (net 30 "Net-(SHIELD1-Pad12)")
  (net 31 "Net-(SHIELD1-Pad13)")
  (net 32 "Net-(SHIELD1-PadGND3)")
  (net 33 "Net-(SHIELD1-PadAREF)")
  (net 34 "Net-(SHIELD1-Pad5V)")
  (net 35 "Net-(D1-Pad2)")
  (net 36 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M2-Pad1)")
    (add_net "Net-(M3-Pad1)")
    (add_net "Net-(M4-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(SHIELD1-Pad10)")
    (add_net "Net-(SHIELD1-Pad11)")
    (add_net "Net-(SHIELD1-Pad12)")
    (add_net "Net-(SHIELD1-Pad13)")
    (add_net "Net-(SHIELD1-Pad3V3)")
    (add_net "Net-(SHIELD1-Pad4)")
    (add_net "Net-(SHIELD1-Pad5)")
    (add_net "Net-(SHIELD1-Pad5V)")
    (add_net "Net-(SHIELD1-Pad6)")
    (add_net "Net-(SHIELD1-Pad7)")
    (add_net "Net-(SHIELD1-Pad8)")
    (add_net "Net-(SHIELD1-Pad9)")
    (add_net "Net-(SHIELD1-PadAD0)")
    (add_net "Net-(SHIELD1-PadAD1)")
    (add_net "Net-(SHIELD1-PadAD2)")
    (add_net "Net-(SHIELD1-PadAD3)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadGND2)")
    (add_net "Net-(SHIELD1-PadGND3)")
    (add_net "Net-(SHIELD1-PadRST)")
  )
  (module "arduino_shields.mod:ARDUINO SHIELD" locked (layer F.Cu) (tedit 4CD6A37D)
    (at 104.05057 101.2992)
    (fp_text reference SHIELD1 (at 2.54 -57.15) (layer F.SilkS))
    (fp_text value ARDUINO_SHIELD (at 5.08 -54.61) (layer F.SilkS) hide)
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SHIELD1-PadAD3)"))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SHIELD1-PadAD0)"))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(SHIELD1-PadAD1)"))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(SHIELD1-PadAD2)"))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad1)"))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SHIELD1-PadGND2)"))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(SHIELD1-Pad3V3)"))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SHIELD1-PadRST)"))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R3-Pad2)"))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R4-Pad2)"))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(M4-Pad1)"))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(M3-Pad1)"))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(SHIELD1-Pad4)"))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(SHIELD1-Pad5)"))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad6)"))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-Pad7)"))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(SHIELD1-Pad8)"))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(SHIELD1-Pad9)"))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(SHIELD1-Pad10)"))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(SHIELD1-Pad11)"))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(SHIELD1-Pad12)"))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(SHIELD1-Pad13)"))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(SHIELD1-PadGND3)"))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(SHIELD1-Pad5V)"))
    (pad "" thru_hole circle (at 66.04 -7.62 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 66.04 -35.56 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 15.24 -50.8 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 13.97 -2.54 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 136.525 54.61 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R1 (at 10.16 -3.31 180) (layer F.SilkS))
    (fp_text value 1Kohm (at 10.16 3.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(M1-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D4.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 106.46 86.73 90)
    (descr "LED, diameter 4.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-43GD(Ver.12B).pdf")
    (tags "LED diameter 4.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.46 90) (layer F.SilkS))
    (fp_text value LED_Small (at 1.27 3.46 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D4.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Barrel_Jack_CUI_PJ-102AH (layer F.Cu) (tedit 59BC552D)
    (at 112.46 52.73 270)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J1 (at 5.75 8.45 360) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -5.5 6.2 360) (layer F.Fab))
    (fp_text user %R (at 0 6.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 0 6 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 3 thru_hole circle (at 4.7 3 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Barrel_Jack_CUI_PJ-102AH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Altech_AK300-2_P5.00mm (layer F.Cu) (tedit 59FF0306)
    (at 135.89 74.93)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference J2 (at -1.92 -6.99) (layer F.SilkS))
    (fp_text value "Motor Connection" (at 2.78 7.75) (layer F.Fab))
    (fp_text user %R (at 2.5 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 5 0) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dom:TO220_Horizontal_Throght_Hole (layer F.Cu) (tedit 5A8727A8)
    (at 114.935 64.77 180)
    (fp_text reference M1 (at 0 2.54 360) (layer F.SilkS))
    (fp_text value "P Channel Mosfet" (at -7.62 -8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 4 "Net-(M1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 4 smd rect (at 0 -11.43 180) (size 10.5 16) (layers F.Cu F.Paste F.Mask))
  )
  (module Dom:TO220_Horizontal_Throght_Hole (layer F.Cu) (tedit 5A8727A8)
    (at 162.56 64.77 180)
    (fp_text reference M2 (at 0 2.54 360) (layer F.SilkS))
    (fp_text value "P Channel Mosfet" (at -7.62 -8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 5 "Net-(M2-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 4 smd rect (at 0 -11.43 180) (size 10.5 16) (layers F.Cu F.Paste F.Mask))
  )
  (module Dom:TO220_Horizontal_Throght_Hole (layer F.Cu) (tedit 5A8727A8)
    (at 126.365 87.63)
    (fp_text reference M3 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value "N Channel Mosfet" (at -7.62 -8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 6 "Net-(M3-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 4 smd rect (at 0 -11.43) (size 10.5 16) (layers F.Cu F.Paste F.Mask))
  )
  (module Dom:TO220_Horizontal_Throght_Hole (layer F.Cu) (tedit 5A8727A8)
    (at 151.13 87.63)
    (fp_text reference M4 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value "N Channel Mosfet" (at -7.62 -8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 8 "Net-(M4-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 2 2) (drill 1.0922) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 4 smd rect (at 0 -11.43) (size 10.5 16) (layers F.Cu F.Paste F.Mask))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 127 64.77 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -3.56 360) (layer F.SilkS))
    (fp_text value PN2222A (at 2.54 2.79 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 360) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(M1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 150.495 65.405)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 2.54 -3.56 180) (layer F.SilkS))
    (fp_text value PN2222A (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(M2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 167.64 54.61 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R2 (at 10.16 -3.31 180) (layer F.SilkS))
    (fp_text value 1Kohm (at 10.16 3.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(M2-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 116.205 60.325)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R3 (at 10.16 -3.31) (layer F.SilkS))
    (fp_text value 100Kohm (at 10.16 3.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 20.32 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 147.32 60.325)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R4 (at 10.16 -3.31) (layer F.SilkS))
    (fp_text value 100Kohm (at 10.16 3.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 20.32 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 107.95 92.075)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R5 (at 10.16 -3.31) (layer F.SilkS))
    (fp_text value 1Mohm (at 10.16 3.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(M3-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 165.735 92.075 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R6 (at 10.16 -3.31 180) (layer F.SilkS))
    (fp_text value 1Mohm (at 10.16 3.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole oval (at 20.32 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(M4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 106.46 60.73 270)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R7 (at 10.16 -3.31 270) (layer F.SilkS))
    (fp_text value 1Kohm (at 10.16 3.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 104.14 101.346) (end 170.18 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.14 48.006) (end 104.14 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 48.006) (end 104.14 48.006) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 49.276) (end 168.91 48.006) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 60.706) (end 170.18 49.276) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 63.246) (end 170.18 60.706) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.72 96.266) (end 172.72 63.246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 98.806) (end 172.72 96.266) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 101.346) (end 170.18 98.806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.18 49.276) (xy 170.18 60.706) (xy 172.72 63.246) (xy 172.72 96.266) (xy 170.18 98.806)
        (xy 170.18 101.346) (xy 104.14 101.346) (xy 104.14 48.006) (xy 168.91 48.006)
      )
    )
  )
)
