(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 42)
    (tracks 206)
    (zones 0)
    (modules 11)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 +5V)
  (net 3 GND)
  (net 4 /IO17)
  (net 5 /IO16)
  (net 6 /IO15)
  (net 7 /IO14)
  (net 8 /IO13)
  (net 9 /IO12)
  (net 10 /IO11)
  (net 11 /IO10)
  (net 12 /IO9)
  (net 13 /IO8)
  (net 14 /IO7)
  (net 15 /IO6)
  (net 16 /IO5)
  (net 17 /IO4)
  (net 18 /IO3)
  (net 19 /IO2)
  (net 20 /IO1)
  (net 21 /IO0)
  (net 22 +3V3)
  (net 23 /IO33)
  (net 24 /IO38)
  (net 25 "Net-(J2-Pad2)")
  (net 26 "Net-(J2-Pad1)")
  (net 27 /USB-)
  (net 28 /USB+)
  (net 29 "Net-(J4-Pad4)")
  (net 30 "Net-(J5-Pad16)")
  (net 31 /IO37)
  (net 32 /IO35)
  (net 33 /IO36)
  (net 34 /IO18)
  (net 35 /RST)
  (net 36 /TMS_IO42)
  (net 37 /TCK_IO39)
  (net 38 /TDO_IO40)
  (net 39 /TDI_IO41)
  (net 40 /IO21)
  (net 41 /IO26)
  (net 42 /IO34)
  (net 43 /TX0_IO43)
  (net 44 /RX0_IO44)
  (net 45 /IO45)
  (net 46 /IO46)
  (net 47 "Net-(J6-Pad7)")
  (net 48 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /IO0)
    (add_net /IO1)
    (add_net /IO10)
    (add_net /IO11)
    (add_net /IO12)
    (add_net /IO13)
    (add_net /IO14)
    (add_net /IO15)
    (add_net /IO16)
    (add_net /IO17)
    (add_net /IO18)
    (add_net /IO2)
    (add_net /IO21)
    (add_net /IO26)
    (add_net /IO3)
    (add_net /IO33)
    (add_net /IO34)
    (add_net /IO35)
    (add_net /IO36)
    (add_net /IO37)
    (add_net /IO38)
    (add_net /IO4)
    (add_net /IO45)
    (add_net /IO46)
    (add_net /IO5)
    (add_net /IO6)
    (add_net /IO7)
    (add_net /IO8)
    (add_net /IO9)
    (add_net /RST)
    (add_net /RX0_IO44)
    (add_net /TCK_IO39)
    (add_net /TDI_IO41)
    (add_net /TDO_IO40)
    (add_net /TMS_IO42)
    (add_net /TX0_IO43)
    (add_net /USB+)
    (add_net /USB-)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J5-Pad16)")
    (add_net "Net-(J6-Pad7)")
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 118.364 104.14 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value R_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 110.49 104.14)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /IO34))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module chickadee:chickadee_3mm_fcu (layer F.Cu) (tedit 0)
    (at 114.3 114.046)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Chickadee 3mm" (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 116.84 78.74 90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J6 (at 0 -4.235 90) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Odd_Even (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 35 /RST))
    (pad 9 smd rect (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 8 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 39 /TDI_IO41))
    (pad 7 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J6-Pad7)"))
    (pad 6 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 38 /TDO_IO40))
    (pad 5 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 37 /TCK_IO39))
    (pad 3 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 36 /TMS_IO42))
    (pad 1 smd rect (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x21_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A421)
    (at 101.6 76.2 180)
    (descr "Through hole straight socket strip, 1x21, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x21 2.54mm single row")
    (fp_text reference J7 (at 0 2.77) (layer B.SilkS) hide)
    (fp_text value Conn_01x21_Female (at 0 -53.57) (layer B.Fab))
    (fp_text user %R (at 0 -25.4 270) (layer B.Fab))
    (pad 21 thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /IO18))
    (pad 20 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /USB-))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /USB+))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /IO21))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /IO26))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IO33))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /IO34))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /IO35))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /IO36))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /IO37))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /IO38))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /TCK_IO39))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /TDO_IO40))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /TDI_IO41))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TMS_IO42))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /TX0_IO43))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /RX0_IO44))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /IO45))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /IO46))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /RST))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x21_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x16_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41E)
    (at 124.46 121.92 180)
    (descr "Through hole straight socket strip, 1x16, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x16 2.54mm single row")
    (fp_text reference J5 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value FeatherBottom (at 0 40.87) (layer F.Fab))
    (fp_text user %R (at 0 19.05 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IO4))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IO5))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /IO37))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /IO35))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /IO36))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IO8))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IO9))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /IO10))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /IO11))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /IO18))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /IO17))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /IO15))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 +3V3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /RST))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:4UCONN_20329_V2_USB (layer F.Cu) (tedit 5C85D8AC)
    (at 114.3 123.984)
    (fp_text reference J4 (at -2.778 5.852) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at -2.778 6.41) (layer F.Fab))
    (fp_text user "PCB EDGE" (at 0 4) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.95 0) (size 0.7 0.7) (drill 0.7) (layers *.Mask B.Cu))
    (pad "" np_thru_hole circle (at 1.95 0) (size 0.7 0.7) (drill 0.7) (layers *.Mask B.Cu))
    (pad 6 thru_hole rect (at 3.6 1.9 180) (size 2.413 2.413) (drill oval 0.8 1.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 thru_hole rect (at -3.6 1.9 180) (size 2.413 2.413) (drill oval 0.9 1.3) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 thru_hole circle (at -3.3 -0.9 180) (size 1.143 1.143) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 thru_hole circle (at 3.3 -0.9) (size 1.143 1.143) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 1 smd rect (at -1.3 -0.775) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 1 "Net-(D1-Pad2)") (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -0.65 -0.775) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 27 /USB-) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 0 -0.775) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 28 /USB+) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 0.65 -0.775) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 29 "Net-(J4-Pad4)") (solder_mask_margin 0.0508))
    (pad 5 smd rect (at 1.3 -0.775) (size 0.4 1.35) (layers F.Cu F.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at -0.75 2 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 0.75 2 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0508))
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 107.315 78.105 180)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J3 (at 0 -3.98) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 3.98) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad MP smd roundrect (at 2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 4 smd roundrect (at 1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /IO45))
    (pad 3 smd roundrect (at 0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /IO0))
    (pad 2 smd roundrect (at -0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +3V3))
    (pad 1 smd roundrect (at -1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41D)
    (at 104.14 111.76 180)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value FeatherTop (at 0 30.71) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IO0))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /IO45))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /IO1))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /IO2))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /IO3))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /IO26))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IO33))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /IO38))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /IO34))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x21_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A421)
    (at 127 76.2 180)
    (descr "Through hole straight socket strip, 1x21, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x21 2.54mm single row")
    (fp_text reference J1 (at 0 2.77) (layer B.SilkS) hide)
    (fp_text value Conn_01x21_Female (at 0 -53.57) (layer B.Fab))
    (fp_text user %R (at 0 -25.4 270) (layer B.Fab))
    (pad 21 thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 20 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /IO17))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /IO16))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /IO15))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /IO14))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /IO13))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /IO12))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /IO11))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /IO10))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IO9))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IO8))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IO7))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IO6))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IO5))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IO4))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /IO3))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /IO2))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /IO1))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IO0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 +3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x21_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 113.03 119.38 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value D_Small (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5V (at 125.73 124.46) (layer F.SilkS))
  (gr_text GND (at 125.73 127) (layer F.SilkS))
  (gr_text 33 (at 102.87 114.3) (layer F.SilkS))
  (gr_text 26 (at 102.87 116.84) (layer F.SilkS))
  (gr_text 21 (at 102.87 119.38) (layer F.SilkS))
  (gr_text 18 (at 102.87 127) (layer F.SilkS))
  (gr_text 20 (at 102.87 121.92) (layer F.SilkS))
  (gr_text 19 (at 102.87 124.46) (layer F.SilkS))
  (gr_text ckd.tech/saola-feather/v1 (at 114.3 101.6 90) (layer F.SilkS))
  (gr_text RST (at 123.19 121.92) (layer F.SilkS))
  (gr_text 3V (at 123.19 119.38) (layer F.SilkS))
  (gr_text ARf (at 123.19 116.84) (layer F.SilkS))
  (gr_text GND (at 123.19 114.3) (layer F.SilkS))
  (gr_text A0 (at 123.19 111.76) (layer F.SilkS))
  (gr_text A1 (at 123.19 109.22) (layer F.SilkS))
  (gr_text A2 (at 123.19 106.68) (layer F.SilkS))
  (gr_text A3 (at 123.19 104.14) (layer F.SilkS))
  (gr_text A4 (at 123.19 101.6) (layer F.SilkS))
  (gr_text A5 (at 123.19 99.06) (layer F.SilkS))
  (gr_text SCK (at 123.19 96.52) (layer F.SilkS))
  (gr_text MOSI (at 123.19 93.98) (layer F.SilkS))
  (gr_text MISO (at 123.19 91.44) (layer F.SilkS))
  (gr_text RX (at 123.19 88.9) (layer F.SilkS))
  (gr_text TX (at 123.19 86.36) (layer F.SilkS))
  (gr_text SDA (at 105.41 83.82) (layer F.SilkS))
  (gr_text SCL (at 105.41 86.36) (layer F.SilkS))
  (gr_text D5 (at 105.41 88.9) (layer F.SilkS))
  (gr_text D6 (at 105.41 91.44) (layer F.SilkS))
  (gr_text D9 (at 105.41 93.98) (layer F.SilkS))
  (gr_text D10 (at 105.41 96.52) (layer F.SilkS))
  (gr_text D11 (at 105.41 99.06) (layer F.SilkS))
  (gr_text D12 (at 105.41 101.6) (layer F.SilkS))
  (gr_text D13 (at 105.41 104.14) (layer F.SilkS))
  (gr_text USB (at 105.41 106.68) (layer F.SilkS))
  (gr_line (start 100.965 74.93) (end 127.635 74.93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.33 127) (end 100.33 75.565) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 128.27) (end 101.6 128.27) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.27 75.565) (end 128.27 127) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127.635 75.565) (end 128.27 75.565) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 100.965 75.565) (end 100.965 74.93) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 127 127) (end 127 128.27) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.6 127) (end 100.33 127) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 128.139619) (xy 100.33 128.139619) (xy 100.33 74.799619) (xy 128.27 74.799619)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.051444 128.27) (xy 100.111444 128.27) (xy 100.111444 118.237) (xy 128.051444 118.11)
      )
    )
  )
)
