(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "User" 150.012 119.99)
	(title_block
		(title "Jaguar Audio/Video Breakout Board")
		(date "2021-05-15")
		(rev "1")
		(company "cubanismo")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(C1-Pad2)")
	(net 2 "Net-(C2-Pad1)")
	(net 3 "GND")
	(net 4 "Net-(J1-Pad4)")
	(net 5 "Net-(J1-Pad11)")
	(net 6 "Net-(J1-Pad12)")
	(net 7 "Net-(J1-Pad15)")
	(net 8 "GND1")
	(net 9 "Net-(J2-Pad3a)")
	(net 10 "Net-(J2-Pad9a)")
	(net 11 "Net-(J2-Pad10a)")
	(net 12 "Net-(J2-Pad12a)")
	(net 13 "Net-(J2-Pad9b)")
	(net 14 "Net-(J2-Pad12b)")
	(net 15 "Net-(J2-Pad6b)")
	(net 16 "Net-(U1-Pad1)")
	(net 17 "Net-(U1-Pad5)")
	(net 18 "Net-(U1-Pad7)")
	(net 19 "/CompSync")
	(net 20 "/VCC5")
	(net 21 "/Red")
	(net 22 "/Blue")
	(net 23 "/Green")
	(net 24 "/HSYNC")
	(net 25 "/VSYNC")
	(net 26 "/Luma")
	(net 27 "/VidComp")
	(net 28 "/AudLeft")
	(net 29 "/VCC9")
	(net 30 "/Chroma")
	(net 31 "/AudRight")
	(footprint "vga_adapter:SOT-89"
		(layer "F.Cu")
		(at 89.75 46.75 90)
		(property "Reference" "U2"
			(at 0 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "‎UA78L05ACPK‎"
			(at 0.25 -5.75 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "/VCC9")
		)
		(pad "2" smd custom
			(at 0 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "GND")
			(zone_connect 0)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1.1 -3.85) (xy 1.1 -1.65) (xy 0.5 -1.05) (xy 0.5 0.75) (xy -0.5 0.75) (xy -0.5 -1.05) (xy -1.1 -1.65)
						(xy -1.1 -3.85) (xy -0.2 -4.75) (xy 0.2 -4.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd rect
			(at 1.5 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/VCC5")
		)
		(model "${KIPRJMOD}/lib/3dmodels/PK0003A.step"
			(offset
				(xyz 0 1.8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "vga_adapter:Jack_MiniDIN-4Pos-Female"
		(layer "F.Cu")
		(at 98 40.75 -90)
		(property "Reference" "J5"
			(at 8.25 -4.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "S-Video"
			(at -0.25 7.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0.75 7.775 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0.75 7.775 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0.75 7.775 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.4 2 270)
			(size 1.7 1.7)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "2" thru_hole circle
			(at 3.4 2 270)
			(size 1.7 1.7)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "3" thru_hole circle
			(at -3.4 4.5 270)
			(size 1.7 1.7)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/Luma")
		)
		(pad "4" thru_hole circle
			(at 3.4 4.5 270)
			(size 1.7 1.7)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/Chroma")
		)
		(pad "5" thru_hole circle
			(at -6.75 -1)
			(size 3.3 3.3)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "5" thru_hole circle
			(at 0 -1.8 270)
			(size 3.3 3.3)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "5" thru_hole circle
			(at 6.75 -1 270)
			(size 3.3 3.3)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(model "${KIPRJMOD}/lib/3dmodels/KMDGX-4S-BS_rC6.step"
			(offset
				(xyz 0 6.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 180 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 88.575 37.5 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -1.675 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/VCC5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "vga_adapter:Jack_Audio_3.5mm"
		(layer "F.Cu")
		(at 69.25 23 -90)
		(property "Reference" "J3"
			(at 8 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "AudioJack4"
			(at -7.57 -0.32 180)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -4 0 270)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "" np_thru_hole circle
			(at 3 0 270)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "R1" thru_hole oval
			(at 5.5 2.85 270)
			(size 2.2 1.4)
			(drill oval 1.6 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/AudRight")
		)
		(pad "R2" thru_hole oval
			(at 5.5 -2.85 270)
			(size 2.2 1.4)
			(drill oval 1.6 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND1")
		)
		(pad "S" thru_hole oval
			(at 6.3 0 270)
			(size 1.4 2.2)
			(drill oval 0.8 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND1")
		)
		(pad "T" thru_hole oval
			(at -2.5 -3.3 270)
			(size 2.2 1.4)
			(drill oval 1.6 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/AudLeft")
		)
		(pad "T" thru_hole oval
			(at -2.5 3.3 270)
			(size 2.2 1.4)
			(drill oval 1.6 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/AudLeft")
		)
		(model "${KIPRJMOD}/lib/3dmodels/54-00174.step"
			(offset
				(xyz 11.9 3.05 -5.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "vga_adapter:TE_5530843-1-rev"
		(layer "F.Cu")
		(at 82.53 54.9257)
		(property "Reference" "J2"
			(at 19.97 0.3243 0)
			(layer "B.SilkS")
		)
		(property "Value" "JagVidConn"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "1b"
			(at -16.51 2.54 0)
			(layer "B.SilkS")
		)
		(fp_text user "1a"
			(at -16.51 -2.54 0)
			(layer "B.SilkS")
		)
		(fp_text user "12a"
			(at 16.51 -2.54 0)
			(layer "B.SilkS")
		)
		(fp_text user "12b"
			(at 16.51 2.54 0)
			(layer "B.SilkS")
		)
		(fp_text user "Jaguar Side"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(pad "1a" thru_hole rect
			(at -13.97 -2.54)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/AudLeft")
			(solder_mask_margin 0.102)
		)
		(pad "1b" thru_hole circle
			(at -13.97 2.54)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/AudRight")
			(solder_mask_margin 0.102)
		)
		(pad "2a" thru_hole circle
			(at -11.43 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND1")
			(solder_mask_margin 0.102)
		)
		(pad "2b" thru_hole circle
			(at -11.43 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "GND1")
			(solder_mask_margin 0.102)
		)
		(pad "3a" thru_hole circle
			(at -8.89 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pad3a)")
			(solder_mask_margin 0.102)
		)
		(pad "3b" thru_hole circle
			(at -8.89 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(solder_mask_margin 0.102)
		)
		(pad "4a" thru_hole circle
			(at -6.35 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(solder_mask_margin 0.102)
		)
		(pad "4b" thru_hole circle
			(at -6.35 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/Red")
			(solder_mask_margin 0.102)
		)
		(pad "5a" thru_hole circle
			(at -3.81 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/Blue")
			(solder_mask_margin 0.102)
		)
		(pad "5b" thru_hole circle
			(at -3.81 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/CompSync")
			(solder_mask_margin 0.102)
		)
		(pad "6a" thru_hole circle
			(at -1.27 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/HSYNC")
			(solder_mask_margin 0.102)
		)
		(pad "6b" thru_hole circle
			(at -1.27 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J2-Pad6b)")
			(solder_mask_margin 0.102)
		)
		(pad "7a" thru_hole circle
			(at 1.27 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/Green")
			(solder_mask_margin 0.102)
		)
		(pad "7b" thru_hole circle
			(at 1.27 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(solder_mask_margin 0.102)
		)
		(pad "8a" thru_hole circle
			(at 3.81 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/Chroma")
			(solder_mask_margin 0.102)
		)
		(pad "8b" thru_hole circle
			(at 3.81 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/Luma")
			(solder_mask_margin 0.102)
		)
		(pad "9a" thru_hole circle
			(at 6.35 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pad9a)")
			(solder_mask_margin 0.102)
		)
		(pad "9b" thru_hole circle
			(at 6.35 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J2-Pad9b)")
			(solder_mask_margin 0.102)
		)
		(pad "10a" thru_hole circle
			(at 8.89 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pad10a)")
			(solder_mask_margin 0.102)
		)
		(pad "10b" thru_hole circle
			(at 8.89 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(solder_mask_margin 0.102)
		)
		(pad "11a" thru_hole circle
			(at 11.43 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/VCC9")
			(solder_mask_margin 0.102)
		)
		(pad "11b" thru_hole circle
			(at 11.43 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/VidComp")
			(solder_mask_margin 0.102)
		)
		(pad "12a" thru_hole circle
			(at 13.97 -2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J2-Pad12a)")
			(solder_mask_margin 0.102)
		)
		(pad "12b" thru_hole circle
			(at 13.97 2.4257)
			(size 1.6383 1.6383)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J2-Pad12b)")
			(solder_mask_margin 0.102)
		)
		(model "${KIPRJMOD}/lib/3dmodels/5530843-1.step"
			(offset
				(xyz 0 0 -17.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 0)
			)
		)
	)
	(footprint "vga_adapter:DSUB-15HD"
		(layer "F.Cu")
		(at 104 17 180)
		(property "Reference" "J1"
			(at 16.25 -17 0)
			(layer "F.SilkS")
		)
		(property "Value" "VGAConn"
			(at 16 1.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "15"
			(at 8.25 -9 0)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at 8.25 -11.5 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 22.75 -14 0)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at 8.25 -14 0)
			(layer "F.SilkS")
		)
		(fp_text user "11"
			(at 22.75 -9 0)
			(layer "F.SilkS")
		)
		(fp_text user "6"
			(at 22.75 -11.5 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole rect
			(at 19.71 -13.97 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/Red")
		)
		(pad "2" thru_hole circle
			(at 17.43 -13.97 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/Green")
		)
		(pad "3" thru_hole circle
			(at 15.15 -13.97 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/Blue")
		)
		(pad "4" thru_hole circle
			(at 12.87 -13.97 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pad4)")
		)
		(pad "5" thru_hole circle
			(at 10.59 -13.97 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "6" thru_hole circle
			(at 20.85 -11.43 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "7" thru_hole circle
			(at 18.57 -11.43 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "8" thru_hole circle
			(at 16.29 -11.43 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "9" thru_hole circle
			(at 14.01 -11.43 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/VCC5")
		)
		(pad "10" thru_hole circle
			(at 11.73 -11.43 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "11" thru_hole circle
			(at 19.71 -8.89 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pad11)")
		)
		(pad "12" thru_hole circle
			(at 17.43 -8.89 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pad12)")
		)
		(pad "13" thru_hole circle
			(at 15.15 -8.89 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/HSYNC")
		)
		(pad "14" thru_hole circle
			(at 12.87 -8.89 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/VSYNC")
		)
		(pad "15" thru_hole circle
			(at 10.59 -8.89 180)
			(size 1.5 1.5)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad15)")
		)
		(pad "16" thru_hole circle
			(at 2.91 -11.43 180)
			(size 4.2 4.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "17" thru_hole circle
			(at 27.9 -11.43 180)
			(size 4.2 4.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(model "${KIPRJMOD}/lib/3dmodels/ICD15S13E6GX00LF.step"
			(offset
				(xyz 15.5 0.4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(at 88.575 40.05)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 1.675 -0.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "680k"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C2-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 88.575 41.2)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.675 0.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C2-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 83.975 39.4)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM1881"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U1-Pad1)")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(C1-Pad2)")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/VSYNC")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "GND")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(U1-Pad5)")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C2-Pad1)")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U1-Pad7)")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/VCC5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 79.425 38.75)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/CompSync")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(C1-Pad2)")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "vga_adapter:Jack_RCA"
		(layer "F.Cu")
		(at 64.8 37.25 90)
		(property "Reference" "J4"
			(at 0 10.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "Composite Video"
			(at 0 11.2 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "shunt"
			(at -2 6 0)
			(layer "F.SilkS")
		)
		(fp_text user "tip"
			(at 2 7 0)
			(layer "F.SilkS")
		)
		(fp_text user "sleeve"
			(at 0 5.5 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole oval
			(at 3.75 7.7 90)
			(size 2 3.6)
			(drill oval 1 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/VidComp")
		)
		(pad "2" thru_hole oval
			(at 0 4 90)
			(size 3.6 2.3)
			(drill oval 2.6 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "3" thru_hole oval
			(at -3.75 7.7 90)
			(size 2 3.6)
			(drill oval 1 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(model "${KIPRJMOD}/lib/3dmodels/PJRAN1X1U04X.step"
			(offset
				(xyz 0 -3.8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 180 0)
			)
		)
	)
	(gr_line
		(start 64.5 60)
		(end 64.5 17)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.5 17)
		(end 104 17)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104 60)
		(end 64.5 60)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104 17)
		(end 104 60)
		(layer "Edge.Cuts")
	)
	(gr_text_box "BOM:\nC1, C2, C3: Capacitor 0603 0.1uF\nJ1: Amphenol ICD15S13E6GX00LF\nJ2: TE Connectivity 5530843-1\nJ3: Tensility 54-00174\nJ4: Switchcraft PJRAN1X1U04X\nJ5: Kycon KMDGX-4S-BS\nR1: Resistor 0603 680k\nU1: Texas Instruments LM1881MX/NOPB\nU2: Texas Instruments UA78L05ACPK"
		(start 63.875 33)
		(end 96.625 51.5)
		(layer "B.SilkS")
		(border no)
	)
	(gr_text_box "\nJaguar AV Breakout v2.0"
		(start 78 18)
		(end 99.5 23.75)
		(layer "B.SilkS")
		(border yes)
	)
	(zone
		(net 20)
		(net_name "/VCC5")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 73.5 29) (xy 71 31.5) (xy 68.5 31.5) (xy 67.5 32.5) (xy 67.5 46) (xy 72.5 51) (xy 72.5 59.5)
				(xy 103.5 59.5) (xy 103.5 17.5) (xy 73.5 17.5)
			)
		)
	)
	(zone
		(net 8)
		(net_name "GND1")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 72.75 29) (xy 70.75 31) (xy 65.75 31) (xy 65.75 17.5) (xy 72.75 17.5)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 73.5 29) (xy 71 31.5) (xy 68.5 31.5) (xy 67.5 32.5) (xy 67.5 46) (xy 72.5 51) (xy 72.5 59.5)
				(xy 103.5 59.5) (xy 103.5 17.5) (xy 73.5 17.5)
			)
		)
	)
)