(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 84)
    (no_connects 0)
    (area 43.449999 43.449999 131.550001 106.050001)
    (thickness 1.6)
    (drawings 8)
    (tracks 299)
    (zones 0)
    (modules 42)
    (nets 40)
  )
  (page A4)
  (title_block
    (title "Brownsource Clone")
    (date 20.03.2005)
    (rev V5)
    (company Lovetone)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.24)
    (user_trace_width 0.254)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.2)
    (via_drill 0.1)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (uvia_size 0.03)
    (uvia_drill 0.02)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.3 1.3)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 43.5 43.5)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C5-Pad2)")
  (net 10 "Net-(C6-Pad1)")
  (net 11 "Net-(C10-Pad2)")
  (net 12 "Net-(C7-Pad1)")
  (net 13 "Net-(C8-Pad1)")
  (net 14 "Net-(C9-Pad1)")
  (net 15 "Net-(C9-Pad2)")
  (net 16 "Net-(C10-Pad1)")
  (net 17 "Net-(C11-Pad1)")
  (net 18 "Net-(C12-Pad1)")
  (net 19 "Net-(C12-Pad2)")
  (net 20 "Net-(C13-Pad1)")
  (net 21 "Net-(CON1-Pad1)")
  (net 22 "Net-(D2-Pad2)")
  (net 23 "Net-(J1-Pad6)")
  (net 24 "Net-(J1-Pad2)")
  (net 25 "Net-(J1-Pad3)")
  (net 26 "Net-(J2-Pad6)")
  (net 27 "Net-(J2-Pad2)")
  (net 28 "Net-(J2-Pad3)")
  (net 29 "Net-(R12-Pad2)")
  (net 30 "Net-(R14-Pad1)")
  (net 31 "Net-(SW1-Pad8)")
  (net 32 "Net-(SW1-Pad10)")
  (net 33 "Net-(SW1-Pad12)")
  (net 34 "Net-(SW1-Pad15)")
  (net 35 "Net-(SW1-Pad2)")
  (net 36 "Net-(SW1-Pad5)")
  (net 37 "Net-(D4-Pad2)")
  (net 38 "Net-(R15-Pad2)")
  (net 39 "Net-(SW2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.2)
    (via_dia 0.2)
    (via_drill 0.1)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(SW1-Pad10)")
    (add_net "Net-(SW1-Pad12)")
    (add_net "Net-(SW1-Pad15)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW1-Pad5)")
    (add_net "Net-(SW1-Pad8)")
    (add_net "Net-(SW2-Pad7)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net VCC)
  )
  (module Potentiometers:Potentiometer_WirePads (layer F.Cu) (tedit 57E8557E)
    (at 69.98 60.35 270)
    (descr "Potentiometer, Wire Pads only, RevA, 30 July 2010,")
    (tags "Potentiometer, Wire Pads only, RevA, 30 July 2010,")
    (fp_text reference VR1 (at -0.45 2.576 270) (layer F.SilkS))
    (fp_text value 25k (at -0.45 7.656 450) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 5.00126 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 3 thru_hole circle (at 0 10.00252 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 57E864A1)
    (at 98.23 58.6)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 4.318 -1.778) (layer F.SilkS))
    (fp_text value 47uF (at 4.75 2.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L27_W9_H17_P23 (layer F.Cu) (tedit 57E86421)
    (at 76.294 73.616 270)
    (descr "Film Capacitor Length 27mm x Width 9mm x Heigth 17mm, Pitch 23mm")
    (tags "Kemet R.46 Capacitor")
    (fp_text reference C2 (at 11.484 -5.436 270) (layer F.SilkS))
    (fp_text value 10uF (at 11.484 0.064 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 23 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L27_W9_H17_P23.wrl
      (at (xyz 0.452756 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W3.5_P5 (layer F.Cu) (tedit 57E8590F)
    (at 48.73 58.1 270)
    (descr "Film Capacitor Length 7mm x Width 3.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.54 2.54 270) (layer F.SilkS))
    (fp_text value 47nF (at 2.794 -1.016 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C3-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W6_P5 (layer F.Cu) (tedit 57E863D4)
    (at 49.116 49.74 270)
    (descr "Film Capacitor Length 7mm x Width 6mm")
    (tags Capacitor)
    (fp_text reference C4 (at -2.14 -2.364 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 2.36 -1.614 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57E82B77)
    (at 76.08 55.25 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C5 (at -0.254 2.032 180) (layer F.SilkS))
    (fp_text value 33nF (at 2.54 1.778 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C5-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W6_P5 (layer F.Cu) (tedit 57E866BC)
    (at 85.5 101.75 90)
    (descr "Film Capacitor Length 7mm x Width 6mm")
    (tags Capacitor)
    (fp_text reference C6 (at 2.5 -3.75 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 2.794 1.524 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57E866AF)
    (at 112.75 100 90)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 2 2 90) (layer F.SilkS))
    (fp_text value 33nF (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57E8667A)
    (at 104.75 95 270)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 3 -2 270) (layer F.SilkS))
    (fp_text value 33nF (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57E82CA4)
    (at 87.73 69.6 270)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 2.54 2.032 270) (layer F.SilkS))
    (fp_text value 22nF (at 2.54 -0.254 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C9-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57E8668C)
    (at 96.75 98.25 270)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 2.5 -2 270) (layer F.SilkS))
    (fp_text value 33nF (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57E8667E)
    (at 100.75 97 270)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C11 (at 2.5 -2 270) (layer F.SilkS))
    (fp_text value 22nF (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W6_P5 (layer F.Cu) (tedit 57E86277)
    (at 122.98 65.35 90)
    (descr "Film Capacitor Length 7mm x Width 6mm")
    (tags Capacitor)
    (fp_text reference C12 (at 0.25 3.75 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 2.5 1.75 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C12-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 57E866AB)
    (at 108.75 95 270)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C13 (at 2.5 -2 270) (layer F.SilkS))
    (fp_text value 33nF (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Connect:BARREL_JACK (layer F.Cu) (tedit 57E855AE)
    (at 104.25 47.5 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at -1.412 5.33 450) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 1.37 -3.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 6.20014 0 270) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole rect (at 0.20066 0 270) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699 270) (size 3.50012 3.50012) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 57E8287B)
    (at 95.48 47.6 180)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D1 (at 5.588 -2.032 180) (layer F.SilkS))
    (fp_text value 1N4001 (at 4.572 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(CON1-Pad1)"))
    (pad 1 thru_hole rect (at 0 -0.00254) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 57E82B67)
    (at 79.08 48.25 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D2 (at 4.826 1.778 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.572 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 57E82B9A)
    (at 68.88 51.05)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D3 (at 5.08 -1.524) (layer F.SilkS))
    (fp_text value 1N4148 (at 5.588 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D2-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:NMJ6HCD2 (layer F.Cu) (tedit 57E8B01E)
    (at 50.25 90.25 90)
    (descr "NMJ6HCD2, TRS 1/4\" jack connector, stereo, switched")
    (tags "NMJ6HCD2 TRS stereo jack connector")
    (fp_text reference J1 (at 2.75 17.5 90) (layer F.SilkS))
    (fp_text value JACK_TRS_6PINS (at 8 -3 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 16.23 6.35 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 16.23 12.7 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 16.23 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 6.35 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 12.7 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connect.3dshapes/NMJ6HCD2.wrl
      (at (xyz 0.32 0.165 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connect:NMJ6HCD2 (layer F.Cu) (tedit 57E8B019)
    (at 124.75 74.25 270)
    (descr "NMJ6HCD2, TRS 1/4\" jack connector, stereo, switched")
    (tags "NMJ6HCD2 TRS stereo jack connector")
    (fp_text reference J2 (at 2.25 17.75 270) (layer F.SilkS))
    (fp_text value JACK_TRS_6PINS (at 7.75 -3 270) (layer F.Fab))
    (pad 6 thru_hole circle (at 16.23 6.35 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad6)"))
    (pad 5 thru_hole circle (at 16.23 12.7 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad2)"))
    (pad 4 thru_hole circle (at 16.23 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 6.35 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 0 12.7 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connect.3dshapes/NMJ6HCD2.wrl
      (at (xyz 0.32 0.165 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz -90 0 180))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Rugged (layer F.Cu) (tedit 57E8B761)
    (at 54.196 58.122 270)
    (descr "TO-92 rugged, leads molded, wide, drill 1mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 5.128 -2.304 270) (layer F.SilkS))
    (fp_text value BC549 (at 2.54 1.778 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 -2.54) (size 2.99974 1.99898) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 thru_hole oval (at 0 0) (size 1.99898 2.99974) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.99898 2.99974) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C3-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Rugged.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E827EB)
    (at 60.546 70.06)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5 -2) (layer F.SilkS))
    (fp_text value 1M2 (at 5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E858F0)
    (at 57.752 70.06 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 1.524 2.032 180) (layer F.SilkS))
    (fp_text value 1M2 (at 5.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E858F3)
    (at 57.752 66.758 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 1.524 -4.572 180) (layer F.SilkS))
    (fp_text value 3k9 (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E829CA)
    (at 53.942 52.534)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 5.08 -2.032) (layer F.SilkS))
    (fp_text value 22k (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E829CD)
    (at 64 47.5 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 5.08 2.032 180) (layer F.SilkS))
    (fp_text value 22k (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E82A35)
    (at 67.404 56.852 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 5.334 2.032 180) (layer F.SilkS))
    (fp_text value 220E (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E85742)
    (at 70.73 65.85 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 5.334 2.032 180) (layer F.SilkS))
    (fp_text value 1k (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(D2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E861E9)
    (at 83.23 80.35 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at 5 2 90) (layer F.SilkS))
    (fp_text value 1k (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E85762)
    (at 117 98.25)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at 5.08 2.032) (layer F.SilkS))
    (fp_text value 3k9 (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(C10-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E85769)
    (at 81.98 56.6 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at 5.334 2.286 90) (layer F.SilkS))
    (fp_text value 3k9 (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(C8-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E82D00)
    (at 91.23 62.85 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R11 (at 5.334 -2.032 270) (layer F.SilkS))
    (fp_text value 330k (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 "Net-(C9-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E82D40)
    (at 95.48 63.1 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R12 (at 5.08 -2.032 270) (layer F.SilkS))
    (fp_text value 3k9 (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R12-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E86249)
    (at 99.73 63.1 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R13 (at 5 -2 270) (layer F.SilkS))
    (fp_text value 22k (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R12-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E8B757)
    (at 111.98 53.35)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R14 (at 5.02 2.15) (layer F.SilkS))
    (fp_text value 220E (at 5.334 -2.032) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(R14-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(C12-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 57E82B7F)
    (at 73.5 59.9)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0.762 10.668) (layer F.SilkS))
    (fp_text value NE5532 (at 3.81 3.556 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C4-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C9-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(R12-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C12-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_WirePads (layer F.Cu) (tedit 57E82968)
    (at 84.48 60.35 90)
    (descr "Potentiometer, Wire Pads only, RevA, 30 July 2010,")
    (tags "Potentiometer, Wire Pads only, RevA, 30 July 2010,")
    (fp_text reference VR2 (at 3.752 -0.82 90) (layer F.SilkS))
    (fp_text value 100k (at 5.784 5.022 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 5.00126 90) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(SW1-Pad8)"))
    (pad 3 thru_hole circle (at 0 10.00252 90) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C8-Pad1)"))
  )
  (module Potentiometers:Potentiometer_WirePads (layer F.Cu) (tedit 57E8296D)
    (at 116.98 60.35 270)
    (descr "Potentiometer, Wire Pads only, RevA, 30 July 2010,")
    (tags "Potentiometer, Wire Pads only, RevA, 30 July 2010,")
    (fp_text reference VR3 (at 3.614 -0.97 270) (layer F.SilkS))
    (fp_text value 10k (at 5.392 5.126 360) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 5.00126 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(SW2-Pad7)"))
    (pad 3 thru_hole circle (at 0 10.00252 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R14-Pad1)"))
  )
  (module Brownsource:Rotarysw0304 (layer F.Cu) (tedit 57E8B00F)
    (at 93.98 85.6)
    (fp_text reference SW1 (at 9.77 6.4) (layer F.SilkS))
    (fp_text value Rotary_3P4T (at -0.23 -6.6) (layer F.Fab))
    (pad 1 thru_hole circle (at -4.76314 -2.75 60) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(C8-Pad1)"))
    (pad 6 thru_hole circle (at 0 5.5 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(C9-Pad2)"))
    (pad 11 thru_hole circle (at 4.76314 -2.75 300) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(R14-Pad1)"))
    (pad 8 thru_hole circle (at 2.588 9.659) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(SW1-Pad8)"))
    (pad 9 thru_hole circle (at 7.070774 7.070939 30) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(SW1-Pad8)"))
    (pad 10 thru_hole circle (at 9.658939 2.588226 60) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(SW1-Pad10)"))
    (pad 12 thru_hole circle (at 9.659 -2.588 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(SW1-Pad12)"))
    (pad 13 thru_hole circle (at 7.070939 -7.070774 120) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(C13-Pad1)"))
    (pad 14 thru_hole circle (at 2.588226 -9.658939 150) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(C13-Pad1)"))
    (pad 15 thru_hole circle (at -2.588 -9.659 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(SW1-Pad15)"))
    (pad 2 thru_hole circle (at -7.070774 -7.070939 210) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(SW1-Pad2)"))
    (pad 3 thru_hole circle (at -9.658939 -2.588226 240) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(C10-Pad1)"))
    (pad 4 thru_hole circle (at -9.659 2.588 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(C11-Pad1)"))
    (pad 5 thru_hole circle (at -7.070939 7.070774 300) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(SW1-Pad5)"))
    (pad 7 thru_hole circle (at -2.588226 9.658939 330) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(C10-Pad2)"))
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 57E8644E)
    (at 55.23 95.35 270)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D4 (at 4 -2.75 270) (layer F.SilkS))
    (fp_text value LED (at 5.25 -1.5 270) (layer F.Fab))
    (fp_text user K (at -2.25 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 57E863B4)
    (at 47.75 93.25 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R15 (at 5 -2 270) (layer F.SilkS))
    (fp_text value 2k2 (at 5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 37 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 "Net-(R15-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Brownsourcev2:footsw_3PDT (layer B.Cu) (tedit 57E8B749)
    (at 65 98.5)
    (fp_text reference SW2 (at -2.25 1.5) (layer F.SilkS))
    (fp_text value footsw3P2T (at 0.5 3.25) (layer B.Fab))
    (pad 5 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(R15-Pad2)"))
    (pad 4 thru_hole circle (at 0 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 6 thru_hole circle (at 0 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad2)"))
    (pad 7 thru_hole circle (at 5 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(SW2-Pad7)"))
    (pad 9 thru_hole circle (at 5 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -5 -5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -5 5) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at -5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
  )
  (gr_text 1 (at 117.25 58) (layer F.SilkS))
  (gr_text 1 (at 95 58) (layer F.SilkS))
  (gr_text 1 (at 70 58) (layer F.SilkS))
  (gr_text "Lovetone Brownsource\nV5 (Rev1)\n9/25/16" (at 118.3 47.3) (layer F.SilkS))
  (gr_line (start 43.5 106) (end 43.5 43.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.5 106) (end 43.5 106) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.5 43.5) (end 131.5 106) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 43.5 43.5) (end 131.5 43.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131 105.5) (xy 44 105.5) (xy 44 44) (xy 131 44)
      )
    )
  )
)
