(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.567)
  )
  (paper "A4")
  (title_block
    (title "SZG-TEMPLATE-TXR")
    (rev "A")
    (company "Opal Kelly Incorporated")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.0254))
      (layer "F.Cu" (type "copper") (thickness 0.0432))
      (layer "dielectric 1" (type "core") (color "FR4 natural") (thickness 0.2021) (material "FR408-HR") (epsilon_r 3.69) (loss_tangent 0.0091))
      (layer "In1.Cu" (type "copper") (thickness 0.0175))
      (layer "dielectric 2" (type "prepreg") (color "FR4 natural") (thickness 0.9906) (material "FR408-HR") (epsilon_r 3.69) (loss_tangent 0.0091))
      (layer "In2.Cu" (type "copper") (thickness 0.0175))
      (layer "dielectric 3" (type "core") (color "FR4 natural") (thickness 0.2021) (material "FR408-HR") (epsilon_r 3.69) (loss_tangent 0.0091))
      (layer "B.Cu" (type "copper") (thickness 0.0432))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.0254))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints yes)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 143.51932 131.463854)
    (grid_origin 143.51932 131.463854)
    (pcbplotparams
      (layerselection 0x00011fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GerberOutput/")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "+3V3")
  (net 4 "/SDI/SDI_X")
  (net 5 "/SDI/SDO_X")
  (net 6 "/SDI/VCC_I")
  (net 7 "/SDI/VCO_I")
  (net 8 "/SDI/SDI_P")
  (net 9 "/R_GA")
  (net 10 "/RSVD_38")
  (net 11 "/RSVD_37")
  (net 12 "/C2P_CLKN")
  (net 13 "/P2C_CLKN")
  (net 14 "/C2P_CLKP")
  (net 15 "/P2C_CLKP")
  (net 16 "/MCU_SDA_MOSI")
  (net 17 "/MCU_SCL_USCK")
  (net 18 "Net-(C12-Pad1)")
  (net 19 "/SDI/SDI_N")
  (net 20 "/SDI/RxCP")
  (net 21 "/SDI/RxCN")
  (net 22 "Net-(U2-LF-)")
  (net 23 "Net-(U2-LF+)")
  (net 24 "Net-(U3-LF-)")
  (net 25 "Net-(U3-LF+)")
  (net 26 "/VIO")
  (net 27 "/SDI/TxCP")
  (net 28 "/SDI/TxCN")
  (net 29 "/SDI/SDO_P")
  (net 30 "/SDI/SDO_N")
  (net 31 "Net-(C20-Pad2)")
  (net 32 "/SDI/VCC_O")
  (net 33 "/SDI/VCCO_O")
  (net 34 "/RX0P")
  (net 35 "/RX0N")
  (net 36 "/REFCLKN")
  (net 37 "/TX2P")
  (net 38 "/S6")
  (net 39 "/TX1P")
  (net 40 "/TX3P")
  (net 41 "/REFCLKP")
  (net 42 "/TX0P")
  (net 43 "/S8")
  (net 44 "/S9")
  (net 45 "/RX1P")
  (net 46 "/RX1N")
  (net 47 "/TX2N")
  (net 48 "/RX2P")
  (net 49 "/SDI/VCO_O")
  (net 50 "/RX2N")
  (net 51 "/TX3N")
  (net 52 "/S7")
  (net 53 "/SDI/TERMO")
  (net 54 "/+2.5V")
  (net 55 "/SDIN")
  (net 56 "/SCLK")
  (net 57 "/TX1N")
  (net 58 "/RX3N")
  (net 59 "/TX0N")
  (net 60 "/RX3P")
  (net 61 "/CLK_OE")
  (net 62 "/SDOUT")
  (net 63 "/CLK_FS")
  (net 64 "/CS_n")
  (net 65 "/AVR/MCU_MISO")
  (net 66 "/AVR/MCU_RESET_B")
  (net 67 "/CLKN")
  (net 68 "/CLKP")
  (net 69 "Net-(U1-PA1)")
  (net 70 "Net-(U1-PA2)")
  (net 71 "Net-(U1-PA3)")
  (net 72 "Net-(U1-PA7)")
  (net 73 "Net-(U1-XTAL1{slash}PB0)")
  (net 74 "Net-(U1-XTAL2{slash}PB1)")
  (net 75 "Net-(U1-PB2)")
  (net 76 "/SDI/GPIO1")
  (net 77 "/SDI/GPIO0")
  (net 78 "/SDI/GPIO2")
  (net 79 "/SDI/GPIO3")
  (net 80 "/SDI/GPIO5")
  (net 81 "/SDI/GPIO4")
  (net 82 "/SDI/GPIO6")
  (net 83 "/SDI/GPIO7")
  (net 84 "unconnected-(U1-NC-Pad6)")
  (net 85 "unconnected-(U1-NC-Pad7)")
  (net 86 "unconnected-(U1-NC-Pad10)")
  (net 87 "unconnected-(U1-NC-Pad17)")
  (net 88 "unconnected-(U1-NC-Pad18)")
  (net 89 "unconnected-(U1-NC-Pad19)")
  (net 90 "unconnected-(U2-RSVD_1-Pad5)")
  (net 91 "unconnected-(U2-RSVD_2-Pad6)")
  (net 92 "unconnected-(U2-RSVD_3-Pad7)")
  (net 93 "unconnected-(U2-RSVD_4-Pad9)")
  (net 94 "/SDI/SDIX")
  (net 95 "unconnected-(U2-~{DDO1}{slash}~{RCO}-Pad22)")
  (net 96 "unconnected-(U2-DDO1{slash}RCO-Pad23)")
  (net 97 "unconnected-(U2-VCO_FILT10-Pad30)")
  (net 98 "unconnected-(U2-RSVD_5-Pad32)")
  (net 99 "unconnected-(U3-RSVD_1-Pad2)")
  (net 100 "unconnected-(U3-RSVD_2-Pad3)")
  (net 101 "unconnected-(U3-RSVD_3-Pad9)")
  (net 102 "unconnected-(U3-~{SDO1}{slash}~{RCO}-Pad22)")
  (net 103 "unconnected-(U3-SDO1{slash}RCO-Pad23)")
  (net 104 "unconnected-(U3-RSVD_4-Pad30)")
  (net 105 "unconnected-(U5-NC-Pad4)")
  (net 106 "/SDI/VCCO_I")
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 160.32412 100.270334 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 1.8148 0.0068) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at -0.0602 -1.0182) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 163.49912 97.196934 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0.0334 1.0102 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/AVR/MCU_RESET_B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 155.87912 98.238334 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -1.7252 -0.0698 90) (layer "F.SilkS"))
    (fp_text value "10K" (at -2.2252 -0.2198 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/R_GA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:QFN-24-4x4mm" (layer "F.Cu")
    (at 160.07012 96.765134 -90)
    (property "Manufacturer" "Microchip")
    (property "Manufacturer_PN" "ATTINY44A-MU")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (attr smd)
    (fp_text reference "U1" (at -3.3016 -2.7392 90) (layer "F.SilkS"))
    (fp_text value "ATtiny44A-MU" (at -3.2016 -0.0392) (layer "F.Fab"))
    (pad "1" smd oval (at -1 2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/MCU_SCL_USCK") (pinfunction "PA4") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "2" smd oval (at -0.5 2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(U1-PA3)") (pinfunction "PA3") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "3" smd oval (at 0 2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(U1-PA2)") (pinfunction "PA2") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "4" smd oval (at 0.5 2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(U1-PA1)") (pinfunction "PA1") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "5" smd oval (at 1 2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/R_GA") (pinfunction "AREF/PA0") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "6" smd oval (at 2 1) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "unconnected-(U1-NC-Pad6)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.0508))
    (pad "7" smd oval (at 2 0.5) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "unconnected-(U1-NC-Pad7)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.0508))
    (pad "8" smd oval (at 2 0) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0508))
    (pad "9" smd oval (at 2 -0.5) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.0508))
    (pad "10" smd oval (at 2 -1) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "unconnected-(U1-NC-Pad10)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.0508))
    (pad "11" smd oval (at 1 -2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(U1-XTAL1{slash}PB0)") (pinfunction "XTAL1/PB0") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "12" smd oval (at 0.5 -2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(U1-XTAL2{slash}PB1)") (pinfunction "XTAL2/PB1") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "13" smd oval (at 0 -2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/AVR/MCU_RESET_B") (pinfunction "~{RESET}/PB3") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "14" smd oval (at -0.5 -2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(U1-PB2)") (pinfunction "PB2") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "15" smd oval (at -1 -2 90) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(U1-PA7)") (pinfunction "PA7") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "16" smd oval (at -2 -1) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/MCU_SDA_MOSI") (pinfunction "PA6") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "17" smd oval (at -2 -0.5) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "unconnected-(U1-NC-Pad17)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.0508))
    (pad "18" smd oval (at -2 0) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "unconnected-(U1-NC-Pad18)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.0508))
    (pad "19" smd oval (at -2 0.5) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "unconnected-(U1-NC-Pad19)") (pinfunction "NC") (pintype "no_connect") (solder_mask_margin 0.0508))
    (pad "20" smd oval (at -2 1) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/AVR/MCU_MISO") (pinfunction "PA5") (pintype "bidirectional") (solder_mask_margin 0.0508))
    (pad "21" smd rect (at 0 0) (size 2.7 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 156.84432 98.238334 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 1.7252 -0.065 90) (layer "F.SilkS"))
    (fp_text value "0.1uF DNP" (at 4.6752 -0.315 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/R_GA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "F.Cu")
    (at 203.51932 129.463854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID1" (at 0 -2 90) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "F.Cu")
    (at 203.51932 83.463854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID2" (at 0 -2 90) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "F.Cu")
    (at 146.08432 128.936854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID3" (at 0 -2 90) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "F.Cu")
    (at 155.29732 83.825854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID4" (at 0 -2 90) (layer "F.SilkS") hide)
    (fp_text value "Fiducial" (at 0 2 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "SYZYGY:TestPoint-20mil" (layer "F.Cu")
    (at 162.30532 99.686134 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr smd)
    (fp_text reference "TP5" (at 0 1.05 90) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -0.9 90) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Mask")
      (net 73 "Net-(U1-XTAL1{slash}PB0)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "SYZYGY:TestPoint-20mil" (layer "F.Cu")
    (at 163.16892 98.797134 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr smd)
    (fp_text reference "TP6" (at 0 1.05 90) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -0.9 90) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Mask")
      (net 74 "Net-(U1-XTAL2{slash}PB1)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "SYZYGY:TestPoint-20mil" (layer "F.Cu")
    (at 163.32132 95.723734 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr smd)
    (fp_text reference "TP7" (at 0 1.05 90) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -0.9 90) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Mask")
      (net 75 "Net-(U1-PB2)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 192.01932 88.463854 -90)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP8" (at -1 0 -90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 76 "/SDI/GPIO1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 190.01932 88.463854 -90)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP9" (at -1 0 -90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 77 "/SDI/GPIO0") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 196.01932 88.463854 -90)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP11" (at -1 0 -90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 79 "/SDI/GPIO3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 194.01932 88.463854 -90)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP10" (at -1 0 -90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 78 "/SDI/GPIO2") (pinfunction "1") (pintype "passive"))
  )
  (footprint "SYZYGY:QTH-020-01-F-D-DP-A" (layer "F.Cu")
    (at 150.51932 106.463854 -90)
    (descr "0.50 mm Q Pairs® High-Speed Ground Plane Terminal Strip, Differential Pair")
    (property "Manufacturer" "Samtec")
    (property "Manufacturer_PN" "QTH-020-01-F-D-DP-A")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.50 mm Q Pairs® High-Speed Ground Plane Terminal Strip, Differential Pair")
    (attr smd)
    (fp_text reference "J1" (at 9.9 -3.8 90) (layer "F.SilkS"))
    (fp_text value "SYZYGY_TXR-4" (at 4.0894 5.0546 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -9.24 -2.03 90) (size 1.02 1.02) (drill 1.02) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (pad "" np_thru_hole circle (at 9.24 -2.03 90) (size 1.02 1.02) (drill 1.02) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (pad "0" smd rect (at -8.44 0 90) (size 2.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "0" smd rect (at -3.17 0 90) (size 4.7 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "0" smd rect (at 3.18 0 90) (size 4.7 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "0" smd rect (at 8.44 0 90) (size 2.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "1" smd rect (at -7.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/MCU_SCL_USCK") (pinfunction "SCL") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "2" smd rect (at -7.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+5V") (pinfunction "5V") (pintype "power_out") (solder_mask_margin 0.0508))
    (pad "3" smd rect (at -6.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/MCU_SDA_MOSI") (pinfunction "SDA") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "4" smd rect (at -6.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/R_GA") (pinfunction "R_GA") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "5" smd rect (at -5.74999 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/RX0P") (pinfunction "RX0p") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "6" smd rect (at -5.74999 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/TX0P") (pinfunction "TX0p") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "7" smd rect (at -5.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/RX0N") (pinfunction "RX0n") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "8" smd rect (at -5.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/TX0N") (pinfunction "TX0n") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "9" smd rect (at -4.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/RX1P") (pinfunction "RX1p") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "10" smd rect (at -4.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/TX1P") (pinfunction "TX1p") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "11" smd rect (at -3.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/RX1N") (pinfunction "RX1n") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "12" smd rect (at -3.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/TX1N") (pinfunction "TX1n") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "13" smd rect (at -2.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/REFCLKP") (pinfunction "REFCLKp") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "14" smd rect (at -2.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/SDIN") (pinfunction "S0") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "15" smd rect (at -2.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/REFCLKN") (pinfunction "REFCLKn") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "16" smd rect (at -2.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/CS_n") (pinfunction "S1") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "17" smd rect (at -1.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/CLK_FS") (pinfunction "S2") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "18" smd rect (at -1.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/SDOUT") (pinfunction "S3") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "19" smd rect (at -0.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/CLK_OE") (pinfunction "S4") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "20" smd rect (at -0.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/SCLK") (pinfunction "S5") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "21" smd rect (at 0.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/S6") (pinfunction "S6") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "22" smd rect (at 0.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/S7") (pinfunction "S7") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "23" smd rect (at 0.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/S8") (pinfunction "S8") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "24" smd rect (at 0.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/S9") (pinfunction "S9") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "25" smd rect (at 1.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/RX3P") (pinfunction "RX3p") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "26" smd rect (at 1.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/TX3P") (pinfunction "TX3p") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "27" smd rect (at 2.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/RX3N") (pinfunction "RX3n") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "28" smd rect (at 2.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/TX3N") (pinfunction "TX3n") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "29" smd rect (at 3.25001 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/RX2P") (pinfunction "RX2p") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "30" smd rect (at 3.25001 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/TX2P") (pinfunction "TX2p") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "31" smd rect (at 3.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/RX2N") (pinfunction "RX2n") (pintype "passive") (solder_mask_margin 0.0508))
    (pad "32" smd rect (at 3.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/TX2N") (pinfunction "TX2n") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "33" smd rect (at 4.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/P2C_CLKP") (pinfunction "P2C_CLKp") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "34" smd rect (at 4.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/C2P_CLKP") (pinfunction "C2P_CLKp") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "35" smd rect (at 5.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/P2C_CLKN") (pinfunction "P2C_CLKn") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "36" smd rect (at 5.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/C2P_CLKN") (pinfunction "C2P_CLKn") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "37" smd rect (at 6.25 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/RSVD_37") (pinfunction "RSVD") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "38" smd rect (at 6.25 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/RSVD_38") (pinfunction "RSVD") (pintype "passive+no_connect") (solder_mask_margin 0.0508))
    (pad "39" smd rect (at 6.75 -3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VIO") (pinfunction "VIO") (pintype "power_out") (solder_mask_margin 0.0508))
    (pad "40" smd rect (at 6.75 3.09 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "+3.3V") (pintype "power_out") (solder_mask_margin 0.0508))
    (pad "MH" thru_hole circle (at -10.845 -0.5 90) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (pad "MH" thru_hole circle (at 10.845 -0.5 90) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/../3D/QTH-020-01-F-D-DP-A.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 197.51932 117.463854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at -0.1 -2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SDI/SDO_N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(C20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 192.21932 91.463854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/VIO") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 187.51932 94.963854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "/SDI/VCCO_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:BEADC1005X55N" (layer "F.Cu")
    (at 200.51932 93.963854 180)
    (descr "MAF1005GWZ102AT000")
    (tags "Filter")
    (property "Manufacturer" "TDK")
    (property "Manufacturer_PN" "MAF1005GWZ102AT000")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Ferrite bead, small symbol")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr smd)
    (fp_text reference "FB2" (at 0 1) (layer "F.SilkS"))
    (fp_text value "Ferrite" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.55 0 270) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VIO") (pintype "passive"))
    (pad "2" smd rect (at 0.55 0 270) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/SDI/VCC_I") (pintype "passive"))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/MAF1005GWZ102AT000.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 197.01932 124.963854)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP14" (at 0 3 90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 82 "/SDI/GPIO6") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 189.71932 114.563854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "470nF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U3-LF-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U3-LF+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 197.01932 118.963854 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C24" (at 2 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/SDI/VCCO_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 195.01932 124.963854)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP12" (at 0 3 90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 80 "/SDI/GPIO5") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 195.21932 122.763854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C31" (at -0.1 -1 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SDI/VCC_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 185.51932 118.063854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 0 2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/TX0P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDI/TxCP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 185.51932 96.663854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/SDI/RxCP") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/RX0N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 157.26932 109.713854)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 1.15 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/RX2P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SamacSys:SOT95P280X145-5N" (layer "F.Cu")
    (at 169.51932 111.463854 90)
    (descr "DBV")
    (tags "Integrated Circuit")
    (property "Description" "")
    (property "Height" "1.45")
    (property "Manufacturer" "TI")
    (property "Manufacturer_Name" "Texas Instruments")
    (property "Manufacturer_PN" "LP5907MFX-2.5/NOPB")
    (property "Manufacturer_Part_Number" "LP5907MFX")
    (property "Mouser Part Number" "")
    (property "Mouser Price/Stock" "")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "TPS73018DBVTG4, Low Dropout Voltage Regulator, 0.2A, 1.8V +/-2%, 2.7 to 5.5Vin, 0.56W, 5-Pin SOT-23")
    (attr smd)
    (fp_text reference "U5" (at 0 3 90) (layer "F.SilkS"))
    (fp_text value "LP5907MFX-2.5/NOPB" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.25 -0.95 180) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "IN") (pintype "input"))
    (pad "2" smd rect (at -1.25 0 180) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.25 0.95 180) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "EN") (pintype "passive"))
    (pad "4" smd rect (at 1.25 0.95 180) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "unconnected-(U5-NC-Pad4)") (pinfunction "NC") (pintype "passive"))
    (pad "5" smd rect (at 1.25 -0.95 180) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/+2.5V") (pinfunction "OUT") (pintype "output"))
    (model "D:\\NewTek\\files\\KiCad-Lib\\SamacSys_Parts.3dshapes\\TPS3840DL46DBVR.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 198.51932 116.463854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/SDI/SDO_P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/SDI/SDO_X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 197.01932 93.963854 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 2 0 90) (layer "F.SilkS"))
    (fp_text value "1.0uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SDI/VCC_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:BEADC1005X55N" (layer "F.Cu")
    (at 187.51932 92.463854)
    (descr "MAF1005GWZ102AT000")
    (tags "Filter")
    (property "Manufacturer" "TDK")
    (property "Manufacturer_PN" "MAF1005GWZ102AT000")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Ferrite bead, small symbol")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr smd)
    (fp_text reference "FB1" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "Ferrite" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.55 0 90) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VIO") (pintype "passive"))
    (pad "2" smd rect (at 0.55 0 90) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "/SDI/VCCO_I") (pintype "passive"))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/MAF1005GWZ102AT000.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 176.24432 86.938854)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_02x03_Odd_Even" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/AVR/MCU_MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "/MCU_SCL_USCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/MCU_SDA_MOSI") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "/AVR/MCU_RESET_B") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 195.21932 121.263854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 2.5 -1) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SDI/VCC_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 193.51932 98.463854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 1) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SDI/VCC_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 199.51932 95.463854 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "2.0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 192.01932 98.963854 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 2 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/SDI/VCO_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 185.51932 95.663854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/SDI/RxCN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/RX0P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 199.51932 117.463854)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "75R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(C20-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 192.81932 121.263854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 2.5 -1) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/VIO") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 157.26932 108.713854)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 1.15 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/RX3N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 187.51932 93.963854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "/SDI/VCCO_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 195.51932 98.463854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "470nF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U2-LF-)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U2-LF+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:BEADC1005X55N" (layer "F.Cu")
    (at 201.51932 118.763854 180)
    (descr "MAF1005GWZ102AT000")
    (tags "Filter")
    (property "Manufacturer" "TDK")
    (property "Manufacturer_PN" "MAF1005GWZ102AT000")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Ferrite bead, small symbol")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr smd)
    (fp_text reference "FB3" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "Ferrite" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.55 0 270) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.55 0 270) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/SDI/VCCO_O") (pintype "passive"))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/MAF1005GWZ102AT000.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 197.51932 95.463854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/SDI/SDI_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 199.51932 118.963854 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C32" (at 2 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/SDI/VCCO_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 195.51932 114.563854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C23" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SDI/VCC_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 157.26932 110.713854)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 1.15 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/RX2N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 185.51932 119.063854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 0 2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/TX0N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/SDI/TxCN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:BNC7T-J-P-XX-ST-EM1D" (layer "F.Cu")
    (at 213.51932 116.463854 90)
    (descr "12G SDI BNC jack, edge mount")
    (tags "12G SDI BNC jack, edge mount")
    (property "Manufacturer" "Samtec")
    (property "Manufacturer_PN" "BNC7T-J-P-GN-ST-EM1D")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "BNC2" (at -1.905 -8.255 90) (layer "F.SilkS"))
    (fp_text value "BNC" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 6.25 -0.25 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 -2.185 90) (size 1.98 1.83) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/SDI/SDO_X") (pinfunction "In") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -4.825 -3.525 90) (size 1.35 6.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -4.25 -3.525 90) (size 1.5 6.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at 4.25 -3.525 90) (size 1.5 6.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at 4.825 -3.525 90) (size 1.35 6.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/BNC7T-J-P-XX-ST-EM1D.step"
      (offset (xyz 0 2.5 0.625))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 -180))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 159.51932 103.463854 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at -2 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "/CLKP") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/REFCLKP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 167.21932 112.463854 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C33" (at 0 -1 90) (layer "F.SilkS"))
    (fp_text value "1.0uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:QFN40P600X400X100-41N-D" (layer "F.Cu")
    (at 192.51932 94.963854 180)
    (descr "QFN40")
    (tags "Integrated Circuit")
    (property "Description" "Equalizers 12G UHD-SDI Retiming Adaptive Cable Equ")
    (property "Height" "1")
    (property "Manufacturer" "Semtech")
    (property "Manufacturer_Name" "SEMTECH")
    (property "Manufacturer_PN" "GS12241-INE3")
    (property "Manufacturer_Part_Number" "GS12241-INE3")
    (property "Mouser Part Number" "947-GS12241-INE3")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Semtech/GS12241-INE3?qs=wd5RIQLrsJi2uBHBmmCXDg%3D%3D")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Equalizers 12G UHD-SDI Retiming Adaptive Cable Equ")
    (attr smd)
    (fp_text reference "U2" (at -5.5 -5) (layer "F.SilkS"))
    (fp_text value "GS12241-INE3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.95 -1.4 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_SDI_1") (pintype "power_in"))
    (pad "2" smd rect (at -2.95 -1 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/SDI/SDI_P") (pinfunction "SDI") (pintype "input"))
    (pad "3" smd rect (at -2.95 -0.6 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/SDI/SDI_N") (pinfunction "SDI_TERM") (pintype "passive"))
    (pad "4" smd rect (at -2.95 -0.2 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/SDI/VCC_I") (pinfunction "VCC_SDI") (pintype "power_in"))
    (pad "5" smd rect (at -2.95 0.2 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "unconnected-(U2-RSVD_1-Pad5)") (pinfunction "RSVD_1") (pintype "passive+no_connect"))
    (pad "6" smd rect (at -2.95 0.6 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "unconnected-(U2-RSVD_2-Pad6)") (pinfunction "RSVD_2") (pintype "passive+no_connect"))
    (pad "7" smd rect (at -2.95 1 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "unconnected-(U2-RSVD_3-Pad7)") (pinfunction "RSVD_3") (pintype "passive+no_connect"))
    (pad "8" smd rect (at -2.95 1.4 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_SDI_2") (pintype "power_in"))
    (pad "9" smd rect (at -2.2 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "unconnected-(U2-RSVD_4-Pad9)") (pinfunction "RSVD_4") (pintype "passive+no_connect"))
    (pad "10" smd rect (at -1.8 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/CS_n") (pinfunction "~{CS}") (pintype "input"))
    (pad "11" smd rect (at -1.4 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/SDIN") (pinfunction "SDIN") (pintype "input"))
    (pad "12" smd rect (at -1 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/SDI/SDIX") (pinfunction "SDOUT") (pintype "output"))
    (pad "13" smd rect (at -0.6 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/SCLK") (pinfunction "SCLK") (pintype "input"))
    (pad "14" smd rect (at -0.2 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS_1") (pintype "power_in"))
    (pad "15" smd rect (at 0.2 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS_2") (pintype "power_in"))
    (pad "16" smd rect (at 0.6 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VIO") (pinfunction "VDD") (pintype "power_in"))
    (pad "17" smd rect (at 1 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/SDI/GPIO1") (pinfunction "GPIO_0") (pintype "bidirectional"))
    (pad "18" smd rect (at 1.4 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/SDI/GPIO0") (pinfunction "GPIO_1") (pintype "bidirectional"))
    (pad "19" smd rect (at 1.8 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_1") (pintype "power_in"))
    (pad "20" smd rect (at 2.2 1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/SDI/VCC_I") (pinfunction "VCCO1P8_1") (pintype "power_in"))
    (pad "21" smd rect (at 2.95 1.4 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEEO_1") (pintype "power_in"))
    (pad "22" smd rect (at 2.95 1 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "unconnected-(U2-~{DDO1}{slash}~{RCO}-Pad22)") (pinfunction "~{DDO1}/~{RCO}") (pintype "output"))
    (pad "23" smd rect (at 2.95 0.6 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "unconnected-(U2-DDO1{slash}RCO-Pad23)") (pinfunction "DDO1/RCO") (pintype "output"))
    (pad "24" smd rect (at 2.95 0.2 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "/SDI/VCCO_I") (pinfunction "VCCO_1") (pintype "power_in"))
    (pad "25" smd rect (at 2.95 -0.2 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "/SDI/VCCO_I") (pinfunction "VCCO_0") (pintype "power_in"))
    (pad "26" smd rect (at 2.95 -0.6 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/SDI/RxCN") (pinfunction "~{DDO0}") (pintype "output"))
    (pad "27" smd rect (at 2.95 -1 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/SDI/RxCP") (pinfunction "DDO0") (pintype "output"))
    (pad "28" smd rect (at 2.95 -1.4 270) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEEO_2") (pintype "power_in"))
    (pad "29" smd rect (at 2.2 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/SDI/VCC_I") (pinfunction "VCCO1P8_0") (pintype "power_in"))
    (pad "30" smd rect (at 1.8 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "unconnected-(U2-VCO_FILT10-Pad30)") (pinfunction "VCO_FILT10") (pintype "passive+no_connect"))
    (pad "31" smd rect (at 1.4 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_2") (pintype "power_in"))
    (pad "32" smd rect (at 1 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "unconnected-(U2-RSVD_5-Pad32)") (pinfunction "RSVD_5") (pintype "passive+no_connect"))
    (pad "33" smd rect (at 0.6 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/SDI/GPIO2") (pinfunction "GPIO_2") (pintype "bidirectional"))
    (pad "34" smd rect (at 0.2 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/SDI/VCO_I") (pinfunction "VCO_FILT") (pintype "passive"))
    (pad "35" smd rect (at -0.2 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/SDI/VCC_I") (pinfunction "VCC_CORE") (pintype "power_in"))
    (pad "36" smd rect (at -0.6 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/SDI/GPIO3") (pinfunction "GPIO_3") (pintype "bidirectional"))
    (pad "37" smd rect (at -1 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_3") (pintype "power_in"))
    (pad "38" smd rect (at -1.4 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_4") (pintype "power_in"))
    (pad "39" smd rect (at -1.8 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(U2-LF+)") (pinfunction "LF+") (pintype "passive"))
    (pad "40" smd rect (at -2.2 -1.95 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(U2-LF-)") (pinfunction "LF-") (pintype "passive"))
    (pad "41" smd rect (at 0 0 270) (size 1.68 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "TAB") (pintype "passive") (zone_connect 0))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/GS12241-INE3.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 157.26932 101.963854)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -2.05 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "/RX1P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 190.51932 98.463854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 1) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SDI/VCC_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:BEADC1005X55N" (layer "F.Cu")
    (at 197.51932 122.763854 180)
    (descr "MAF1005GWZ102AT000")
    (tags "Filter")
    (property "Manufacturer" "TDK")
    (property "Manufacturer_PN" "MAF1005GWZ102AT000")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Ferrite bead, small symbol")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr smd)
    (fp_text reference "FB4" (at -0.1 -1 180) (layer "F.SilkS"))
    (fp_text value "Ferrite" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.55 0 270) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VIO") (pintype "passive"))
    (pad "2" smd rect (at 0.55 0 270) (size 0.6 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SDI/VCC_O") (pintype "passive"))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/MAF1005GWZ102AT000.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 157.26932 102.963854)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at -2.05 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0.015 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.015 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/RX1N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 199.01932 124.963854)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP15" (at 0 3 90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 83 "/SDI/GPIO7") (pinfunction "1") (pintype "passive"))
  )
  (footprint "SYZYGY:QFN40P600X400X100-41N-D" (layer "F.Cu")
    (at 192.51932 117.763854)
    (descr "QFN40")
    (tags "Integrated Circuit")
    (property "Description" "Video ICs 12G UHD-SDI ReTIMING Cable Driver")
    (property "Height" "1")
    (property "Manufacturer" "Semtech")
    (property "Manufacturer_Name" "SEMTECH")
    (property "Manufacturer_PN" "GS12281-INTE3")
    (property "Manufacturer_Part_Number" "GS12281-INTE3")
    (property "Mouser Part Number" "947-GS12281-INTE3")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Semtech/GS12281-INTE3?qs=f9yNj16SXrKyyvPQgg3Jvg%3D%3D")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Video ICs 12G UHD-SDI ReTIMING Cable Driver")
    (attr smd)
    (fp_text reference "U3" (at -5.5 -3.8) (layer "F.SilkS"))
    (fp_text value "GS12281-INTE3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.95 -1.4 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_DDI_1") (pintype "passive"))
    (pad "2" smd rect (at -2.95 -1 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "unconnected-(U3-RSVD_1-Pad2)") (pinfunction "RSVD_1") (pintype "passive+no_connect"))
    (pad "3" smd rect (at -2.95 -0.6 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "unconnected-(U3-RSVD_2-Pad3)") (pinfunction "RSVD_2") (pintype "passive+no_connect"))
    (pad "4" smd rect (at -2.95 -0.2 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SDI/VCC_O") (pinfunction "VCC_DDI") (pintype "passive"))
    (pad "5" smd rect (at -2.95 0.2 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/SDI/TERMO") (pinfunction "TERM") (pintype "passive"))
    (pad "6" smd rect (at -2.95 0.6 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SDI/TxCP") (pinfunction "DDI") (pintype "passive"))
    (pad "7" smd rect (at -2.95 1 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/SDI/TxCN") (pinfunction "~{DDI}") (pintype "passive"))
    (pad "8" smd rect (at -2.95 1.4 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_DDI_2") (pintype "passive"))
    (pad "9" smd rect (at -2.2 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(U3-RSVD_3-Pad9)") (pinfunction "RSVD_3") (pintype "passive+no_connect"))
    (pad "10" smd rect (at -1.8 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/CS_n") (pinfunction "~{CS}") (pintype "passive"))
    (pad "11" smd rect (at -1.4 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "/SDI/SDIX") (pinfunction "SDIN") (pintype "passive"))
    (pad "12" smd rect (at -1 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/SDOUT") (pinfunction "SDOUT") (pintype "passive"))
    (pad "13" smd rect (at -0.6 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/SCLK") (pinfunction "SCLK") (pintype "passive"))
    (pad "14" smd rect (at -0.2 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS_1") (pintype "passive"))
    (pad "15" smd rect (at 0.2 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS_2") (pintype "passive"))
    (pad "16" smd rect (at 0.6 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/VIO") (pinfunction "VDD") (pintype "passive"))
    (pad "17" smd rect (at 1 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/SDI/GPIO4") (pinfunction "GPIO0") (pintype "passive"))
    (pad "18" smd rect (at 1.4 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/SDI/GPIO5") (pinfunction "GPIO1") (pintype "passive"))
    (pad "19" smd rect (at 1.8 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_1") (pintype "passive"))
    (pad "20" smd rect (at 2.2 1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SDI/VCC_O") (pinfunction "VCCO1P8_1") (pintype "passive"))
    (pad "21" smd rect (at 2.95 1.4 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEEO_1") (pintype "passive"))
    (pad "22" smd rect (at 2.95 1 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "unconnected-(U3-~{SDO1}{slash}~{RCO}-Pad22)") (pinfunction "~{SDO1}/~{RCO}") (pintype "passive+no_connect"))
    (pad "23" smd rect (at 2.95 0.6 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "unconnected-(U3-SDO1{slash}RCO-Pad23)") (pinfunction "SDO1/RCO") (pintype "passive+no_connect"))
    (pad "24" smd rect (at 2.95 0.2 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/SDI/VCCO_O") (pinfunction "VCCO_1") (pintype "passive"))
    (pad "25" smd rect (at 2.95 -0.2 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/SDI/VCCO_O") (pinfunction "VCCO_0") (pintype "passive"))
    (pad "26" smd rect (at 2.95 -0.6 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SDI/SDO_N") (pinfunction "~{SDO0}") (pintype "passive"))
    (pad "27" smd rect (at 2.95 -1 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/SDI/SDO_P") (pinfunction "SDO0") (pintype "passive"))
    (pad "28" smd rect (at 2.95 -1.4 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEEO_2") (pintype "passive"))
    (pad "29" smd rect (at 2.2 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SDI/VCC_O") (pinfunction "VCCO1P8_0") (pintype "passive"))
    (pad "30" smd rect (at 1.8 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "unconnected-(U3-RSVD_4-Pad30)") (pinfunction "RSVD_4") (pintype "passive+no_connect"))
    (pad "31" smd rect (at 1.4 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_2") (pintype "passive"))
    (pad "32" smd rect (at 1 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "REF_CLK") (pintype "passive"))
    (pad "33" smd rect (at 0.6 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/SDI/GPIO6") (pinfunction "GPIO2") (pintype "passive"))
    (pad "34" smd rect (at 0.2 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/SDI/VCO_O") (pinfunction "VCO_FILT") (pintype "passive"))
    (pad "35" smd rect (at -0.2 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SDI/VCC_O") (pinfunction "VCC_CORE") (pintype "passive"))
    (pad "36" smd rect (at -0.6 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/SDI/GPIO7") (pinfunction "GPIO3") (pintype "passive"))
    (pad "37" smd rect (at -1 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_3") (pintype "passive"))
    (pad "38" smd rect (at -1.4 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VEE_CORE_4") (pintype "passive"))
    (pad "39" smd rect (at -1.8 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(U3-LF+)") (pinfunction "LF+") (pintype "passive"))
    (pad "40" smd rect (at -2.2 -1.95) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U3-LF-)") (pinfunction "LF-") (pintype "passive"))
    (pad "41" smd rect (at 0 0 90) (size 1.68 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "EP") (pintype "passive") (zone_connect 0))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/GS12241-INE3.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 198.01932 118.963854 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at 2 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/SDI/VCCO_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:TestPoint-20mil" (layer "F.Cu")
    (at 156.74272 95.114134)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr smd)
    (fp_text reference "TP3" (at 0 1.05) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -0.9) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Mask")
      (net 71 "Net-(U1-PA3)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 167.21932 110.463854 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C34" (at 0 2 90) (layer "F.SilkS"))
    (fp_text value "1.0uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/+2.5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 193.51932 114.563854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C28" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/SDI/VCO_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 157.26932 107.713854)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 1.15 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/RX3P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 187.51932 117.763854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C29" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/SDI/TERMO") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:TestPoint-20mil" (layer "F.Cu")
    (at 156.74272 95.977734)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr smd)
    (fp_text reference "TP2" (at 0 1.05) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -0.9) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Mask")
      (net 70 "Net-(U1-PA2)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 198.51932 93.963854 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C30" (at 2 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SDI/VCC_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:TestPoint-20mil" (layer "F.Cu")
    (at 163.32132 94.809334)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr smd)
    (fp_text reference "TP4" (at 0 1.05) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -0.9) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Mask")
      (net 72 "Net-(U1-PA7)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "SYZYGY:TestPoint-20mil" (layer "F.Cu")
    (at 156.74272 96.841334)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr smd)
    (fp_text reference "TP1" (at 0 1.05) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -0.9) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Mask")
      (net 69 "Net-(U1-PA1)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0508))
  )
  (footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen" (layer "F.Cu")
    (at 201.51932 106.463854)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "OSHW-Logo_5.7x6mm_SilkScreen" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (at 159.51932 104.463854 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/CLKN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/REFCLKN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 191.61932 114.563854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C26" (at 0 2) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SDI/VCC_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:Si513-A" (layer "F.Cu")
    (at 169.26932 105.213854 90)
    (descr "SI512, SI513, Programmable oscillator, 7.0 x 5.0")
    (tags "SI512, SI513, Programmable oscillator, 7.0 x 5.0")
    (property "Manufacturer" "Skyworks")
    (property "Manufacturer_PN" "513FCA000270AAG")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual frequency crystal oscillator (XO) 100 kHz to 250 MHz, Single-ended CMOS output")
    (property "ki_keywords" "Dual frequency crystal oscillator")
    (attr smd)
    (fp_text reference "U4" (at -2.75 4.25 90) (layer "F.SilkS"))
    (fp_text value "513FCA000270AAG" (at -0.1 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.5 2.1 90) (size 1.55 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/CLK_OE") (pinfunction "OE") (pintype "input"))
    (pad "2" smd rect (at 0 2.1 90) (size 1.55 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/CLK_FS") (pinfunction "FS") (pintype "input"))
    (pad "3" smd rect (at 2.5 2.1 90) (size 1.55 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at 2.5 -2.1 90) (size 1.55 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/CLKP") (pinfunction "CLK+") (pintype "output"))
    (pad "5" smd rect (at 0 -2.1 90) (size 1.55 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/CLKN") (pinfunction "CLK-") (pintype "output"))
    (pad "6" smd rect (at -2.5 -2.1 90) (size 1.55 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/+2.5V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SI570_SI571_Standard.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 198.51932 96.463854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDI/SDI_X") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/SDI/SDI_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 189.91932 91.463854)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 -1) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SDI/VCC_I") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (at 193.01932 124.963854)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP13" (at 0 3 90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 81 "/SDI/GPIO4") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (at 188.01932 116.263854 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C27" (at 0 -1 90) (layer "F.SilkS"))
    (fp_text value "1.0uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SDI/VCC_O") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SYZYGY:BNC7T-J-P-XX-ST-EM1D" (layer "F.Cu")
    (at 213.51932 96.463854 90)
    (descr "12G SDI BNC jack, edge mount")
    (tags "12G SDI BNC jack, edge mount")
    (property "Manufacturer" "Samtec")
    (property "Manufacturer_PN" "BNC7T-J-P-GN-ST-EM1D")
    (property "Sheetfile" "sdi.kicad_sch")
    (property "Sheetname" "SDI")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "BNC1" (at -1.905 -8.255 90) (layer "F.SilkS"))
    (fp_text value "BNC" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 6.25 -0.25 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 -2.185 90) (size 1.98 1.83) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SDI/SDI_X") (pinfunction "In") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -4.825 -3.525 90) (size 1.35 6.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -4.25 -3.525 90) (size 1.5 6.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at 4.25 -3.525 90) (size 1.5 6.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at 4.825 -3.525 90) (size 1.35 6.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive") (solder_mask_margin 0.102))
    (model "D:/NewTek/files/SYZYGY/KiCAD/3D/BNC7T-J-P-XX-ST-EM1D.step"
      (offset (xyz 0 2.5 0.625))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 -180))
    )
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "B.Cu")
    (at 146.08432 128.936854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID6" (at 0 2 90) (layer "B.SilkS") hide)
    (fp_text value "Fiducial" (at 0 -2 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "B.Cu")
    (at 203.51932 83.463854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID7" (at 0 2 90) (layer "B.SilkS") hide)
    (fp_text value "Fiducial" (at 0 -2 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "B.Cu")
    (at 203.51932 129.463854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID8" (at 0 2 90) (layer "B.SilkS") hide)
    (fp_text value "Fiducial" (at 0 -2 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "SYZYGY:MountingHole_3.2mm_M3_6.5mm_Pad_TopBottom" (layer "B.Cu")
    (at 150.51932 87.553854 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H1" (at 0 -0.5 90) (layer "B.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 0.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0 90) (layer "B.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 3.6 3.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "SYZYGY:MountingHole_3.2mm_M3_6.5mm_Pad_TopBottom" (layer "B.Cu")
    (at 150.51932 125.373854 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H2" (at 0 -0.5 90) (layer "B.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 0.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0 90) (layer "B.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 3.6 3.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "SYZYGY:MountingHole_3.2mm_M3_6.5mm_Pad_TopBottom" (layer "B.Cu")
    (at 160.51932 86.463854 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H3" (at 0 -0.5 90) (layer "B.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 0.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0 90) (layer "B.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 3.6 3.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "SYZYGY:MountingHole_3.2mm_M3_6.5mm_Pad_TopBottom" (layer "B.Cu")
    (at 160.51932 126.463854 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H4" (at 0 -0.5 90) (layer "B.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 0.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0 90) (layer "B.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 3.6 3.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "SYZYGY:MountingHole_3.2mm_M3_6.5mm_Pad_TopBottom" (layer "B.Cu")
    (at 208.51932 86.463854 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H5" (at 0 -0.5 90) (layer "B.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 0.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0 90) (layer "B.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 3.6 3.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "SYZYGY:MountingHole_3.2mm_M3_6.5mm_Pad_TopBottom" (layer "B.Cu")
    (at 208.51932 126.463854 -90)
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole)
    (fp_text reference "H6" (at 0 -0.5 90) (layer "B.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 0.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0 90) (layer "B.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 3.6 3.6) (drill 3.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0 270) (size 6.5 6.5) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "B.Cu")
    (at 155.29732 83.825854 -90)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "SZG-SDI-12G-Fire.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fiducial Marker")
    (property "ki_keywords" "fiducial marker")
    (attr smd)
    (fp_text reference "FID5" (at 0 2 90) (layer "B.SilkS") hide)
    (fp_text value "Fiducial" (at 0 -2 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab") hide)
    (pad "" smd circle (at 0 0 270) (size 1 1) (layers "B.Cu" "B.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "SYZYGY:SYZYGY_Logo" (layer "B.Cu")
    (at 146.86932 105.913854 -90)
    (attr through_hole)
    (fp_text reference "LOGO2" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "B.SilkS") hide)
  )
  (footprint "SYZYGY:Tag-Connect_TC2030-IDC-FP_2x03_P1.27mm_Vertical" locked (layer "B.Cu")
    (at 169.11932 89.463854 180)
    (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC.pdf")
    (tags "tag connect programming header pogo pins")
    (property "Manufacturer" "N/A")
    (property "Manufacturer_PN" "Part of PCB")
    (property "Sheetfile" "avr.kicad_sch")
    (property "Sheetname" "AVR")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at 4.05 -0.05 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x06" (at 0 4.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 4.05 -0.05 90) (layer "F.SilkS"))
    (fp_text user "KEEPOUT" (at 0 0) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "" np_thru_hole circle locked (at -2.54 -2.54 180) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at -2.54 2.54 180) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at 0.635 -2.54 180) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at 0.635 2.54 180) (size 2.3749 2.3749) (drill 2.3749) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle locked (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle locked (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers "B.Cu" "B.Mask")
      (net 65 "/AVR/MCU_MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "1" connect circle locked (at -1.27 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 65 "/AVR/MCU_MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" connect circle locked (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 3 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "2" connect circle locked (at -1.27 0.635 180) (size 0.7874 0.7874) (layers "B.Cu" "B.Mask")
      (net 3 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" connect circle locked (at 0 -0.635 180) (size 0.7874 0.7874) (layers "B.Cu" "B.Mask")
      (net 17 "/MCU_SCL_USCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "3" connect circle locked (at 0 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 17 "/MCU_SCL_USCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" connect circle locked (at 0 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 16 "/MCU_SDA_MOSI") (pinfunction "Pin_4") (pintype "passive"))
    (pad "4" connect circle locked (at 0 0.635 180) (size 0.7874 0.7874) (layers "B.Cu" "B.Mask")
      (net 16 "/MCU_SDA_MOSI") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" connect circle locked (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers "B.Cu" "B.Mask")
      (net 66 "/AVR/MCU_RESET_B") (pinfunction "Pin_5") (pintype "passive"))
    (pad "5" connect circle locked (at 1.27 0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 66 "/AVR/MCU_RESET_B") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" connect circle locked (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "6" connect circle locked (at 1.27 0.635 180) (size 0.7874 0.7874) (layers "B.Cu" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
  )
  (footprint "SYZYGY:SYZYGY_TXR4_Logo" (layer "B.Cu")
    (at 146.71932 90.663854 -90)
    (attr smd)
    (fp_text reference "LOGO1" (at 0 0.5 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "SYZYGY_STD_Logo" (at 0 -1 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "TXR4" (at -2.956787 1.103821 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab") hide)
  )
  (gr_line (start 143.51932 81.463854) (end 143.51932 131.463854)
    (layer "Edge.Cuts"))
  (gr_line (start 213.51932 81.463854) (end 143.51932 81.463854)
    (layer "Edge.Cuts"))
  (gr_line (start 213.51932 131.463854) (end 213.51932 81.463854)
    (layer "Edge.Cuts"))
  (gr_line (start 143.51932 131.463854) (end 213.51932 131.463854)
    (layer "Edge.Cuts"))
  (gr_text "SZG-SDI-12G-Fire\nRev.A" (at 150.09552 100.346854 90) (layer "B.SilkS"))
  (gr_text "SYG-SDI-12G-Fire\nRev.A\nLicensed under\nCERN-OHL-P v2" (at 177.51932 110.463854) (layer "F.SilkS"))
  (gr_text "SDI Tx" (at 209.51932 109.463854) (layer "F.SilkS"))
  (gr_text "SDI Rx" (at 209.51932 103.463854) (layer "F.SilkS"))
  (gr_text "Top View" (at 83.51392 127.759604) (layer "Cmts.User"))
  (gr_text "MH2" (at 83.51392 119.759604) (layer "Cmts.User"))
  (gr_text "SYZYGY Connector\nre: BeagleV-Fire MH2\nX = 67.0054\nY = 16.29575" (at 103.51932 111.463854) (layer "Cmts.User"))
  (gr_text "BeagleV M2\nre: SYZYGY TXR4 Origin\nX = 60.0054\nY = 8.70425" (at 103.50932 136.463534) (layer "Cmts.User"))
  (gr_text "Carrier board edge" (at 156.71932 107.463854 90) (layer "Eco1.User"))
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 143.51932 81.463854) (xy 213.51932 81.463854))
    (height -16)
    (orientation 0)
    (gr_text "70.0000 mm" (at 178.51932 64.313854) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 143.51932 81.463854) (xy 152.54932 97.223854))
    (height -7.5)
    (orientation 1)
    (gr_text "15.760 mm" (at 134.86932 89.343854 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 213.51932 81.463854) (xy 208.51932 126.463854))
    (height 8)
    (orientation 1)
    (gr_text "45.0000 mm" (at 220.36932 103.963854 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 213.51932 81.463854) (xy 208.51932 86.463854))
    (height 4)
    (orientation 1)
    (gr_text "5.0 mm" (at 219.01932 84.963854 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 1))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 208.51932 86.463854) (xy 213.51932 81.463854))
    (height -9)
    (orientation 0)
    (gr_text "5.0 mm" (at 210.01932 75.963854) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 1))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 160.51932 86.463854) (xy 143.51932 81.463854))
    (height -17)
    (orientation 0)
    (gr_text "17.000 mm" (at 152.01932 68.313854) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 143.51932 81.463854) (xy 150.51932 87.553854))
    (height -4)
    (orientation 1)
    (gr_text "6.090 mm" (at 138.01932 85.963854 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 152.54932 97.223854) (xy 143.51932 81.463854))
    (height -23.76032)
    (orientation 0)
    (gr_text "9.030 mm" (at 148.03932 71.963854) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 3))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 150.51932 87.553854) (xy 143.51932 81.463854))
    (height -10.09)
    (orientation 0)
    (gr_text "7.0 mm" (at 147.01932 75.963854) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 1))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 143.51932 81.463854) (xy 150.51932 125.373854))
    (height -11.5)
    (orientation 1)
    (gr_text "43.9100 mm" (at 130.86932 103.418854 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "Dwgs.User")
    (pts (xy 143.51932 81.463854) (xy 143.51932 131.463854))
    (height -15.5)
    (orientation 1)
    (gr_text "50.0000 mm" (at 126.86932 106.463854 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.15432 99.363854)
        (xy 148.15432 98.413854)
        (xy 146.70432 98.413854)
        (xy 146.70432 99.363854)
      )
    )
  )
  (zone (net 26) (net_name "/VIO") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3048))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.52732 114.113334)
        (xy 154.52732 113.071934)
        (xy 152.87952 113.071934)
        (xy 152.87952 113.863534)
        (xy 153.10932 114.113334)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.61932 111.993854)
        (xy 151.61932 107.293854)
        (xy 150.19932 107.293854)
        (xy 150.19932 111.993854)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.61932 105.643854)
        (xy 151.61932 100.943854)
        (xy 150.19932 100.943854)
        (xy 150.19932 105.643854)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.61932 116.173854)
        (xy 151.61932 113.633854)
        (xy 150.19932 113.633854)
        (xy 150.19932 116.173854)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.127) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.61932 99.293854)
        (xy 151.61932 96.763854)
        (xy 150.19932 96.753854)
        (xy 150.19932 99.293854)
      )
    )
  )
  (zone (net 3) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.12552 113.138654)
        (xy 148.12552 114.078454)
        (xy 146.70312 114.078454)
        (xy 146.70312 113.138654)
      )
    )
  )
  (zone locked (net 2) (net_name "GND") (layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2794))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.18) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 213.01932 82.063854)
        (xy 144.01932 82.063854)
        (xy 144.01932 130.963854)
        (xy 213.01932 130.963854)
      )
    )
  )
  (zone (net 3) (net_name "+3V3") (layer "In1.Cu") (hatch edge 0.508)
    (priority 80)
    (connect_pads (clearance 0.2794))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.15292 96.613054)
        (xy 155.32792 93.438054)
        (xy 163.81932 93.438854)
        (xy 166.81932 96.513854)
        (xy 162.97572 100.473854)
        (xy 156.80351 100.473854)
        (xy 156.37172 100.042054)
        (xy 152.15532 100.042054)
      )
    )
  )
  (zone (net 6) (net_name "/SDI/VCC_I") (layer "In2.Cu") (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.15) (thermal_bridge_width 0.15))
    (polygon
      (pts
        (xy 189.01932 90.463854)
        (xy 190.01932 90.463854)
        (xy 190.51932 90.963854)
        (xy 190.51932 91.963854)
        (xy 191.01932 92.463854)
        (xy 197.01932 92.463854)
        (xy 198.01932 93.463854)
        (xy 198.01932 94.963854)
        (xy 194.01932 99.463854)
        (xy 189.01932 99.463854)
        (xy 188.51932 98.963854)
        (xy 188.51932 90.963854)
      )
    )
  )
  (zone (net 32) (net_name "/SDI/VCC_O") (layer "In2.Cu") (name "VCC_O") (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.15))
    (min_thickness 0.15) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.15) (thermal_bridge_width 0.15))
    (polygon
      (pts
        (xy 196.01932 113.463854)
        (xy 196.51932 113.963854)
        (xy 196.51932 121.963854)
        (xy 196.01932 122.463854)
        (xy 194.51932 122.463854)
        (xy 194.01932 121.963854)
        (xy 194.01932 120.963854)
        (xy 193.01932 119.963854)
        (xy 188.51932 119.963854)
        (xy 187.01932 118.463854)
        (xy 187.01932 114.963854)
        (xy 188.51932 113.463854)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Paste") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.87017 95.565184)
        (xy 159.87017 96.565184)
        (xy 158.87017 96.565184)
        (xy 158.87017 95.565184)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Paste") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.27007 95.565184)
        (xy 161.27007 96.565184)
        (xy 160.27007 96.565184)
        (xy 160.27007 95.565184)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Paste") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.27007 96.965084)
        (xy 161.27007 97.965084)
        (xy 160.27007 97.965084)
        (xy 160.27007 96.965084)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Paste") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.87017 96.965084)
        (xy 159.87017 97.965084)
        (xy 158.87017 97.965084)
        (xy 158.87017 96.965084)
      )
    )
  )
)
