(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 67)
    (no_connects 0)
    (area 74.405 44.064999 163.545001 132.555001)
    (thickness 1.6)
    (drawings 6)
    (tracks 353)
    (zones 0)
    (modules 24)
    (nets 36)
  )
  (page A4)
  (title_block
    (title Main)
    (date 2017-03-28)
    (rev 1)
    (company "CU Rocket Engineering")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 VBAT)
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(IC1-Pad1)")
  (net 7 "Net-(IC1-Pad15)")
  (net 8 "Net-(IC1-Pad2)")
  (net 9 "Net-(IC1-Pad16)")
  (net 10 "Net-(IC1-Pad3)")
  (net 11 "Net-(IC1-Pad17)")
  (net 12 "Net-(IC1-Pad4)")
  (net 13 "Net-(IC1-Pad18)")
  (net 14 "Net-(IC1-Pad5)")
  (net 15 "Net-(IC1-Pad19)")
  (net 16 "Net-(IC1-Pad21)")
  (net 17 "Net-(IC1-Pad9)")
  (net 18 "Net-(IC1-Pad23)")
  (net 19 "Net-(IC1-Pad10)")
  (net 20 "Net-(IC1-Pad24)")
  (net 21 "Net-(IC1-Pad25)")
  (net 22 "Net-(IC1-Pad12)")
  (net 23 "Net-(IC1-Pad26)")
  (net 24 "Net-(IC1-Pad13)")
  (net 25 "Net-(IC1-Pad27)")
  (net 26 "Net-(IC1-Pad14)")
  (net 27 "Net-(IC1-Pad28)")
  (net 28 "Net-(J3-Pad6)")
  (net 29 "Net-(J3-Pad7)")
  (net 30 "Net-(J4-Pad2)")
  (net 31 "Net-(J5-Pad2)")
  (net 32 "Net-(Q1-Pad3)")
  (net 33 "Net-(Q2-Pad2)")
  (net 34 "Net-(U2-Pad4)")
  (net 35 "Net-(J6-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net VBAT)
    (add_net VCC)
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 58765D06)
    (at 114.3 118.11 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1 -3.56 270) (layer F.SilkS))
    (fp_text value "10 µF" (at 1 3.56 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 58765D06)
    (at 114.3 111.76 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C2 (at 1.25 -2.36 270) (layer F.SilkS))
    (fp_text value "0.1 µF" (at 1.25 2.36 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VBAT))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 58765D06)
    (at 144.78 85.09 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 1.25 -1.86 90) (layer F.SilkS))
    (fp_text value "22 pF" (at 1.25 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 58765D06)
    (at 139.7 85.09 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C4 (at 1.25 -1.86 90) (layer F.SilkS))
    (fp_text value "22 pF" (at 1.25 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_Socket (layer B.Cu) (tedit 586281B5)
    (at 149.86 64.77 90)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference IC1 (at 3.81 2.39 90) (layer B.SilkS))
    (fp_text value AVR (at 3.81 -35.41 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 -33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad15)"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 -30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad16)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(IC1-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 -27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(IC1-Pad17)"))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(IC1-Pad4)"))
    (pad 18 thru_hole oval (at 7.62 -25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(IC1-Pad18)"))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(IC1-Pad5)"))
    (pad 19 thru_hole oval (at 7.62 -22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(IC1-Pad19)"))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 20 thru_hole oval (at 7.62 -20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 21 thru_hole oval (at 7.62 -17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(IC1-Pad21)"))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole oval (at 7.62 -15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(IC1-Pad9)"))
    (pad 23 thru_hole oval (at 7.62 -12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(IC1-Pad23)"))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(IC1-Pad10)"))
    (pad 24 thru_hole oval (at 7.62 -10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(IC1-Pad24)"))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 25 thru_hole oval (at 7.62 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(IC1-Pad25)"))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(IC1-Pad12)"))
    (pad 26 thru_hole oval (at 7.62 -5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(IC1-Pad26)"))
    (pad 13 thru_hole oval (at 0 -30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad13)"))
    (pad 27 thru_hole oval (at 7.62 -2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(IC1-Pad27)"))
    (pad 14 thru_hole oval (at 0 -33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad14)"))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(IC1-Pad28)"))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 58F67F67)
    (at 81.28 57.15 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J1 (at 2.5 5.9 270) (layer F.SilkS))
    (fp_text value CtrlTerm (at 2.5 -6.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(IC1-Pad12)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 58F67F5C)
    (at 81.28 67.31 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J2 (at 2.5 5.9 270) (layer F.SilkS))
    (fp_text value PayloadTerm (at 2.5 -6.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 27 "Net-(IC1-Pad28)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 25 "Net-(IC1-Pad27)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:DB9FC (layer F.Cu) (tedit 587FDE78)
    (at 152.4 106.68 180)
    (descr "Connecteur DB9 femelle couche")
    (tags "CONN DB9")
    (fp_text reference J3 (at 5.46 2.28 180) (layer F.SilkS))
    (fp_text value PanelTerm (at 6.73 -5.08 180) (layer F.Fab))
    (pad "" thru_hole circle (at 18.29 -2.54 180) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -7.11 -2.54 180) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.79 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.46 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(IC1-Pad23)"))
    (pad 4 thru_hole circle (at 8.26 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 "Net-(IC1-Pad24)"))
    (pad 5 thru_hole circle (at 11.05 0 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 "Net-(IC1-Pad25)"))
    (pad 6 thru_hole circle (at 1.4 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad6)"))
    (pad 7 thru_hole circle (at 4.19 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at 6.86 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 9.65 -2.54 180) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (model Connectors.3dshapes/DB9FC.wrl
      (at (xyz 0.2086614173228347 0.05314960629921261 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 58F67F4F)
    (at 81.28 91.44 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J4 (at 2.5 5.9 270) (layer F.SilkS))
    (fp_text value MainTerm (at 2.5 -6.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VBAT))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 "Net-(J4-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 58F67F55)
    (at 81.28 81.28 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J5 (at 2.5 5.9 270) (layer F.SilkS))
    (fp_text value DrogueTerm (at 2.5 -6.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VBAT))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 58F67F6C)
    (at 81.28 46.99 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J6 (at 2.5 5.9 270) (layer F.SilkS))
    (fp_text value IgniterTerm (at 2.5 -6.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VBAT))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 35 "Net-(J6-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 58F67FC6)
    (at 158.75 95.25)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value ProgramHeader (at -2.54 1.27 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(IC1-Pad18)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(IC1-Pad19)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(IC1-Pad17)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(IC1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58F67F7B)
    (at 110.49 48.26 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Accelerometer (at 2.54 6.35 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(IC1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(IC1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(IC1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 58F67FD4)
    (at 161.29 52.07)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Barometer (at -2.54 2.54 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad14)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad15)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Horizontal1_Inline_Narrow_Oval (layer F.Cu) (tedit 58F67F99)
    (at 95.25 99.06 90)
    (descr "TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -1.78 270) (layer F.SilkS))
    (fp_text value MainCtrl (at 1.27 10.03 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.78 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 "Net-(IC1-Pad9)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Horizontal1_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Horizontal1_Inline_Narrow_Oval (layer F.Cu) (tedit 58F67FA2)
    (at 107.95 88.9 270)
    (descr "TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -1.78 450) (layer F.SilkS))
    (fp_text value ArmCtrl (at 1.27 10.03 450) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.78 270) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 33 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Horizontal1_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Horizontal1_Inline_Narrow_Oval (layer F.Cu) (tedit 58F67FA8)
    (at 95.25 83.82 90)
    (descr "TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -1.78 270) (layer F.SilkS))
    (fp_text value DrogueCtrl (at 1.27 10.03 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.78 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 "Net-(IC1-Pad10)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Horizontal1_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 138.43 100.33 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value "10 kΩ" (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad6)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 130.81 90.17 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value "10 kΩ" (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad7)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Horizontal (layer F.Cu) (tedit 58F68E82)
    (at 105.41 119.38 90)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (fp_text reference U1 (at 2.54 -20.58 90) (layer F.SilkS))
    (fp_text value "3.3V Reg" (at 2.54 1.9 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58 90) (layer F.Fab))
    (pad 0 thru_hole oval (at 2.54 -16.66 90) (size 6 6) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 VBAT))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer B.Cu) (tedit 586281B4)
    (at 115.57 104.14)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 2.39) (layer B.SilkS))
    (fp_text value 74LS00 (at 3.81 -17.63) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad6)"))
    (pad 8 thru_hole oval (at 7.62 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(Q2-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(Q2-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad7)"))
    (pad 12 thru_hole oval (at 7.62 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad4)"))
    (pad 13 thru_hole oval (at 7.62 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 139.7 76.2)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.44 -3.525) (layer F.SilkS))
    (fp_text value Crystal (at 2.44 3.525) (layer F.Fab))
    (fp_text user %R (at 2.44 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 58F67F47)
    (at 81.28 101.6 270)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J7 (at 2.5 5.9 270) (layer F.SilkS))
    (fp_text value BatteryTerm (at 2.5 -6.6 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 VBAT))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Horizontal1_Inline_Narrow_Oval (layer F.Cu) (tedit 58F67F8B)
    (at 107.95 104.14 270)
    (descr "TO-92 horizontal, leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 1.27 -1.78 450) (layer F.SilkS))
    (fp_text value IgniterCtrl (at 1.27 10.03 450) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.78 270) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 23 "Net-(IC1-Pad26)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 35 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Horizontal1_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_line (start 73.66 124.46) (end 73.66 43.18) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.1 124.46) (end 73.66 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.1 48.26) (end 165.1 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.1 43.18) (end 165.1 48.26) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.66 43.18) (end 165.1 43.18) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "CU Rocket Engineering\nMain Board\nRevision 1" (at 105.41 73.66) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.71 121.92) (xy 78.74 121.92) (xy 78.74 111.76) (xy 92.71 111.76)
      )
    )
  )
)
