(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 55)
    (zones 0)
    (modules 11)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 /Coin1)
  (net 2 GND)
  (net 3 /Coin2)
  (net 4 +12V)
  (net 5 /Counter1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /Coin1)
    (add_net /Coin2)
    (add_net /Counter1)
    (add_net GND)
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 53 55 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D1 (at 2.54 -2.42 180) (layer F.SilkS))
    (fp_text value "Coin 1 Zener" (at 2.54 2.42 180) (layer F.Fab))
    (fp_text user %R (at 2.78 0 180) (layer F.Fab))
    (fp_text user K (at 0 -2 180) (layer F.Fab))
    (fp_text user K (at 0 -2 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Coin1))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_T-1_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 69 55 180)
    (descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D2 (at 2.54 -2.42 180) (layer F.SilkS))
    (fp_text value "Coin 2 Zener" (at 2.54 2.42 180) (layer F.Fab))
    (fp_text user K (at 0 -2 180) (layer F.SilkS))
    (fp_text user K (at 0 -2 180) (layer F.Fab))
    (fp_text user %R (at 2.78 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Coin2))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C8E72B9)
    (at 65 64)
    (descr "JST XH series connector, B02B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J1 (at 1.25 -3.55) (layer F.SilkS))
    (fp_text value "Power Input" (at 1.25 4.6) (layer F.SilkS))
    (fp_text user %R (at 1.25 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 4 +12V))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B04B-XH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C8E72D0)
    (at 47 46)
    (descr "JST XH series connector, B04B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J2 (at 3.75 -3.55) (layer F.SilkS))
    (fp_text value "Coin Mech 1" (at 3.75 4.6) (layer F.SilkS))
    (fp_text user %R (at 3.75 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 5 /Counter1))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 /Coin1))
    (pad 4 thru_hole oval (at 7.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 +12V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B04B-XH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B04B-XH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C8E72DB)
    (at 62 46)
    (descr "JST XH series connector, B04B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J3 (at 3.75 -3.55) (layer F.SilkS))
    (fp_text value "Coin Mech 2" (at 3.75 4.6) (layer F.SilkS))
    (fp_text user %R (at 3.75 2.7) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 +12V))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 /Coin2))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 5 /Counter1))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B04B-XH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C8E72C0)
    (at 48 64)
    (descr "JST XH series connector, B03B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J4 (at 2.5 -3.55) (layer F.SilkS))
    (fp_text value "KB Enc" (at 2.5 4.6) (layer F.SilkS))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 /Coin1))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 /Coin2))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B03B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C8E72DF)
    (at 78.74 54 270)
    (descr "JST XH series connector, B02B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH side entry")
    (fp_text reference J5 (at 1.25 -3.55 270) (layer F.SilkS))
    (fp_text value Counter (at 1.25 4.6 270) (layer F.SilkS))
    (fp_text user %R (at 1.25 2.7 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 +12V))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 5 /Counter1))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5C8E64F5)
    (at 39 46)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at -7.62 8.89) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5C8E656E)
    (at 39 66)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5C8E65B8)
    (at 78.74 66)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.26 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5C8E65BE)
    (at 79 45.72)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (gr_text "kiall.macinnes.ie/p/coinmech-interface\nv1.0" (at 59 52) (layer B.SilkS))
  (gr_text "Coin Mech\nInterface\nv1.0" (at 39 56 90) (layer F.SilkS))
  (gr_line (start 34 66) (end 34 46) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 71) (end 39 71) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 39 41) (end 79 41) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84 46) (end 84 66) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 79 46) (end 84 46) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 79 66) (end 79 71) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 39 66) (end 34 66) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 39 46) (end 39 41) (angle -90) (layer Edge.Cuts) (width 0.1))
)
