(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 29)
    (no_connects 0)
    (area 64.924999 44.924999 95.075001 175.075001)
    (thickness 1.6)
    (drawings 4)
    (tracks 66)
    (zones 0)
    (modules 5)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.85 0.85)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /H)
  (net 3 /V)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /H)
    (add_net /V)
    (add_net GND)
  )
  (net_class Antenna ""
    (clearance 0.1524)
    (trace_width 1.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class "Signal Trace" ""
    (clearance 0.1524)
    (trace_width 1)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.00mm (layer F.Cu) (tedit 59A5D6CA)
    (at 80 61.65)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference "" (at 0 -1.56) (layer F.SilkS))
    (fp_text value "" (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMA_SMD_Jack_Straight (layer F.Cu) (tedit 58C35474)
    (at 72.5 85 90)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference J1 (at 0 -5 90) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 5 90) (layer F.Fab))
    (fp_text user %R (at 0 -5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 2.38 110) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.85 2.38 70) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.85 -2.38 70) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.85 -2.38 110) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.515 1.749 140) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.515 1.749 40) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.515 -1.749 40) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.515 -1.749 140) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.6 2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.8 180) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.6 2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.6 -2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd circle (at 0 0 180) (size 1.73 1.73) (layers F.Cu F.Paste F.Mask)
      (net 2 /H))
    (pad 2 smd rect (at 0 -2.8 180) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.6 -2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Connectors:SMA_SMD_Jack_Straight (layer F.Cu) (tedit 58C35474)
    (at 87.5 85 90)
    (descr "SMA pcb surface mount jack")
    (tags "SMA SMD Jack Straight")
    (attr smd)
    (fp_text reference J2 (at 0 -5 90) (layer F.SilkS))
    (fp_text value CONN_COAXIAL (at 0 5 90) (layer F.Fab))
    (fp_text user %R (at 0 -5 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 2.38 110) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.85 2.38 70) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.85 -2.38 70) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.85 -2.38 110) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.515 1.749 140) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.515 1.749 40) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.515 -1.749 40) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.515 -1.749 140) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.6 2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.8 180) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.6 2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.6 -2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd circle (at 0 0 180) (size 1.73 1.73) (layers F.Cu F.Paste F.Mask)
      (net 3 /V))
    (pad 2 smd rect (at 0 -2.8 180) (size 1.51 7.11) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.6 -2.38 180) (size 2.35 1.91) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.00mm (layer F.Cu) (tedit 59A5DBD3)
    (at 80 55)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference "" (at 0 -1.56) (layer F.SilkS))
    (fp_text value "" (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 /V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch1.00mm (layer F.Cu) (tedit 59A5DBDA)
    (at 80 56.3)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference "" (at 0 -1.56) (layer F.SilkS))
    (fp_text value "" (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch1.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 95 45) (end 95 175) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65 45) (end 95 45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65 175) (end 65 45) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65 175) (end 95 175) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95 175) (xy 65 175) (xy 65 85) (xy 95 85)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 88) (xy 95 88) (xy 95 175) (xy 65 175)
      )
    )
  )
)
