(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 68)
    (zones 0)
    (modules 13)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.762)
    (user_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(J1-Pad0)")
  (net 6 GNDREF)
  (net 7 "Net-(J4-Pad0)")
  (net 8 "Net-(J4-Pad5)")
  (net 9 "Net-(J4-Pad3)")
  (net 10 "Net-(J4-Pad1)")
  (net 11 "Net-(C3-Pad2)")
  (net 12 "Net-(C3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDREF)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J4-Pad0)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad5)")
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 132.45 130.7465)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 132.52 104.3305)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module New_SMD:C_1808 (layer F.Cu) (tedit 5DCDBDCB)
    (at 109.841 115.2525 180)
    (attr smd)
    (fp_text reference C1 (at -0.014 2.0955) (layer F.SilkS))
    (fp_text value 1200pf (at 0 2.794) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.3 0 180) (size 1.75 2.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 2.3 0 180) (size 1.75 2.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module New_SMD:C_1808 (layer F.Cu) (tedit 5DCDBDCB)
    (at 109.7775 122.809)
    (attr smd)
    (fp_text reference C2 (at 0.0495 -2.3495) (layer F.SilkS))
    (fp_text value 1200pf (at 0 2.794) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.3 0) (size 1.75 2.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -2.3 0) (size 1.75 2.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
  )
  (module Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm (layer F.Cu) (tedit 59FEDEE2)
    (at 103.1875 122.7455 270)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (fp_text reference J1 (at -5.461 6.477 90) (layer F.SilkS))
    (fp_text value DB9_Female_MountingHoles (at -5.54 18.61 90) (layer F.Fab))
    (fp_text user %R (at -5.54 6.5405 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C3-Pad2)"))
    (pad 6 thru_hole circle (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at -18.04 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad0)"))
    (pad 0 thru_hole circle (at 6.96 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad0)"))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:RF_SMA_RightAngle_5-1814400-1 (layer F.Cu) (tedit 5A4BE44C)
    (at 125.5395 104.267)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1814400&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference J2 (at -5.588 -1.3335) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 6.27) (layer F.Fab))
    (fp_text user %R (at 0 -4.48) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
  )
  (module digikey-footprints:RF_SMA_RightAngle_5-1814400-1 (layer F.Cu) (tedit 5A4BE44C)
    (at 110.0455 130.7465 180)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1814400&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference J3 (at -4.5085 0.127) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 6.27) (layer F.Fab))
    (fp_text user %R (at 0 -4.48) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm (layer F.Cu) (tedit 59FEDEE2)
    (at 137.541 111.9505 90)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (fp_text reference J4 (at -5.7785 5.969 90) (layer F.SilkS))
    (fp_text value DB9_Male_MountingHoles (at -5.54 18.61 90) (layer F.Fab))
    (fp_text user %R (at -5.715 5.969 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 6.96 1.42 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad0)"))
    (pad 0 thru_hole circle (at -18.04 1.42 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad0)"))
    (pad 9 thru_hole circle (at -9.695 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -6.925 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -4.155 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.385 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -11.08 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad5)"))
    (pad 4 thru_hole circle (at -8.31 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -5.54 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at -2.77 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ADCH-80A:ADCH-80A (layer F.Cu) (tedit 5DCD83C8)
    (at 119.634 121.539 180)
    (fp_text reference L1 (at -5.715 -0.0635) (layer F.SilkS))
    (fp_text value RFChoke (at 0 5.588) (layer F.Fab))
    (pad 6 smd rect (at -2.54 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (pad 5 smd rect (at 0 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.54 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 2.54 2.54 180) (size 1.6764 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0 2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.54 2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
  )
  (module ADCH-80A:ADCH-80A (layer F.Cu) (tedit 5DCD83C8)
    (at 119.4435 130.175 180)
    (fp_text reference L2 (at -6.223 0) (layer F.SilkS))
    (fp_text value RFChoke (at 0 5.588) (layer F.Fab))
    (pad 1 smd rect (at -2.54 2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 2.54 2.54 180) (size 1.6764 2.54) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 2.54 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.54 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J4-Pad1)"))
  )
  (module New_SMD:C_1808 (layer F.Cu) (tedit 5DCDBDCB)
    (at 109.714 111.0615 180)
    (attr smd)
    (fp_text reference C3 (at 0.014 2.54) (layer F.SilkS))
    (fp_text value 1200pf (at 0 2.794) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.3 0 180) (size 1.75 2.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -2.3 0 180) (size 1.75 2.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C3-Pad1)"))
  )
  (module digikey-footprints:RF_SMA_RightAngle_5-1814400-1 (layer F.Cu) (tedit 5A4BE44C)
    (at 109.855 104.2035)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1814400&DocType=Customer+Drawing&DocLang=English)
    (fp_text reference J5 (at 5.0165 -1.143) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 6.27) (layer F.Fab))
    (fp_text user %R (at 0 -4.48) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 GNDREF))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 12 "Net-(C3-Pad1)"))
  )
  (module ADCH-80A:ADCH-80A (layer F.Cu) (tedit 5DCD83C8)
    (at 119.761 113.03 180)
    (fp_text reference L3 (at -5.588 -0.0635) (layer F.SilkS))
    (fp_text value RFChoke (at 0 5.588) (layer F.Fab))
    (pad 1 smd rect (at -2.54 2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 2.54 2.54 180) (size 1.6764 2.54) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C3-Pad2)"))
    (pad 4 smd rect (at 2.54 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.54 -2.54 180) (size 1.651 2.54) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J4-Pad5)"))
  )
  (gr_text "Wire 2" (at 132.6515 101.219) (layer B.SilkS))
  (gr_text "Wire 3" (at 116.586 101.1555) (layer B.SilkS))
  (gr_text "Wire 1" (at 103.1875 134.0485) (layer B.SilkS))
  (gr_text "Male Input" (at 95.4405 117.5385 270) (layer B.SilkS))
  (gr_text "Female Output" (at 145.0975 117.602 270) (layer B.SilkS))
  (gr_text "Wire 3" (at 116.586 101.092) (layer F.SilkS))
  (gr_text "Wire 2" (at 132.588 101.219) (layer F.SilkS))
  (gr_text "Wire 1" (at 103.251 134.112) (layer F.SilkS))
  (gr_text "Female Output" (at 145.161 117.5385 90) (layer F.SilkS))
  (gr_text "Male Input" (at 95.3135 117.5385 90) (layer F.SilkS))
  (gr_text "FRIB PM_Duplexer V01" (at 102.4255 125.1585) (layer B.SilkS))
  (gr_line (start 147.8915 135.255) (end 92.6465 135.255) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.6465 99.822) (end 92.6465 135.255) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.955 99.822) (end 92.6465 99.822) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.8915 135.255) (end 147.955 99.822) (layer Edge.Cuts) (width 0.05))
  (zone (net 6) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.1385 99.3775) (xy 148.717 99.3775) (xy 148.6535 136.017) (xy 92.0115 135.9535) (xy 92.1385 135.9535)
      )
    )
  )
  (zone (net 6) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.075 99.314) (xy 149.0345 99.187) (xy 149.0345 136.271) (xy 92.075 136.2075)
      )
    )
  )
)
