<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="14.605" y1="60.325" x2="0" y2="60.325" width="0.1524" layer="20"/>
<wire x1="0" y1="60.325" x2="0" y2="43.688" width="0.1524" layer="20"/>
<wire x1="0" y1="36.322" x2="0" y2="30.226" width="0.1524" layer="20"/>
<wire x1="0" y1="28.194" x2="0" y2="12.2428" width="0.1524" layer="20"/>
<wire x1="0" y1="10.16" x2="0" y2="5.08" width="0.1524" layer="20"/>
<wire x1="14.605" y1="60.325" x2="14.605" y2="18.542" width="0.1524" layer="20"/>
<wire x1="27.305" y1="18.542" x2="27.305" y2="60.325" width="0.1524" layer="20"/>
<wire x1="27.305" y1="60.325" x2="36.83" y2="60.325" width="0.1524" layer="20"/>
<wire x1="36.83" y1="60.325" x2="36.83" y2="33.02" width="0.1524" layer="20"/>
<wire x1="36.83" y1="18.796" x2="36.83" y2="5.08" width="0.1524" layer="20"/>
<wire x1="17.907" y1="15.24" x2="24.003" y2="15.24" width="0.1524" layer="20"/>
<wire x1="24.003" y1="15.24" x2="27.305" y2="18.542" width="0.1524" layer="20"/>
<wire x1="14.605" y1="18.542" x2="17.907" y2="15.24" width="0.1524" layer="20"/>
<wire x1="5.08" y1="0" x2="31.75" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="0.1524" layer="20"/>
<wire x1="31.75" y1="0" x2="36.83" y2="5.08" width="0.1524" layer="20"/>
<hole x="7.62" y="43.815" drill="3.175"/>
<hole x="31.75" y="22.225" drill="3.175"/>
<wire x1="34.61740625" y1="18.796" x2="34.61740625" y2="33.02" width="0.1524" layer="20"/>
<wire x1="34.61740625" y1="18.796" x2="36.83" y2="18.796" width="0.1524" layer="20"/>
<wire x1="34.61740625" y1="33.02" x2="36.83" y2="33.02" width="0.1524" layer="20"/>
<wire x1="0" y1="43.688" x2="3.4798" y2="43.688" width="0.1524" layer="20"/>
<wire x1="3.4798" y1="43.688" x2="3.4798" y2="36.322" width="0.1524" layer="20"/>
<wire x1="3.4798" y1="36.322" x2="0" y2="36.322" width="0.1524" layer="20"/>
<wire x1="-5.23875" y1="29.21" x2="-5.23875" y2="11.176" width="0.1524" layer="20"/>
<wire x1="-5.23875" y1="11.176" x2="-4.22275" y2="10.16" width="0.1524" layer="20"/>
<wire x1="-4.22275" y1="10.16" x2="0" y2="10.16" width="0.1524" layer="20"/>
<wire x1="-5.23875" y1="29.21" x2="-4.22275" y2="30.226" width="0.1524" layer="20"/>
<wire x1="-4.22275" y1="30.226" x2="0" y2="30.226" width="0.1524" layer="20"/>
<wire x1="-3.2385" y1="28.194" x2="-3.2385" y2="12.2428" width="0.1524" layer="20"/>
<wire x1="-3.2385" y1="12.2428" x2="0" y2="12.2428" width="0.1524" layer="20"/>
<wire x1="-3.2385" y1="28.194" x2="0" y2="28.194" width="0.1524" layer="20"/>
<hole x="0" y="12.192" drill="1.016"/>
<hole x="0" y="10.16" drill="1.016"/>
<hole x="0" y="30.1625" drill="0.889"/>
<hole x="0" y="28.2575" drill="0.889"/>
<text>V2</text>
</plain>
<libraries>
<library name="SwitchTesterLib">
<packages>
<package name="RIGHTANGLEPOGO">
</package>
<package name="104238-0210">
</package>
</packages>
</library>
<library name="Eagle_WR-TBL Spring Clamp (rev21a)">
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Terminal Blocks - WR-TBL Spring Clamp &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-02-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="691412320005">
<description>&lt;b&gt;WR-TBL Serie 4123 - 3.81 mm Screwless 45° Entry 
&lt;br&gt;&lt;/b&gt;Max Height = 13.2mm , Pitch 3.81mm , 5pins</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SwitchTesterLib" package="RIGHTANGLEPOGO" value="LONG_POGO">
<attribute name="NAME"/>
</element>
<element name="J2" library="SwitchTesterLib" package="RIGHTANGLEPOGO" value="LONG_POGO">
<attribute name="NAME"/>
</element>
<element name="J3" library="SwitchTesterLib" package="RIGHTANGLEPOGO" value="LONG_POGO">
<attribute name="NAME"/>
</element>
<element name="J4" library="SwitchTesterLib" package="RIGHTANGLEPOGO" value="LONG_POGO">
<attribute name="NAME"/>
</element>
<element name="J5" library="SwitchTesterLib" package="104238-0210" value="104238-0210">
<attribute name="NAME"/>
</element>
<element name="X1" library="Eagle_WR-TBL Spring Clamp (rev21a)" package="691412320005" value=" 691412320005 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691412320005.pdf"/>
<attribute name="IR-UL" value="4A"/>
<attribute name="IR-VDE" value="4A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 691412320005 "/>
<attribute name="PINS" value=" 5 "/>
<attribute name="PITCH" value="3.81mm"/>
<attribute name="TYPE" value="45°"/>
<attribute name="WIRE" value="16 to 30 (AWG) 1.31 to 0.05 (mm²)"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="450V (AC)"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J2" pad="P$1"/>
<contactref element="J3" pad="P$1"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="J5" pad="B2"/>
<contactref element="J5" pad="B1"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="5"/>
<contactref element="J5" pad="A2"/>
<contactref element="J5" pad="A1"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="P$1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="P$1"/>
<contactref element="X1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
