(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 0)
    (area 92.942857 68.125 123.133334 90.735)
    (thickness 1.6)
    (drawings 35)
    (tracks 80)
    (zones 0)
    (modules 32)
    (nets 10)
  )
  (page USLetter)
  (title_block
    (title "Si5351A PicoBoB")
    (date 2017-06-24)
    (rev A)
    (company Etherkit)
    (comment 4 "Creative Commons License CC-BY-SA")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.2 0.2)
    (pad_drill 0.15)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad3)")
  (net 7 "Net-(J3-Pad5)")
  (net 8 "Net-(U1-Pad3)")
  (net 9 "Net-(U2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.4)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U2-Pad3)")
  )
  (net_class 50ohm ""
    (clearance 0.2)
    (trace_width 0.82)
    (via_dia 0.4)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 594EC6B8)
    (at 102.5 72.5)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED822)
    (at 111.6 78.1)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED81F)
    (at 111.5 77.6)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED815)
    (at 111.1 77.2)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED80F)
    (at 110.8 76.8)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED80B)
    (at 110.8 76.2)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED807)
    (at 110.8 75.6)
    (clearance 0.1)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED7FE)
    (at 109.2 77.3)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED7EF)
    (at 109.2 75.6)
    (clearance 0.01)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED7F5)
    (at 109.2 76.2)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED7FA)
    (at 109.2 76.8)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED803)
    (at 109.3 77.8)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED819)
    (at 109.7 78.3)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED827)
    (at 110.1 78.7)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED82B)
    (at 110.5 79.2)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED82F)
    (at 110.5 79.8)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED836)
    (at 110.5 80.4)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED83E)
    (at 110.8 81.1)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED85D)
    (at 111 81.6)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED845)
    (at 111.4 81.2)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594EC8F2)
    (at 114.6 81.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -1.9 0 360) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594EC8E8)
    (at 107.7 77.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.3) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 594EC62F)
    (at 102 77.5)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 9.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module EtherkitKicadLibrary:SMA-ENDLAUNCH (layer F.Cu) (tedit 594EC5CC)
    (at 110 75.2)
    (fp_text reference J2 (at 0 1) (layer F.SilkS))
    (fp_text value SMA-END (at 0.2 -6.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 -2.54) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 3 -2.54) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3 -2.54) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3 -0.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -4.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -3.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -3.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -2.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -1.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -1.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -0.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -4.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -3.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -3.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -2.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -1.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -1.5) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 smd rect (at 3 -2.54) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3 -2.54) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 594EC636)
    (at 118.1 73.5)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 15.03) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 594EC8FC)
    (at 109.2 85.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 594EC907)
    (at 106.2 85.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:ASTX-H11-25.000MHZ-T (layer F.Cu) (tedit 594EC5EA)
    (at 108.1 81)
    (fp_text reference U1 (at 0 -2.2) (layer F.SilkS))
    (fp_text value ASTX-H11-25.000MHZ-T (at 0 -2.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.15 0.95) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
    (pad 2 smd rect (at 1.15 0.95) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.15 -0.95) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -1.15 -0.95) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V))
  )
  (module EtherkitKicadLibrary:MSOP-10 (layer F.Cu) (tedit 594EC4C4)
    (at 112.1 81.9)
    (descr "Mini SOP10 10pins pitch 0.5mm")
    (clearance 0.1)
    (attr smd)
    (fp_text reference U2 (at 0 -3.6) (layer F.SilkS))
    (fp_text value SI5351A (at -2.2 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V) (solder_paste_margin_ratio -0.1))
    (pad 2 smd rect (at -0.5 2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad3)") (solder_paste_margin_ratio -0.1))
    (pad 3 smd rect (at 0 2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U2-Pad3)") (solder_paste_margin_ratio -0.1))
    (pad 4 smd rect (at 0.5 2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)") (solder_paste_margin_ratio -0.1))
    (pad 5 smd rect (at 1 2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)") (solder_paste_margin_ratio -0.1))
    (pad 6 smd rect (at 1.016 -2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad5)") (solder_paste_margin_ratio -0.1))
    (pad 7 smd rect (at 0.508 -2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V) (solder_paste_margin_ratio -0.1))
    (pad 8 smd rect (at 0 -2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.1))
    (pad 9 smd rect (at -0.508 -2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad3)") (solder_paste_margin_ratio -0.1))
    (pad 10 smd rect (at -1.016 -2.35) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)") (solder_paste_margin_ratio -0.1))
    (model smd\MSOP_10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.35 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:VIA (layer F.Cu) (tedit 594ED841)
    (at 111.8 80.7)
    (clearance 0.2)
    (fp_text reference VIA (at 0 1.2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 1.2) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.2 0.2) (drill 0.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.05) (zone_connect 2))
  )
  (module EtherkitKicadLibrary:EtherkitLogoSmall (layer F.Cu) (tedit 0)
    (at 114.7 87.1)
    (fp_text reference Ref** (at 0 3.25) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -2.95) (layer F.SilkS) hide)
  )
  (module EtherkitKicadLibrary:OSHWLogo4mm (layer B.Cu) (tedit 0)
    (at 114.5 82.5 180)
    (fp_text reference G*** (at 0 -2.35966 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 2.35966 180) (layer B.SilkS) hide)
  )
  (gr_text Corr. (at 114.9 85.1) (layer B.SilkS))
  (gr_text "Creative Commons License CC-BY-SA" (at 110 89) (layer B.SilkS))
  (gr_text "etherkit.com 2017" (at 105.1 88.8) (layer F.SilkS))
  (gr_text "Rev A" (at 105.1 76.2) (layer F.Cu))
  (gr_text "Si5351A PicoBoB" (at 100.9 87.5) (layer F.SilkS))
  (gr_text SDA (at 104.4 82.6) (layer F.SilkS))
  (gr_text SCL (at 104.4 80) (layer F.SilkS))
  (gr_text +3.3V (at 104.6 77.5) (layer F.SilkS))
  (gr_text CLK0 (at 115.4 73.6) (layer F.SilkS))
  (gr_text CLK1 (at 115.4 78.7) (layer F.SilkS))
  (gr_text CLK2 (at 115.4 83.8) (layer F.SilkS))
  (gr_arc (start 102 88) (end 102 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118 88) (end 120 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118 72) (end 118 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102 72) (end 100 72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 88) (end 100 72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118 90) (end 102 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120 72) (end 120 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 70) (end 118 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106 79.2) (xy 110.2 79.2) (xy 110.2 82.8) (xy 106 82.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing chamfer))
    (polygon
      (pts
        (xy 101 71) (xy 119 71) (xy 119 89) (xy 101 89)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing chamfer))
    (polygon
      (pts
        (xy 101 70.999925) (xy 119 70.999925) (xy 119 88.999925) (xy 101 88.999925)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.986128 79.2) (xy 110.186128 79.2) (xy 110.186128 82.8) (xy 105.986128 82.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.SilkS) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing chamfer))
    (polygon
      (pts
        (xy 104 85.7) (xy 116.1 85.7) (xy 116.1 88.3) (xy 104 88.3)
      )
    )
  )
)
