(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.10.1)
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 794)
    (zones 0)
    (modules 90)
    (nets 81)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 152.908 89.662)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C9-Pad1)")
  (net 2 "Net-(C9-Pad2)")
  (net 3 "Net-(C13-Pad1)")
  (net 4 "Net-(C13-Pad2)")
  (net 5 "Net-(C10-Pad2)")
  (net 6 +3V3)
  (net 7 GND)
  (net 8 "Net-(C14-Pad1)")
  (net 9 /SCL)
  (net 10 /PG9616_RESET)
  (net 11 "Net-(J4-Pad12)")
  (net 12 "Net-(C8-Pad1)")
  (net 13 /SDA)
  (net 14 "Net-(U10-Pad1)")
  (net 15 "Net-(U10-Pad2)")
  (net 16 "Net-(U10-Pad3)")
  (net 17 "Net-(U10-Pad4)")
  (net 18 "Net-(C21-Pad1)")
  (net 19 +5V)
  (net 20 /JTMS)
  (net 21 /JTCK)
  (net 22 /JTDO)
  (net 23 /JNTRST)
  (net 24 /JTDI)
  (net 25 +12V)
  (net 26 "Net-(R15-Pad1)")
  (net 27 "Net-(C21-Pad2)")
  (net 28 /+3.3VA)
  (net 29 "Net-(Q2-Pad2)")
  (net 30 "Net-(R1-Pad2)")
  (net 31 "Net-(Q2-Pad1)")
  (net 32 /COLD_JUNC)
  (net 33 "Net-(U1-Pad1)")
  (net 34 "Net-(C3-Pad1)")
  (net 35 "Net-(C2-Pad1)")
  (net 36 /OIL_TEMP_IN)
  (net 37 "Net-(Q1-Pad1)")
  (net 38 /TACH)
  (net 39 "Net-(D1-Pad3)")
  (net 40 /THERMOCOUPLE_IN+)
  (net 41 /THERMOCOUPLE_IN-)
  (net 42 /TACH_IN)
  (net 43 "Net-(C7-Pad1)")
  (net 44 "Net-(C7-Pad2)")
  (net 45 /THERMOCOUPLE)
  (net 46 "Net-(R17-Pad2)")
  (net 47 /-3.3VA)
  (net 48 "Net-(R18-Pad1)")
  (net 49 /OIL_TEMP)
  (net 50 "Net-(R7-Pad1)")
  (net 51 "Net-(R6-Pad1)")
  (net 52 /STEPPER4)
  (net 53 /STEPPER3)
  (net 54 /STEPPER2)
  (net 55 /STEPPER1)
  (net 56 "Net-(C31-Pad1)")
  (net 57 "Net-(C31-Pad2)")
  (net 58 "Net-(C32-Pad1)")
  (net 59 "Net-(U6-Pad46)")
  (net 60 "Net-(U6-Pad45)")
  (net 61 /UART_RX)
  (net 62 /UART_TX)
  (net 63 "Net-(U6-Pad41)")
  (net 64 "Net-(U6-Pad33)")
  (net 65 "Net-(U6-Pad19)")
  (net 66 "Net-(U6-Pad18)")
  (net 67 "Net-(U6-Pad16)")
  (net 68 "Net-(U6-Pad15)")
  (net 69 "Net-(U6-Pad14)")
  (net 70 "Net-(U6-Pad10)")
  (net 71 /NRST)
  (net 72 "Net-(C17-Pad1)")
  (net 73 "Net-(C16-Pad1)")
  (net 74 "Net-(U6-Pad4)")
  (net 75 "Net-(U6-Pad3)")
  (net 76 "Net-(U6-Pad2)")
  (net 77 /STEPPER_EN)
  (net 78 "Net-(U6-Pad28)")
  (net 79 "Net-(U6-Pad27)")
  (net 80 "Net-(U6-Pad26)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /+3.3VA)
    (add_net /-3.3VA)
    (add_net /COLD_JUNC)
    (add_net /JNTRST)
    (add_net /JTCK)
    (add_net /JTDI)
    (add_net /JTDO)
    (add_net /JTMS)
    (add_net /NRST)
    (add_net /OIL_TEMP)
    (add_net /OIL_TEMP_IN)
    (add_net /PG9616_RESET)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /STEPPER1)
    (add_net /STEPPER2)
    (add_net /STEPPER3)
    (add_net /STEPPER4)
    (add_net /STEPPER_EN)
    (add_net /TACH)
    (add_net /TACH_IN)
    (add_net /THERMOCOUPLE)
    (add_net /THERMOCOUPLE_IN+)
    (add_net /THERMOCOUPLE_IN-)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net GND)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C31-Pad2)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U10-Pad1)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad3)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U6-Pad10)")
    (add_net "Net-(U6-Pad14)")
    (add_net "Net-(U6-Pad15)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U6-Pad18)")
    (add_net "Net-(U6-Pad19)")
    (add_net "Net-(U6-Pad2)")
    (add_net "Net-(U6-Pad26)")
    (add_net "Net-(U6-Pad27)")
    (add_net "Net-(U6-Pad28)")
    (add_net "Net-(U6-Pad3)")
    (add_net "Net-(U6-Pad33)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U6-Pad41)")
    (add_net "Net-(U6-Pad45)")
    (add_net "Net-(U6-Pad46)")
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 163.068 105.283)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C39 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1.0/10 (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:mountinghole-1.5mm (layer F.Cu) (tedit 5E6ADB29)
    (at 176.149 115.443)
    (fp_text reference J6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu F.Mask)
      (net 25 +12V))
  )
  (module footprints:mountinghole-1.5mm (layer F.Cu) (tedit 5E6ADB25)
    (at 172.593 115.443)
    (fp_text reference J7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu F.Mask)
      (net 7 GND))
  )
  (module footprints:mountinghole-1.5mm (layer F.Cu) (tedit 5E6ADAF5)
    (at 146.939 115.443)
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu F.Mask)
      (net 36 /OIL_TEMP_IN))
  )
  (module footprints:mountinghole-1.5mm (layer F.Cu) (tedit 5E6ADAF9)
    (at 153.924 115.443)
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu F.Mask)
      (net 42 /TACH_IN))
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 168.966907 109.394078 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C27 (at -3.429 2.921 270) (layer B.SilkS))
    (fp_text value 22/10 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:WSON-12-1EP_3x2mm_Pitch0.5mm_ThermalVias (layer B.Cu) (tedit 5E697D21)
    (at 132.334 78.867 90)
    (descr "WSON-12 http://www.ti.com/lit/ds/symlink/lm27762.pdf")
    (tags WSON-12)
    (attr smd)
    (fp_text reference U7 (at 3.302 4.191 90) (layer B.SilkS))
    (fp_text value LM27762 (at 0 -2.921 90) (layer B.Fab))
    (fp_text user %R (at 0 0.25) (layer B.Fab))
    (pad 13 smd rect (at 0 0.685 90) (size 0.95 1.17) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 13 smd rect (at 0 -0.685 90) (size 0.95 1.17) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 13 smd rect (at 0 -0.88 90) (size 1 0.88) (layers B.Cu)
      (net 7 GND))
    (pad 13 smd rect (at 0 0 90) (size 1 0.89) (layers B.Cu)
      (net 7 GND))
    (pad 13 smd rect (at 0 0.88 90) (size 1 0.88) (layers B.Cu)
      (net 7 GND))
    (pad 13 smd rect (at 0 0 90) (size 1 0.89) (layers F.Cu)
      (net 7 GND))
    (pad 13 smd rect (at 0 -0.88 90) (size 1 0.88) (layers F.Cu)
      (net 7 GND))
    (pad 13 smd rect (at 0 0.88 90) (size 1 0.88) (layers F.Cu)
      (net 7 GND))
    (pad 13 thru_hole circle (at 0 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu B.Mask)
      (net 7 GND))
    (pad 13 thru_hole circle (at 0 1) (size 0.6 0.6) (drill 0.3) (layers *.Cu B.Mask)
      (net 7 GND))
    (pad 13 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu B.Mask)
      (net 7 GND))
    (pad 12 smd rect (at 0.95 1.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (pad 11 smd rect (at 0.95 0.75 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 10 smd rect (at 0.95 0.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C31-Pad1)"))
    (pad 9 smd rect (at 0.95 -0.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C31-Pad2)"))
    (pad 8 smd rect (at 0.95 -0.75 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (pad 7 smd rect (at 0.95 -1.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R18-Pad1)"))
    (pad 6 smd rect (at -0.95 -1.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 47 /-3.3VA))
    (pad 5 smd rect (at -0.95 -0.75 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C32-Pad1)"))
    (pad 4 smd rect (at -0.95 -0.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 3 smd rect (at -0.95 0.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (pad 2 smd rect (at -0.95 0.75 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R17-Pad2)"))
    (pad 1 smd rect (at -0.95 1.25 90) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Housings_SON.3dshapes/WSON-12-1EP_3x2mm_Pitch0.5mm_ThermalVias.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 135.89 94.615 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 1.651 -2.159 180) (layer B.SilkS))
    (fp_text value 0.1/10 (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm locked (layer F.Cu) (tedit 5E698A6F)
    (at 173.607 89.362)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm locked (layer F.Cu) (tedit 5E698A6B)
    (at 133.548 89.362)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 163.068 112.9016)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at -2.667 0) (layer F.SilkS))
    (fp_text value 1.0/10 (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 163.068 108.2054 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 2.667 0.127 180) (layer F.SilkS))
    (fp_text value 2.2/10 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C14-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 163.068 114.427 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 2.159 0 180) (layer F.SilkS))
    (fp_text value 1.0/10 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 163.068 106.68 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 2.286 0 180) (layer F.SilkS))
    (fp_text value 2.2/10 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Bourns_3224J (layer B.Cu) (tedit 58826B0B)
    (at 149.606 107.442 180)
    (descr "Spindle Trimmer Potentiometer, Bourns 3224J, https://www.bourns.com/pdfs/3224.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3224J")
    (attr smd)
    (fp_text reference RV1 (at 2.032 3.429) (layer B.SilkS))
    (fp_text value 100k (at 0 -3.65 180) (layer B.Fab))
    (pad 3 smd rect (at 2 -1.15 180) (size 2 1.3) (layers B.Cu B.Mask)
      (net 30 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -2 0 180) (size 2 2) (layers B.Cu B.Mask)
      (net 30 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at 2 1.15 180) (size 2 1.3) (layers B.Cu B.Mask)
      (net 28 /+3.3VA))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3224J.wrl
      (offset (xyz 0.7619999885559082 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 131.445 104.267)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at -2.54 0 -90) (layer B.SilkS))
    (fp_text value BAS40-04 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 133.604 76.073 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C31 (at -0.254 1.397 180) (layer B.SilkS))
    (fp_text value 1.0/10 (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C31-Pad2)"))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C31-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 135.636 78.867 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C36 (at 0 -1.27 270) (layer B.SilkS))
    (fp_text value 10/10 (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 129.794 79.121 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C37 (at 0 1.27 270) (layer B.SilkS))
    (fp_text value 10/10 (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 47 /-3.3VA))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 131.318 81.915 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value 4.7/10 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 133.858 81.788 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C38 (at -2.54 -0.254 -90) (layer B.SilkS))
    (fp_text value 10/10 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 176.332907 104.568078 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D5 (at 4.953 -0.381 270) (layer B.SilkS))
    (fp_text value B340A-13-F (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 2.5 270) (layer B.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 138.303 92.837 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 1.397 180) (layer B.SilkS))
    (fp_text value 0.01/10 (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 45 /THERMOCOUPLE))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 163.068 111.3762)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at -2.667 0) (layer F.SilkS))
    (fp_text value 0.022/50 (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 131.318 101.219 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -2.667 90) (layer B.SilkS))
    (fp_text value 0.01/25 (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 135.763 96.901 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 2.032 0 270) (layer B.SilkS))
    (fp_text value 0.1/16 (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 47 /-3.3VA))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 146.177 101.219 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 2.032 0 90) (layer B.SilkS))
    (fp_text value 0.01/10 (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 49 /OIL_TEMP))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 141.097 106.299)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -1.397 -1.016 -180) (layer B.SilkS))
    (fp_text value 0.1/16 (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 135.509 101.219 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 2.667 90) (layer B.SilkS))
    (fp_text value 0.01u/25 (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 173.736 74.93)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 2.54 -0.127) (layer F.SilkS))
    (fp_text value 18p (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C16-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 173.736 68.961)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 2.54 0) (layer F.SilkS))
    (fp_text value 18p (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 168.204907 98.726078 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at -0.127 -1.27 90) (layer B.SilkS))
    (fp_text value 0.1/10 (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 173.736 67.564)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at 2.54 0) (layer F.SilkS))
    (fp_text value 0.1/10 (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 71 /NRST))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 173.736 76.327)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 2.54 0) (layer F.SilkS))
    (fp_text value 0.1/10 (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 168.204907 94.662078 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C23 (at 0.127 1.397 270) (layer B.SilkS))
    (fp_text value 0.1/10 (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 164.719 68.961)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C24 (at 2.667 -0.127) (layer B.SilkS))
    (fp_text value 0.1/10 (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 160.782 73.914 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C26 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 0.1/10 (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 169.926 77.216 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C28 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value 0.1/10 (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 173.736 66.167)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C30 (at 2.54 0) (layer F.SilkS))
    (fp_text value 0.1/10 (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 /+3.3VA))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 161.671 66.04)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C33 (at 0.127 1.397 -180) (layer F.SilkS))
    (fp_text value 0.1/25 (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 140.208 111.76)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 2.159 0 180) (layer B.SilkS))
    (fp_text value 0.1/16 (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 170.490907 108.886078 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at -2.921 3.175 270) (layer B.SilkS))
    (fp_text value 0.1/50 (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 25 +12V))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 176.078907 111.299078 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0.127 -1.524) (layer B.SilkS))
    (fp_text value 0.47/35 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C21-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 167.061907 109.394078 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C29 (at 3.175 0.762 270) (layer B.SilkS))
    (fp_text value 22/10 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 172.649907 94.662078 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 10/10 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 172.649907 98.726078 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 10/10 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 156.337 67.31 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C34 (at 0 -4.064 90) (layer B.SilkS))
    (fp_text value 1.0/10 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 158.623 67.31 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C35 (at 0 -3.175 270) (layer B.SilkS))
    (fp_text value 10/10 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 176.149 111.149 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10/50 (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 +12V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-2_P5.08mm (layer B.Cu) (tedit 59FF03AB)
    (at 136.017 113.284 180)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (fp_text reference J1 (at 6.477 4.699 180) (layer B.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.54 -5.08 180) (layer B.Fab))
    (fp_text user %R (at 2.54 0 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 40 /THERMOCOUPLE_IN+))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 41 /THERMOCOUPLE_IN-))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_TXC_7M-4pin_3.2x2.5mm (layer F.Cu) (tedit 58CD2E9D)
    (at 174.371 71.882 270)
    (descr "SMD Crystal TXC 7M http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0.127 -2.794 180) (layer F.SilkS))
    (fp_text value 16MHz (at 0 2.45 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at -1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.1 -0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C16-Pad1)"))
    (pad 1 smd rect (at -1.1 0.85 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_TXC_7M-4pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 167.005 71.12 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U6 (at -4.318 -4.699 180) (layer F.SilkS))
    (fp_text value STM32F103CBTx (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U6-Pad46)"))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U6-Pad45)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 /UART_RX))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 /UART_TX))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U6-Pad41)"))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /JNTRST))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 /JTDO))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 /JTDI))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /JTCK))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 /JTMS))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U6-Pad33)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 /STEPPER1))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 /STEPPER2))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 /STEPPER3))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /STEPPER4))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U6-Pad28)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U6-Pad27)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U6-Pad26)"))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 /STEPPER_EN))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /SDA))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCL))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /PG9616_RESET))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U6-Pad19)"))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U6-Pad18)"))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /TACH))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U6-Pad16)"))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U6-Pad15)"))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U6-Pad14)"))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /COLD_JUNC))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 /THERMOCOUPLE))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 /OIL_TEMP))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U6-Pad10)"))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /+3.3VA))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 /NRST))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C17-Pad1)"))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C16-Pad1)"))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U6-Pad4)"))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U6-Pad3)"))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U6-Pad2)"))
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 133.223 96.901 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -3.175 90) (layer B.SilkS))
    (fp_text value LTC2053 (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 8 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 7 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (pad 6 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(C7-Pad2)"))
    (pad 5 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 4 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 47 /-3.3VA))
    (pad 3 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R7-Pad1)"))
    (pad 1 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 47 /-3.3VA))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 156.591 68.072)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U8 (at -5.461 -1.905) (layer F.SilkS))
    (fp_text value 74ABT126 (at 0 3.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V))
    (pad 13 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 /STEPPER_EN))
    (pad 12 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 /STEPPER1))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U10-Pad1)"))
    (pad 10 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 /STEPPER_EN))
    (pad 9 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 /STEPPER2))
    (pad 8 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U10-Pad2)"))
    (pad 7 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U10-Pad3)"))
    (pad 5 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 /STEPPER3))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 /STEPPER_EN))
    (pad 3 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U10-Pad4)"))
    (pad 2 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 /STEPPER4))
    (pad 1 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 /STEPPER_EN))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 172.466 80.137)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at -2.54 0) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SDA))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 140.462 107.823 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 1.905 -0.127 270) (layer B.SilkS))
    (fp_text value 22k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 141.859 107.823 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -1.905 0.127 90) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 158.198422 106.44618 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.397 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 154.642422 104.41418 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 1.905 -0.127 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 38 /TACH))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 132.715 101.219 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 2.667 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 134.112 101.219 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -2.667 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 144.907 101.219 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 2.032 0 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 /OIL_TEMP))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 /OIL_TEMP_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 136.271 92.837 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0.889 1.397 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 131.191 76.327 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R20 (at -1.651 0.508 180) (layer B.SilkS))
    (fp_text value 73.2k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R18-Pad1)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 133.096 83.439)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at -0.889 1.27 -180) (layer B.SilkS))
    (fp_text value 73.2k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 129.794 76.327 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 0.254 -1.397 -90) (layer B.SilkS))
    (fp_text value 124k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 47 /-3.3VA))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 134.874 83.439 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at -0.254 -1.27) (layer B.SilkS))
    (fp_text value 127k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 168.077907 111.807078)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 0.508 1.27) (layer B.SilkS))
    (fp_text value 8.45k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R15-Pad1)"))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 170.109907 111.807078)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 1.524 1.27) (layer B.SilkS))
    (fp_text value 1.54k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 172.466 81.661)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at -2.54 0) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 /SCL))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E0A804)
    (at 163.068 109.7908)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at -2.667 0) (layer F.SilkS))
    (fp_text value 634k (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad12)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 138.557 94.615 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 2.413 -0.127 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 /THERMOCOUPLE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 137.16 94.615 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at -1.905 0 90) (layer B.SilkS))
    (fp_text value 151k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 58E0A804)
    (at 145.092 104.394 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.35 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 158.198422 108.85918 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference TH1 (at 0 -1.397 270) (layer B.SilkS))
    (fp_text value Thermistor_PTC (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 /TACH_IN))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 135.128 107.188)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference TH3 (at 2.667 0) (layer B.SilkS))
    (fp_text value Thermistor_PTC (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 /THERMOCOUPLE_IN-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 131.699 107.188 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference TH2 (at 2.667 0 180) (layer B.SilkS))
    (fp_text value Thermistor_PTC (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 /THERMOCOUPLE_IN+))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 58CE4E7E)
    (at 173.309907 96.694078)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U5 (at 3.404 -3.302) (layer B.SilkS))
    (fp_text value LM2937xMP-3.3 (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -3.15 2.3) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V))
    (pad 3 smd rect (at -3.15 -2.3) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 142.24 99.568 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 0 2.5 270) (layer B.SilkS))
    (fp_text value BAS40-04 (at 0 -2.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 /OIL_TEMP_IN))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 155.531422 107.33518)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 0 2.5) (layer B.SilkS))
    (fp_text value BAS40-04 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 25 +12V))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 157.182422 103.52518 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.5 90) (layer B.SilkS))
    (fp_text value MMBT3904-7-F (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 38 /TACH))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 142.24 103.251 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.54 -90) (layer B.SilkS))
    (fp_text value MMBT3906-7-F (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 /OIL_TEMP_IN))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 135.382 104.267 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D4 (at -2.413 0 90) (layer B.SilkS))
    (fp_text value BAS40-04 (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353_SC-70-5 (layer B.Cu) (tedit 58CE4E7F)
    (at 140.193 114.239 90)
    (descr "SOT-353, SC-70-5")
    (tags "SOT-353 SC-70-5")
    (attr smd)
    (fp_text reference U1 (at -2.22 0.015 180) (layer B.SilkS))
    (fp_text value TMP20AIDCK (at 0 -2 -90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 0.95 0.65 90) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 4 smd rect (at 0.95 -0.65 90) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 2 smd rect (at -0.95 0 90) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 3 smd rect (at -0.95 -0.65 90) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 32 /COLD_JUNC))
    (pad 1 smd rect (at -0.95 0.65 90) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-353_SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23-5 (layer B.Cu) (tedit 58CE4E80)
    (at 144.399 107.315 90)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags TSOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -3.048 -0.254) (layer B.SilkS))
    (fp_text value TLV6001 (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.31 0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 28 /+3.3VA))
    (pad 4 smd rect (at 1.31 -0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at -1.31 -0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -1.31 0 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.31 0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23-6 (layer B.Cu) (tedit 58CE4E80)
    (at 172.903907 110.029078 90)
    (descr "6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf")
    (tags "TSOT-23-6 MK06A TSOT-6")
    (attr smd)
    (fp_text reference U4 (at 0.508 2.286 -90) (layer B.SilkS))
    (fp_text value LM2840X (at 0 -2.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 6 smd rect (at 1.31 0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C21-Pad1)"))
    (pad 5 smd rect (at 1.31 0 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 25 +12V))
    (pad 4 smd rect (at 1.31 -0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 25 +12V))
    (pad 3 smd rect (at -1.31 -0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at -1.31 0 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 1 smd rect (at -1.31 0.95 90) (size 1.22 0.65) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:FTSH-105-01-L-DV-007-K (layer B.Cu) (tedit 5E67F2E4)
    (at 130.556 72.136 90)
    (attr smd)
    (fp_text reference J5 (at 4.699 7.493 180) (layer B.SilkS))
    (fp_text value FTSH-105-01-L-DV-007-K (at -1.27 -2.54 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (pad 3 smd rect (at 1.27 0 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 5 smd rect (at 2.54 0 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 9 smd rect (at 5.08 0 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0 4.07 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 20 /JTMS))
    (pad 4 smd rect (at 1.27 4.064 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 21 /JTCK))
    (pad 6 smd rect (at 2.54 4.064 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 22 /JTDO))
    (pad 10 smd rect (at 5.08 4.064 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 23 /JNTRST))
    (pad 8 smd rect (at 3.81 4.064 90) (size 0.74 2.79) (layers B.Cu B.Paste B.Mask)
      (net 24 /JTDI))
  )
  (module footprints:MSS6132T (layer B.Cu) (tedit 5E6ABE24)
    (at 173.157907 104.187078 90)
    (fp_text reference L1 (at 2.032 -6.096 90) (layer B.SilkS))
    (fp_text value LPS5030/15uH (at 0.1 6.45 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 6 2) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C21-Pad1)") (zone_connect 0))
    (pad 2 smd rect (at 0 -4 90) (size 6 2) (layers B.Cu B.Paste B.Mask)
      (net 19 +5V) (zone_connect 0))
  )
  (module footprints:X27.589 locked (layer B.Cu) (tedit 5E6ADB78)
    (at 152.908 89.662)
    (fp_text reference U10 (at -4.953 -21.082) (layer B.SilkS) hide)
    (fp_text value X27.589 (at 0 -5.08) (layer B.Fab))
    (pad "" np_thru_hole circle (at 0 -16.75) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 13.5 -6) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -13.5 -6) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 11.45 -2.19) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(U10-Pad1)"))
    (pad 2 thru_hole circle (at 11.43 -9.81) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(U10-Pad2)"))
    (pad 3 thru_hole circle (at -11.43 -9.81) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(U10-Pad3)"))
    (pad 4 thru_hole circle (at -11.43 -2.19) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(U10-Pad4)"))
  )
  (module footprints:XF2M-1415-1A locked (layer F.Cu) (tedit 5E681251)
    (at 165.608 110.692 90)
    (fp_text reference J4 (at 0.075 6.35 180) (layer F.SilkS))
    (fp_text value XF2M-1415-1A (at -3.15 -7.2 90) (layer F.Fab))
    (pad 1 smd rect (at -3.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at -2.75 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C9-Pad2)"))
    (pad 3 smd rect (at -2.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C13-Pad1)"))
    (pad 4 smd rect (at -1.75 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C13-Pad2)"))
    (pad 6 smd rect (at -0.75 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C10-Pad2)"))
    (pad 5 smd rect (at -1.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 8 smd rect (at 0.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 7 smd rect (at -0.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 13 smd rect (at 2.75 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C14-Pad1)"))
    (pad 10 smd rect (at 1.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCL))
    (pad 9 smd rect (at 0.75 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 /PG9616_RESET))
    (pad 12 smd rect (at 2.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J4-Pad12)"))
    (pad 14 smd rect (at 3.25 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 11 smd rect (at 1.75 0 90) (size 0.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 /SDA))
    (pad "" smd rect (at -4.9 3.9 90) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 4.9 3.9 90) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at -4.4 -0.85 90) (size 1 1) (layers F.SilkS))
  )
  (gr_text JTAG (at 139.573 69.85) (layer B.SilkS))
  (gr_text T+ (at 131.191 116.332) (layer F.SilkS))
  (gr_text T- (at 136.144 116.332) (layer F.SilkS))
  (gr_text TACH (at 154.178 112.522) (layer F.SilkS))
  (gr_text "OIL TEMP" (at 145.288 112.522) (layer F.SilkS))
  (gr_text "PRINT AND CHECK AGAINST FRAME" (at 152.904 62.738) (layer Cmts.User))
  (gr_line (start 127.408 64.662) (end 178.408 64.662) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.408 117.602) (end 127.408 64.662) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.427 117.602) (end 127.408 117.602) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.408 64.662) (end 178.427 117.602) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.989 110.998) (xy 171.252907 111.045078) (xy 171.252907 110.537078) (xy 172.522907 110.537078) (xy 172.522907 111.934078)
        (xy 173.284907 111.934078) (xy 173.284907 110.537078) (xy 177.348907 110.537078) (xy 177.348907 105.203078) (xy 174.681907 105.203078)
        (xy 174.752 109.474) (xy 165.989 109.474)
      )
    )
  )
  (zone (net 25) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.030907 108.251078) (xy 172.974 108.251078) (xy 172.974 113.538) (xy 167.64 113.538) (xy 167.64 106.807)
        (xy 170.744907 106.807) (xy 170.744907 106.600078) (xy 173.030907 106.600078)
      )
    )
  )
  (zone (net 25) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.355 109.22) (xy 171.577 109.22) (xy 171.577 108.585) (xy 170.18 108.585) (xy 170.18 107.569)
        (xy 173.355 107.569)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.292 110.998) (xy 177.292 109.474) (xy 169.418 109.474) (xy 169.418 110.998)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 137.541 88.7095) (xy 148.209 96.901) (xy 153.416 96.901) (xy 153.416 110.363) (xy 128.016 110.363)
        (xy 128.016 85.31225) (xy 137.541 85.344)
      )
    )
  )
  (zone (net 28) (net_name /+3.3VA) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.89 78.359) (xy 132.842 78.359) (xy 132.842 77.089) (xy 135.89 77.089)
      )
    )
  )
  (zone (net 19) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 79.629) (xy 132.461 79.629) (xy 132.461 80.391) (xy 133.096 80.899) (xy 133.604 80.899)
        (xy 133.604 82.423) (xy 135.382 82.423) (xy 135.382 80.518) (xy 134.366 80.518) (xy 133.858 80.518)
        (xy 133.223 80.518) (xy 133.096 80.518) (xy 132.715 80.137) (xy 132.715 80.01)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.967907 97.583078) (xy 168.712907 97.583078) (xy 168.712907 98.472078) (xy 167.823907 98.472078) (xy 167.823907 94.916078)
        (xy 168.712907 94.916078) (xy 168.712907 95.805078) (xy 176.967907 95.805078)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.760907 94.408078) (xy 167.950907 94.408078) (xy 167.950907 93.773078) (xy 169.220907 93.773078) (xy 169.220907 92.757078)
        (xy 171.760907 92.757078)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.665907 98.218078) (xy 173.665907 95.170078) (xy 171.760907 95.170078) (xy 171.760907 98.218078)
      )
    )
  )
  (zone (net 19) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.242 84.455) (xy 171.069 97.282) (xy 171.069 99.107078) (xy 173.665907 99.107078) (xy 173.665907 100.631078)
        (xy 170.236907 100.631078) (xy 170.236907 100.584) (xy 168.021 100.584) (xy 156.591 89.154) (xy 156.5275 65.913)
        (xy 158.1785 65.913)
      )
    )
  )
  (zone (net 6) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.561 85.09) (xy 171.196 85.725) (xy 171.196 90.297) (xy 171.831 90.932) (xy 171.831 92.757078)
        (xy 173.665907 92.757078) (xy 173.665907 94.154078) (xy 170.236907 94.154078) (xy 170.236907 94.107) (xy 169.926 94.107)
        (xy 169.926 86.36) (xy 169.164 85.598) (xy 169.164 78.74) (xy 170.561 78.74)
      )
    )
  )
  (zone (net 47) (net_name /-3.3VA) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.017 97.155) (xy 132.588 97.155) (xy 131.953 97.155) (xy 131.953 99.441) (xy 132.461 99.441)
        (xy 132.461 98.171) (xy 133.985 98.171) (xy 133.985 99.187) (xy 134.493 99.187) (xy 134.493 97.79)
        (xy 136.017 97.79)
      )
    )
  )
  (zone (net 28) (net_name /+3.3VA) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.017 96.647) (xy 133.985 96.647) (xy 133.985 94.361) (xy 134.366 94.361) (xy 134.366 96.012)
        (xy 136.017 96.012)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.8 96.139) (xy 148.209 96.139) (xy 138.43 88.519) (xy 138.43 73.787) (xy 128.016 73.787)
        (xy 128.016 64.897) (xy 177.673 64.897)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 154.051 97.663) (xy 154.051 110.363) (xy 167.35425 110.363) (xy 167.41775 97.663)
      )
    )
  )
  (zone (net 19) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.894 98.933) (xy 170.18 98.933) (xy 170.18 107.188) (xy 169.545 107.188) (xy 169.545 108.839)
        (xy 167.894 108.839)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.323 116.713) (xy 173.863 116.713) (xy 173.863 112.141) (xy 173.355 112.141) (xy 173.355 110.617)
        (xy 172.466 110.617) (xy 172.466 112.141) (xy 172.085 112.141) (xy 171.323 112.903)
      )
    )
  )
  (zone (net 25) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.419 116.713) (xy 177.419 111.125) (xy 172.085 111.125) (xy 172.085 113.538) (xy 174.879 113.538)
        (xy 174.879 116.713)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.752 108.077) (xy 177.292 108.077) (xy 177.292 110.236) (xy 174.752 110.236)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 128.016 85.598) (xy 128.016 74.676) (xy 137.541 74.676) (xy 137.541 85.598)
      )
    )
  )
)
