<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="77.47" y2="0" width="0.1524" layer="20"/>
<wire x1="77.47" y1="0" x2="77.47" y2="63.5" width="0.1524" layer="20"/>
<wire x1="77.47" y1="63.5" x2="0" y2="63.5" width="0.1524" layer="20"/>
<wire x1="0" y1="63.5" x2="0" y2="49.022" width="0.1524" layer="20"/>
<wire x1="0" y1="49.022" x2="7.5692" y2="49.022" width="0.1524" layer="20"/>
<wire x1="7.5692" y1="49.022" x2="7.5692" y2="42.7228" width="0.1524" layer="20"/>
<wire x1="7.5692" y1="42.7228" x2="0" y2="42.7228" width="0.1524" layer="20"/>
<wire x1="0" y1="42.7228" x2="0" y2="36.3855" width="0.1524" layer="20"/>
<wire x1="0" y1="36.3855" x2="-0.0127" y2="35.7505" width="0.1524" layer="20"/>
<wire x1="-0.0127" y1="35.7505" x2="-0.0127" y2="34.9631" width="0.1524" layer="20"/>
<wire x1="-0.0127" y1="34.9631" x2="0" y2="34.2138" width="0.1524" layer="20"/>
<wire x1="0" y1="34.2138" x2="0" y2="22.86" width="0.1524" layer="20"/>
<wire x1="0" y1="22.86" x2="12.7" y2="22.86" width="0.1524" layer="20"/>
<wire x1="12.7" y1="22.86" x2="12.7" y2="12.7" width="0.1524" layer="20"/>
<wire x1="12.7" y1="12.7" x2="0" y2="12.7" width="0.1524" layer="20"/>
<wire x1="0" y1="12.7" x2="0" y2="0" width="0.1524" layer="20"/>
<hole x="6.35" y="3.7465" drill="5.08" locked="yes"/>
<hole x="71.3486" y="3.7465" drill="5.08" locked="yes"/>
<hole x="71.3486" y="59.7535" drill="5.08" locked="yes"/>
<hole x="6.35" y="59.7535" drill="5.08" locked="yes"/>
<text>Battery</text>
<text>+</text>
<text>-</text>
<text>LED</text>
<text>   LCD
D0=D22
D1=D23
D2=D24
D3=D25
D4=D26
D5=D27
D6=D28
D7=D29
C/S=A0
C/D=A1
W/R=A2
RD=A3
X-=A4
Y+=A5
X+=D8
Y-=D9
</text>
<text>D7=Optional IR LED
D10=HomeSwitch
D11=TXData
D12=PowerOff
D32=Optional LED
A6=BatterySense
A11=Photocell PGM
</text>
<text>RV-Project.Com Remote Board</text>
<text>Power with (2) 14500 
3.7V rechargeable 
Li-Ion batteries only.</text>
<text>Reset 1</text>
<text>Reset 2</text>
<text>Backlight</text>
<text>                     Options
Reset 1: Reset LCD to 2560 Reset Pin
Reset 2: Reset LCD to 2560 D46 (PWM)
Backlight: Control LCD with 2560 D44 (PWM)
3.3V Ref: Battery Voltage Sense Option</text>
<text>3.3V Ref</text>
<text>7.4V</text>
<text>TP1</text>
<text>Made in USA</text>
<text></text>
<text>Transmit Voltage</text>
<text>3.3V</text>
<text>5V</text>
<text>Batt</text>
<text></text>
<text>  V5.2  3/23/2019</text>
<text>Switch</text>
<hole x="73.6346" y="55.3974" drill="2.9464"/>
<text>A</text>
<text>C</text>
<text>TP1</text>
<text>IR-TX</text>
<text>Enable</text>
<text>Disable</text>
<text>Options</text>
<text>IR</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor.&lt;br&gt;Pitch:0.1&lt;br&gt;
Dia: 0.2"Dia (5.08mm)</description>
</package>
<package name="DIODE-1N4148">
<description>Pitch: 0.3"</description>
</package>
<package name="SMD-JUMPER_2">
<description>Pad Size: 0.12"x0.06"&lt;br&gt;Resist remoted between pads for ease of solder bridge.</description>
</package>
<package name="1X02">
<description>Pitch: 0.1" (2.54mm)&lt;br&gt;Drill: 0.040" dia</description>
</package>
<package name="ADAFRUIT2.8BREAKOUT_HEADER">
<description>Adafruit 1743 (3.2") and 1770 (2.8") LCD Breakout for 8-bit parallel end.</description>
</package>
<package name="TO-92-AMMO">
</package>
<package name="1206-RES">
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;Pitch: 0.35"</description>
</package>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="STX882">
</package>
<package name="MEDUINO_MEGA_MINI">
<description>Meduino Version (not Robodyn) of Mini 2560  Narrower pad orientation
 and relocated AREF and RST pins.</description>
</package>
<package name="ART_CHEROKEE_MEDIUM">
</package>
<package name="DIODE-ZENER">
<description>Pitch: 0.28"</description>
</package>
<package name="1X01_HEADER">
<description>Drill: 0.039" dia</description>
</package>
<package name="CREATIVECOMMONS@1">
</package>
<package name="GENERIC_0100_DEVICE_100_SPACING">
<description>Pitch: 0.1" (2.54mm)</description>
</package>
<package name="FS1000_H">
</package>
<package name="1X03">
<description>Pitch: 0.1" (2.54mm)
&lt;br&gt;Drill: 0.040" dia</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="D2" library="a-lib" package="DIODE-1N4148" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="J12" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="J11" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="LCD1" library="a-lib" package="ADAFRUIT2.8BREAKOUT_HEADER" value=""/>
<element name="Q2" library="a-lib" package="TO-92-AMMO" value="2N2222">
<attribute name="NAME"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SR1" library="a-lib" package="DIL04" value="TLP222">
<attribute name="NAME"/>
</element>
<element name="TX1" library="a-lib" package="STX882" value=""/>
<element name="U1" library="a-lib" package="MEDUINO_MEGA_MINI" value="">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="a-lib" package="ART_CHEROKEE_MEDIUM" value="Cherokee Medium"/>
<element name="J8" library="a-lib" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="J9" library="a-lib" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="J10" library="a-lib" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="D1" library="a-lib" package="DIODE-ZENER" value="1N4735">
<attribute name="NAME"/>
<attribute name="VALUE" value="1N4735"/>
</element>
<element name="J2" library="a-lib" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="J7" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="JP1" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="a-lib" package="CREATIVECOMMONS@1" value=""/>
<element name="U$3" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
<element name="D3" library="a-lib" package="DIODE-ZENER" value="1N4730A">
<attribute name="NAME"/>
<attribute name="VALUE" value="1N4727"/>
</element>
<element name="J6" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="a-lib" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="J4" library="a-lib" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="J5" library="a-lib" package="SMD-JUMPER_2" value="M2JUMPER1"/>
<element name="Q1" library="a-lib" package="TO-92-AMMO" value="2N2222">
<attribute name="NAME"/>
</element>
<element name="R7" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C3" library="a-lib" package="GENERIC_0100_DEVICE_100_SPACING" value="0.1UF">
<attribute name="MARKING" value="104 (100nF)"/>
<attribute name="NAME"/>
</element>
<element name="TX2" library="a-lib" package="FS1000_H" value=""/>
<element name="J13" library="a-lib" package="1X03" value="M3HEADER"/>
<element name="J1" library="a-lib" package="1X02" value="M2HEADER">
<attribute name="PITCH" value="2.54MM"/>
</element>
<element name="U$2" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_SMALL" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="J12" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="SR1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="TX1" pad="GND"/>
<contactref element="U1" pad="GND3"/>
<contactref element="LCD1" pad="GND8"/>
<contactref element="U1" pad="GND1"/>
<contactref element="R2" pad="1"/>
<contactref element="J7" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="TX2" pad="GND"/>
<contactref element="U1" pad="GND2"/>
<contactref element="U1" pad="GND4"/>
</signal>
<signal name="N$23">
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="SR1" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="D12"/>
</signal>
<signal name="N$25">
<contactref element="J11" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="U1" pad="D10"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="D22"/>
<contactref element="LCD1" pad="D08"/>
</signal>
<signal name="N$4">
<contactref element="LCD1" pad="D18"/>
<contactref element="U1" pad="D23"/>
</signal>
<signal name="N$5">
<contactref element="LCD1" pad="D28"/>
<contactref element="U1" pad="D24"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="D25"/>
<contactref element="LCD1" pad="D38"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="D26"/>
<contactref element="LCD1" pad="D48"/>
</signal>
<signal name="N$8">
<contactref element="LCD1" pad="D58"/>
<contactref element="U1" pad="D27"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="D28"/>
<contactref element="LCD1" pad="D68"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="LCD1" pad="D78"/>
<contactref element="U1" pad="D29"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="LCD1" pad="CD8"/>
<contactref element="U1" pad="A1"/>
</signal>
<signal name="N$13">
<contactref element="LCD1" pad="WR8"/>
<contactref element="U1" pad="A2"/>
</signal>
<signal name="N$14">
<contactref element="LCD1" pad="RD8"/>
<contactref element="U1" pad="A3"/>
</signal>
<signal name="N$16">
<contactref element="LCD1" pad="CS8"/>
<contactref element="U1" pad="A0"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="D11"/>
<contactref element="TX1" pad="DATA"/>
<contactref element="TX2" pad="DATA"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="VIN2"/>
<contactref element="R6" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="SR1" pad="3"/>
<contactref element="U1" pad="VIN1"/>
<contactref element="D1" pad="P$2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="SR1" pad="4"/>
<contactref element="J12" pad="1"/>
<contactref element="D3" pad="P$2"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="A6"/>
<contactref element="R2" pad="2"/>
<contactref element="D1" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="LCD1" pad="X-8"/>
<contactref element="U1" pad="A4"/>
</signal>
<signal name="N$20">
<contactref element="LCD1" pad="Y+8"/>
<contactref element="U1" pad="A5"/>
</signal>
<signal name="N$26">
<contactref element="LCD1" pad="Y-8"/>
<contactref element="U1" pad="D9"/>
</signal>
<signal name="N$21">
<contactref element="LCD1" pad="X+8"/>
<contactref element="U1" pad="D8"/>
</signal>
<signal name="N$15">
<contactref element="LCD1" pad="RST8"/>
<contactref element="J10" pad="1"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="LCD1" pad="LITE8"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="U1" pad="RST"/>
<contactref element="J10" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="U1" pad="D46"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="U1" pad="D44"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U1" pad="AREF"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="3V31"/>
<contactref element="U1" pad="3V32"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="J11" pad="2"/>
<contactref element="D3" pad="P$1"/>
</signal>
<signal name="N$35">
<contactref element="J6" pad="2"/>
<contactref element="U1" pad="D32"/>
</signal>
<signal name="N$36">
<contactref element="J6" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="TX1" pad="VCC"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="TX2" pad="VCC"/>
</signal>
<signal name="N$38">
<contactref element="U1" pad="D5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="LCD1" pad="VIN8"/>
<contactref element="U1" pad="5V1"/>
<contactref element="U1" pad="5V2"/>
<contactref element="J7" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J13" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R7" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="Q1" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="J1" pad="2"/>
<contactref element="J13" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
