<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<circle x="23" y="23" radius="23" width="0.1" layer="20"/>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8S1">
<description>&lt;b&gt;8S1&lt;/b&gt; 8-lead (0.150" Wide Body)&lt;p&gt;
Plastic Gull Wing Small Outline (JEDEC SOIC)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT89">
</package>
<package name="1206">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT669">
<description>&lt;b&gt;SOT 669 (LFPAK)&lt;/b&gt;&lt;p&gt;
Source: http://www.nxp.com/acrobat_download/datasheets/PH7030L_4.pdf</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="8S1" value="TINY13V-10SSU">
<attribute name="OC_NEWARK" value="58M3773"/>
<attribute name="MPN" value="ATTINY13V-10SSU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1455135"/>
</element>
<element name="U$1" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="U$2" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="U$3" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="Q1" library="transistor-power" package="SOT669" value="PH7030L"/>
<element name="Q2" library="transistor-power" package="SOT669" value="PH7030L"/>
<element name="Q3" library="transistor-power" package="SOT669" value="PH7030L"/>
<element name="R2" library="SparkFun" package="1206" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="1206" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="1206" value="100nF"/>
<element name="SWITCH" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWITCH_LED" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="8V4_1" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="8V4_2" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="GND_1" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="GND_2" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="U1" library="SparkFun" package="SOT23-5" value="V_REG_LDOSMD"/>
<element name="C2" library="SparkFun" package="1206" value="100nF"/>
<element name="C3" library="SparkFun" package="1206" value="100nF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="4"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="GND_1" pad="TP"/>
<contactref element="GND_2" pad="TP"/>
<contactref element="U1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="1"/>
<contactref element="Q1" pad="MB"/>
<contactref element="U$2" pad="1"/>
<contactref element="Q2" pad="MB"/>
<contactref element="U$3" pad="1"/>
<contactref element="Q3" pad="MB"/>
</signal>
<signal name="N$4">
<contactref element="Q3" pad="4"/>
<contactref element="Q2" pad="4"/>
<contactref element="Q1" pad="4"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$3" pad="3"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="8V4_1" pad="TP"/>
<contactref element="8V4_2" pad="TP"/>
<contactref element="U1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="U1" pad="5"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="2"/>
<contactref element="SWITCH" pad="TP"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="3"/>
<contactref element="SWITCH_LED" pad="TP"/>
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
