(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 56)
    (zones 0)
    (modules 2)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1778)
    (trace_clearance 0.2)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (user_via 0.4064 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.1778)
    (uvia_min_drill 0.1)
    (edge_width 0.0254)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4 1.4)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /RI)
  (net 2 /DTR)
  (net 3 /DCD)
  (net 4 /SG)
  (net 5 /DSR)
  (net 6 /CTS)
  (net 7 /RTS)
  (net 8 /RXD)
  (net 9 /TXD)
  (net 10 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CTS)
    (add_net /DCD)
    (add_net /DSR)
    (add_net /DTR)
    (add_net /RI)
    (add_net /RTS)
    (add_net /RXD)
    (add_net /SG)
    (add_net /TXD)
    (add_net GND)
  )
  (module 0_LOCAL:DSUB-25_Male_Vertical_P2.77x2.84mm (layer F.Cu) (tedit 5F17AABC)
    (at 144.2212 113.0427 90)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J2 (at 1.4605 1.2827 270) (layer F.SilkS) hide)
    (fp_text value DB25_Male (at 16.62 8.73 270) (layer F.Fab))
    (fp_text user %R (at 16.62 1.42 270) (layer F.Fab))
    (pad 25 thru_hole circle (at 31.855 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 29.085 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 26.315 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 23.545 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 /RI))
    (pad 21 thru_hole circle (at 20.775 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 18.005 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 /DTR))
    (pad 19 thru_hole circle (at 15.235 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 12.465 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 9.695 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 6.925 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 4.155 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 1.385 2.84 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 33.24 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 30.47 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 27.7 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 24.93 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 22.16 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 19.39 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 /DCD))
    (pad 7 thru_hole circle (at 16.62 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 /SG))
    (pad 6 thru_hole circle (at 13.85 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 5 /DSR))
    (pad 5 thru_hole circle (at 11.08 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 6 /CTS))
    (pad 4 thru_hole circle (at 8.31 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 7 /RTS))
    (pad 3 thru_hole circle (at 5.54 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 8 /RXD))
    (pad 2 thru_hole circle (at 2.77 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 9 /TXD))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/connector_a-ds_25_pp_z.stp
      (offset (xyz 16.625 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:DSUB-25_Male_EdgeMount_P2.77mm (layer F.Cu) (tedit 5F053F30)
    (at 136.75 96.42 270)
    (descr "25-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 47.1mm")
    (attr smd)
    (fp_text reference J1 (at -15.267 -0.4688 270) (layer F.SilkS) hide)
    (fp_text value DB25_Male (at 0 16.69 270) (layer F.Fab))
    (fp_text user "PCB edge" (at -21.55 1.323333 270) (layer Dwgs.User))
    (fp_text user %R (at 0 3.39 270) (layer F.Fab))
    (pad 25 smd oval (at 15.235 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 24 smd oval (at 12.465 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd oval (at 9.695 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 22 smd oval (at 6.925 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask)
      (net 1 /RI))
    (pad 21 smd oval (at 4.155 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd oval (at 1.385 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /DTR))
    (pad 19 smd oval (at -1.385 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd oval (at -4.155 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd oval (at -6.925 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd oval (at -9.695 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd oval (at -12.465 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd oval (at -15.235 -0.5 270) (size 1 4.6) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd oval (at 16.62 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd oval (at 13.85 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd oval (at 11.08 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd oval (at 8.31 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd oval (at 5.54 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd oval (at 2.77 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /DCD))
    (pad 7 smd oval (at 0 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /SG))
    (pad 6 smd oval (at -2.77 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /DSR))
    (pad 5 smd oval (at -5.54 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /CTS))
    (pad 4 smd oval (at -8.31 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /RTS))
    (pad 3 smd oval (at -11.08 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /RXD))
    (pad 2 smd oval (at -13.85 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /TXD))
    (pad 1 smd rect (at -16.62 -0.5 270) (size 1 4.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/connector_a-ds_25_pp_z.stp
      (offset (xyz 0 -8.199999999999999 -0.87))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text github.com/bkw777/WiModem_to_100 (at 145.65 96.4 90) (layer B.SilkS))
  (gr_text 25 (at 145.923 81.2292 90) (layer B.SilkS))
  (gr_text 13 (at 145.4404 79.7814 90) (layer B.SilkS))
  (gr_text 14 (at 145.8976 111.7092 90) (layer B.SilkS))
  (gr_text 1 (at 145.4404 113.0554 90) (layer B.SilkS))
  (gr_text 25 (at 140.25 111.6584 90) (layer B.SilkS))
  (gr_text 14 (at 140.25 81.1784 90) (layer B.SilkS))
  (gr_text 13 (at 140.25 113.05 90) (layer F.SilkS))
  (gr_text 1 (at 140.25 79.8068 90) (layer F.SilkS))
  (gr_text 25 (at 145.923 81.2292 90) (layer F.SilkS))
  (gr_text 14 (at 145.8976 111.7092 90) (layer F.SilkS))
  (gr_text 13 (at 145.4404 79.7814 90) (layer F.SilkS))
  (gr_text 1 (at 145.4404 113.0554 90) (layer F.SilkS))
  (gr_text "A-DS 25 PP/Z" (at 145.675 96.425 90) (layer F.SilkS))
  (gr_text "connector this side" (at 142.25 96.425 90) (layer F.SilkS))
  (gr_text "TRS-80 Model 100" (at 142.425 96.4311 90) (layer B.SilkS))
  (gr_text WiModem232 (at 140.625 96.4057 90) (layer B.SilkS))
  (gr_line (start 134.9 113.7666) (end 147.7772 113.7666) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 134.9 79.0829) (end 134.9 113.7666) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 134.9 79.0829) (end 147.7772 79.0829) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 147.7772 113.7666) (end 147.7772 79.0829) (layer Edge.Cuts) (width 0.0254))
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 147.7772 113.7666) (xy 134.9 113.7666) (xy 134.9 79.08544) (xy 147.7772 79.0829)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3048) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 147.7772 113.7666) (xy 134.9 113.7666) (xy 134.9 79.08544) (xy 147.7772 79.0829)
      )
    )
  )
)
