(kicad_pcb (version 20171130) (host pcbnew 5.1.5-5.1.5)
  (general
    (thickness 1.6)
    (drawings 59)
    (tracks 843)
    (zones 0)
    (modules 49)
    (nets 49)
  )
  (page USLetter)
  (title_block
    (title "Neo Teensy")
    (date 2019-12-31)
    (rev 3.3)
    (comment 1 "Copyright (C) 2019 Aaron Williams")
    (comment 2 aaron.w2@gmail.com)
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu mixed)
    (2 In2.Cu mixed)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.5)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 +5V)
  (net 4 /DO)
  (net 5 /IO12)
  (net 6 /IO11)
  (net 7 /IO10)
  (net 8 /IO9)
  (net 9 /IO8)
  (net 10 /IO7)
  (net 11 /IO6)
  (net 12 /IO5)
  (net 13 /IO4)
  (net 14 /IO3)
  (net 15 /IO2)
  (net 16 /IO1)
  (net 17 /IO0)
  (net 18 /ON_OFF)
  (net 19 /Program)
  (net 20 /IO23)
  (net 21 /IO22)
  (net 22 /IO21)
  (net 23 /IO20)
  (net 24 /IO19)
  (net 25 /IO18)
  (net 26 /IO15)
  (net 27 /IO14)
  (net 28 /IO13)
  (net 29 /IO6_H)
  (net 30 /VBat)
  (net 31 /DIN)
  (net 32 /12-Boost/SS)
  (net 33 /12-Boost/COMP)
  (net 34 "Net-(C205-Pad1)")
  (net 35 +12V)
  (net 36 /12-Boost/SW)
  (net 37 /12-Boost/FET_DRV)
  (net 38 FET_CTL)
  (net 39 /12-Boost/FREQ)
  (net 40 /12-Boost/FB)
  (net 41 "Net-(U201-Pad5)")
  (net 42 "Net-(U201-Pad10)")
  (net 43 "Net-(U201-Pad14)")
  (net 44 /IO16)
  (net 45 /IO9_H)
  (net 46 /IO8_H)
  (net 47 "Net-(RN1-Pad10)")
  (net 48 "Net-(RN1-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /12-Boost/COMP)
    (add_net /12-Boost/FB)
    (add_net /12-Boost/FET_DRV)
    (add_net /12-Boost/FREQ)
    (add_net /12-Boost/SS)
    (add_net /12-Boost/SW)
    (add_net /DIN)
    (add_net /DO)
    (add_net /IO0)
    (add_net /IO1)
    (add_net /IO10)
    (add_net /IO11)
    (add_net /IO12)
    (add_net /IO13)
    (add_net /IO14)
    (add_net /IO15)
    (add_net /IO16)
    (add_net /IO18)
    (add_net /IO19)
    (add_net /IO2)
    (add_net /IO20)
    (add_net /IO21)
    (add_net /IO22)
    (add_net /IO23)
    (add_net /IO3)
    (add_net /IO4)
    (add_net /IO5)
    (add_net /IO6)
    (add_net /IO6_H)
    (add_net /IO7)
    (add_net /IO8)
    (add_net /IO8_H)
    (add_net /IO9)
    (add_net /IO9_H)
    (add_net /ON_OFF)
    (add_net /Program)
    (add_net /VBat)
    (add_net FET_CTL)
    (add_net GND)
    (add_net "Net-(C205-Pad1)")
    (add_net "Net-(RN1-Pad10)")
    (add_net "Net-(RN1-Pad11)")
    (add_net "Net-(U201-Pad10)")
    (add_net "Net-(U201-Pad14)")
    (add_net "Net-(U201-Pad5)")
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 27.66 62.54)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0.09 1.53 -180) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 47 "Net-(RN1-Pad10)"))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 33.16 55.75)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 2.6 -0.12) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 48 "Net-(RN1-Pad11)"))
  )
  (module Fiducial:Fiducial_0.5mm_Mask1mm (layer B.Cu) (tedit 5C18CB26)
    (at 45.12 32.68)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID5 (at -2.44 -0.16) (layer B.SilkS))
    (fp_text value FIDUCIAL_1MM (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers B.Cu B.Mask)
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (module Fiducial:Fiducial_0.5mm_Mask1mm (layer B.Cu) (tedit 5C18CB26)
    (at 19.98 32.67)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID4 (at 2.18 0) (layer B.SilkS))
    (fp_text value FIDUCIAL_1MM (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers B.Cu B.Mask)
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (module Fiducial:Fiducial_0.5mm_Mask1mm (layer F.Cu) (tedit 5C18CB26)
    (at 47.68 32.67)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID3 (at -1.76 -0.32) (layer F.SilkS))
    (fp_text value FIDUCIAL_1MM (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (module Fiducial:Fiducial_0.5mm_Mask1mm (layer B.Cu) (tedit 5C18CB26)
    (at 47.84 68.89)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID6 (at -2.18 -0.04) (layer B.SilkS))
    (fp_text value FIDUCIAL_1MM (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers B.Cu B.Mask)
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (module Aaron:SW_SPST_KMR2 (layer F.Cu) (tedit 5BBAE414)
    (at 35.55 33.7 180)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.45 180) (layer F.SilkS))
    (fp_text value SW_SPST_KMR2 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.45) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.05 -0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /Program))
    (pad 2 smd rect (at -2.05 0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.05 -0.8 270) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /Program))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_KMR2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/aaronw/kicad/library/aaron/packages3d/KMR231GLFS.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_8x0602 (layer B.Cu) (tedit 58E0A8FC)
    (at 34.2 58.35 90)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 3 90) (layer B.SilkS))
    (fp_text value 100K (at 0 -3 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 10 smd rect (at 0.9 -1.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(RN1-Pad10)"))
    (pad 12 smd rect (at 0.9 -0.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /IO0))
    (pad 11 smd rect (at 0.9 -0.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(RN1-Pad11)"))
    (pad 13 smd rect (at 0.9 0.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 16 /IO1))
    (pad 14 smd rect (at 0.9 0.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 15 /IO2))
    (pad 15 smd rect (at 0.9 1.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /IO3))
    (pad 7 smd rect (at -0.9 -1.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 44 /IO16))
    (pad 6 smd rect (at -0.9 -0.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 27 /IO14))
    (pad 5 smd rect (at -0.9 -0.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /IO12))
    (pad 4 smd rect (at -0.9 0.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 /IO11))
    (pad 3 smd rect (at -0.9 0.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /IO10))
    (pad 2 smd rect (at -0.9 1.25 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 13 /IO4))
    (pad 9 smd rect (at 0.9 -1.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 38 FET_CTL))
    (pad 8 smd rect (at -0.9 -1.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 26 /IO15))
    (pad 16 smd rect (at 0.9 1.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -0.9 1.75 90) (size 0.8 0.3) (layers B.Cu B.Paste B.Mask)
      (net 12 /IO5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical (layer F.Cu) (tedit 5DC900D9)
    (at 43.18 49.784)
    (descr "Through hole straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.54mm double row")
    (fp_text reference J8 (at 4.7752 4.064 90) (layer F.SilkS))
    (fp_text value Conn_02x07_Odd_Even (at 2.73 7.376 90) (layer F.Fab))
    (fp_text user %R (at 1.27 7.62 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /IO16))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /IO15))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /IO14))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /IO12))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /IO11))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /IO10))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IO4))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IO5))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IO3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IO2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IO1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IO0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 44.45 33.782 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 3.05 0.902) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 33.8455 48.021 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0.221 -1.3455 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 32.5755 45.593)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 28.7655 49.1744)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -1.8405 -0.0744 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 37.211 48.514 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.554 0.009 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 30.7595 37.211 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 33.11 42.67)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at -2.05 -0.83) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 31 /DIN))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5DDB819C)
    (at 35.555 63.725 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (zone_connect 2)
    (fp_text reference J201 (at 0 -2.145 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 1.985 2.855 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /12-Boost/FET_DRV) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +12V) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:QFN-16-1EP_3x3mm_P0.5mm_EP2.7x2.7mm_ThermalVias (layer F.Cu) (tedit 5BC76CBA)
    (at 32.4 53.55 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U201 (at -2.85 -5.325 180) (layer F.SilkS))
    (fp_text value TPS55340-Q1 (at 17.51 0.06 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /12-Boost/SW))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /12-Boost/SS))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U201-Pad5)"))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /12-Boost/COMP))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /12-Boost/FB))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /12-Boost/FREQ))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U201-Pad10)"))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U201-Pad14)"))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /12-Boost/SW))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /12-Boost/SW))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers B.Cu)
      (net 1 GND))
    (pad "" smd rect (at 0.5 -0.5 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0 0 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.5 -0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at 0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad 17 thru_hole circle (at -0.5 0.5 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND))
    (pad "" smd rect (at -0.5 -0.5 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at -0.5 0.5 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.5 0.5 270) (size 0.73 0.73) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP2.7x2.7mm_ThermalVias.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/aaronw/kicad/library/git-old/kicad-library/modules/packages3d/Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31 57.4 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R204 (at 4.5 1.425 180) (layer F.SilkS))
    (fp_text value 10k (at 0.13 0.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /12-Boost/FB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 32.5 57.4 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R203 (at 0.3 6.7 90) (layer F.SilkS))
    (fp_text value 86.6k (at -2.33 0.18 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /12-Boost/FB))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 28.7375 53.65)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R202 (at -1.8375 -0.15 90) (layer F.SilkS))
    (fp_text value 1.62k (at -3.3775 -0.06) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /12-Boost/COMP))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C205-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 28.75 58.15 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R201 (at 1.8 0 90) (layer F.SilkS))
    (fp_text value 18.7K (at 3.59 -0.13) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /12-Boost/FREQ))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer F.Cu) (tedit 5A02FF57)
    (at 28.95 60.2)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q201 (at -2.1 0.325 90) (layer F.SilkS))
    (fp_text value BSS214NW (at -4.63 0.08) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 37 /12-Boost/FET_DRV))
    (pad 2 smd rect (at -1 0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 270) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 38 FET_CTL))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aaron:L_Vishay_IHLP-1212 (layer F.Cu) (tedit 5BC76786)
    (at 36.3 53.75 270)
    (descr "Inductor, Vishay, IHLP series, 3.0mmx3.0mm")
    (tags "inductor vishay ihlp smd")
    (attr smd)
    (fp_text reference L201 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 3.3uH (at -0.13 -2.34 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 /12-Boost/SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Vishay_IHLP-1212.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/aaronw/kicad/library/aaron/packages3d/IND_IHLP-1212BZ.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 37.65 58.35 90)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D201 (at -2.925 0.475 180) (layer F.SilkS))
    (fp_text value SS24FL (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at -3.27 0.45 90) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0 90) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 36 /12-Boost/SW))
    (pad 1 smd rect (at -1.4 0 90) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 31.4 60.4 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C207 (at 0.4 -1.25 90) (layer F.SilkS))
    (fp_text value 1uF (at 0.06 1.07 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 34.9 58.4 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C206 (at -2.75 -0.1 180) (layer F.SilkS))
    (fp_text value 47uF (at -2.39 0.24 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 28 55.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C205 (at 0 1.1 90) (layer F.SilkS))
    (fp_text value 47nF (at 0.19 2.32 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(C205-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.5 55.9 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C204 (at -0.12 -1.65 180) (layer F.SilkS))
    (fp_text value 820pF (at -0.81 -1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /12-Boost/COMP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 28 51.4 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C203 (at 0.3 -1.025 90) (layer F.SilkS))
    (fp_text value 22nF (at -0.03 -2.34 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /12-Boost/SS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 30.25 50.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C202 (at 0.65 -1 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.61 2.74 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 33.25 50.65)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C201 (at 2.15 -0.8 90) (layer F.SilkS))
    (fp_text value 22uF (at 2.9 0.24) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N14 (layer F.Cu) (tedit 5A0AA2C1)
    (at 35.433 39.1795)
    (descr "Texas_S-PVQFN-N14  http://www.ti.com/lit/ds/symlink/txb0104.pdf")
    (tags Texas_S-PVQFN-N14_4.3x4.3_Pitch0.5mm_ThermalPad)
    (attr smd)
    (fp_text reference U1 (at -3.108 0.9955) (layer F.SilkS))
    (fp_text value SN74AHCT125N (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 15 smd rect (at 0 0 270) (size 2.05 2.05) (layers F.Cu F.Mask))
    (pad "" smd rect (at 0.56 -0.56 270) (size 0.82 0.82) (layers F.Paste))
    (pad "" smd rect (at -0.56 -0.56 270) (size 0.82 0.82) (layers F.Paste))
    (pad "" smd rect (at -0.56 0.56 270) (size 0.82 0.82) (layers F.Paste))
    (pad "" smd rect (at 0.56 0.56 270) (size 0.82 0.82) (layers F.Paste))
    (pad 14 smd rect (at 0.75 -1.725 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 13 smd rect (at 1.725 -1 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 20 /IO23))
    (pad 12 smd rect (at 1.725 -0.5 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 8 /IO9))
    (pad 11 smd rect (at 1.725 0 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 45 /IO9_H))
    (pad 10 smd rect (at 1.725 0.5 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 20 /IO23))
    (pad 9 smd rect (at 1.725 1 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 9 /IO8))
    (pad 8 smd rect (at 0.75 1.725 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 46 /IO8_H))
    (pad 7 smd rect (at -0.75 1.725 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1.725 1 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 31 /DIN))
    (pad 5 smd rect (at -1.725 0.5 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 10 /IO7))
    (pad 4 smd rect (at -1.725 0 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 20 /IO23))
    (pad 3 smd rect (at -1.725 -0.5 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 29 /IO6_H))
    (pad 2 smd rect (at -1.725 -1 270) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask)
      (net 11 /IO6))
    (pad 1 smd rect (at -0.75 -1.725 270) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 20 /IO23))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 44.1325 67.818)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 1.397) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 28.2575 41.275 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 2.3114 -0.0127 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.335 -1.4975 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 5DC900FD)
    (at 43.18 37.084)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (zone_connect 2)
    (fp_text reference J11 (at 4.318 -2.0955) (layer F.SilkS))
    (fp_text value Conn_02x04_Odd_Even (at 12.83 2.396 180) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3) (zone_connect 2))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducial:Fiducial_0.5mm_Mask1mm (layer F.Cu) (tedit 5C18CB26)
    (at 48.3235 64.7065)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID2 (at 0 -2.3495 90) (layer F.SilkS))
    (fp_text value FIDUCIAL_1MM (at 7.0165 0.3535) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (module Fiducial:Fiducial_0.5mm_Mask1mm (layer F.Cu) (tedit 5C18CB26)
    (at 24.1935 32.766)
    (descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
    (tags fiducial)
    (attr smd)
    (fp_text reference FID1 (at -1.2827 -0.0508) (layer F.SilkS))
    (fp_text value FIDUCIAL_1MM (at -5.1535 -1.856) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 0.5 0.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.25) (clearance 0.25))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5DD51B11)
    (at 30.48 34.544 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (zone_connect 2)
    (fp_text reference J12 (at 1.406 -2.07 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at -2.604 0.43 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_WS2813-mini:LED_WS2813-MINI-2 (layer F.Cu) (tedit 5D184666)
    (at 29.2735 46.0375 90)
    (attr smd)
    (fp_text reference D1 (at 2.9083 1.1557 180) (layer F.SilkS))
    (fp_text value WS2813-MINI (at 1.0625 -2.2485 90) (layer F.Fab))
    (pad 6 smd rect (at 1.5 -1.1 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.5 0 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.5 1.1 270) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /DIN))
    (pad 3 smd rect (at -1.5 1.1 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /DO))
    (pad 2 smd rect (at -1.5 0 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -1.5 -1.1 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model /home/aaronw/kicad/library/aaron/WS2813-MINI--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer F.Cu) (tedit 5DD65BBA)
    (at 21.59 67.564 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (zone_connect 2)
    (fp_text reference J10 (at 1.9304 25.6032 90) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 3.13 6.064 90) (layer F.Fab))
    (fp_text user %R (at 0 16.51 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3) (zone_connect 2))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IO22) (zone_connect 2))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /IO21) (zone_connect 2))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IO20) (zone_connect 2))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /IO19) (zone_connect 2))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /IO18) (zone_connect 2))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 FET_CTL) (zone_connect 2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /DO) (zone_connect 2))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /IO6_H) (zone_connect 2))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /IO9_H) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /IO8_H) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer B.Cu) (tedit 5DD51B04)
    (at 25.4 67.564)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J7 (at 2.325 -5.189 180) (layer B.SilkS))
    (fp_text value Conn_01x14_Male (at -0.22 -25.554 90) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 270) (layer B.Fab))
    (pad 14 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 13 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 12 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 11 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /IO23))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IO22))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /IO21))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IO20))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /IO19))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /IO18))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 FET_CTL))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /IO16))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /IO15))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /IO14))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /IO13))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 5DD51B1E)
    (at 27.94 37.084)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J9 (at -0.3048 2.3368) (layer B.SilkS))
    (fp_text value Conn_01x01_Male (at 2.39 0.056 90) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer B.Cu) (tedit 5DC900CD)
    (at 38.1 67.564 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 2.2352 -6.0452 180) (layer B.SilkS))
    (fp_text value Conn_01x05_Male (at -2.806 -5.89) (layer B.Fab))
    (fp_text user %R (at 0 -5.08) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /ON_OFF))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /Program))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /VBat))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer B.Cu) (tedit 5DC90104)
    (at 40.64 34.544 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J3 (at -2.435 0.019 180) (layer B.SilkS))
    (fp_text value Conn_01x14_Male (at 0.05 -6.656 90) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 270) (layer B.Fab))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /IO12))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /IO11))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /IO10))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /IO9))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /IO8))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /IO7))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /IO6))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /IO5))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IO4))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /IO3))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /IO2))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /IO1))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IO0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 43.942 47.244 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -3.937 -2.2225 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.762 -0.016) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 46.99 47.244)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 1.0668 -2.1336 90) (layer F.SilkS))
    (fp_text value 1uF (at 2.26 0.006) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 37.33 36.36)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.4 0) (layer B.SilkS))
    (fp_text value 1uF (at -2.5555 -0.0445) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 37.33 34.87)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -2.45 -0.25) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PRG (at 38.9 33.3 270) (layer F.SilkS))
  (gr_text U201: (at 24.83 70.99) (layer F.Fab))
  (gr_text GND (at 23.73 67.99 90) (layer F.SilkS))
  (gr_text "F +12 G" (at 32.9 65.8) (layer F.SilkS))
  (gr_text "Neo Teensy" (at 36.5 43.5 90) (layer B.SilkS))
  (gr_text DO (at 23.71 57.45 90) (layer F.SilkS))
  (gr_text 6H (at 23.7236 65.024 90) (layer F.SilkS))
  (gr_text 5H (at 23.7236 62.4332 90) (layer F.SilkS))
  (gr_text 0H (at 23.7236 59.8932 90) (layer F.SilkS))
  (gr_text 17 (at 23.7744 54.864 90) (layer F.SilkS))
  (gr_text 18 (at 23.7236 52.2732 90) (layer F.SilkS))
  (gr_text 19 (at 23.7236 49.6824 90) (layer F.SilkS))
  (gr_text 20 (at 23.7744 47.1932 90) (layer F.SilkS))
  (gr_text 21 (at 23.7744 44.6532 90) (layer F.SilkS))
  (gr_text 22 (at 23.7236 42.164 90) (layer F.SilkS))
  (gr_text 3V (at 23.7236 39.5732 90) (layer F.SilkS))
  (gr_text GND (at 23.7236 36.9824 90) (layer F.SilkS))
  (gr_text +5 (at 23.7744 34.3916 90) (layer F.SilkS))
  (gr_text "GND +5" (at 29.3116 32.512) (layer F.SilkS))
  (gr_text G (at 42.3672 34.798) (layer F.SilkS))
  (gr_text "+5\n+5\n+5\n+3" (at 48.1076 39.2684) (layer F.SilkS))
  (gr_line (start 19.05 69.85) (end 19.05 31.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.53 69.85) (end 19.05 69.85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.53 31.75) (end 49.53 69.85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 19.05 31.75) (end 49.53 31.75) (layer Edge.Cuts) (width 0.05))
  (gr_text CC (at 47.1805 34.1884) (layer B.SilkS))
  (gr_text "Revision 3.3.0" (at 48.075 41.325 90) (layer B.SilkS))
  (gr_text "NeoPixel Driver Board\n© 2020 by Aaron Williams\nDesigned for Teensy 4.0 and 3.2" (at 29.25 49.7 90) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.059146 31.75) (xy 49.539146 31.75) (xy 49.539146 69.85) (xy 19.059146 69.85)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.05 31.75) (xy 49.53 31.75) (xy 49.53 69.85) (xy 19.05 69.85)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49.53 69.85) (xy 19.06 69.85) (xy 19.05 31.75) (xy 49.53 31.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49.55 69.85) (xy 19.05 69.85) (xy 19.05 31.75) (xy 49.55 31.75)
      )
    )
  )
)
