<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160.02" y2="24.13" width="0" layer="20"/>
<wire x1="160.02" y1="24.13" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.556" y="5.5499" drill="2.75"/>
<hole x="3.556" y="94.4499" drill="2.75"/>
<text>Young Lab</text>
<text>Due Module</text>
<text>V.1.0</text>
<text>Ultra-Precise Modular System</text>
<text>James Ehrets II</text>
<text>Carlos Kometter</text>
</plain>
<libraries>
<library name="con-vg">
<description>&lt;b&gt;VG Connectors (DIN 41612/DIN 41617)&lt;/b&gt;&lt;p&gt;
The library contains devices which allow to place the contacts individually or 
in one or several blocks.&lt;p&gt;
This behavior is indicated by the key words &lt;i&gt;single&lt;/i&gt; and &lt;i&gt;block&lt;/i&gt; in
the respective device descriptions.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MABC96L">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
male, 96 pins, type C, rows ABC, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="arduino_due_shield">
<packages>
<package name="ARDUINO_DUE_SHIELD">
</package>
</packages>
</library>
<library name="cap-master">
<description>&lt;b&gt;CAP MASTER! v4.02 - Electrolytic, Film and Tantalum&lt;/b&gt;&lt;br&gt;
&lt;p&gt;This library is a collection of SMD and through hole capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CNP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;small&gt;DISCLAIMER: The author does not warrant that this library is free from error or that it will meet your specific requirements.&lt;/small&gt;&lt;/p&gt;
&lt;author&gt;by Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 05/28/2005 - Rev 4.02&lt;/author&gt;&lt;br&gt;&lt;br&gt;</description>
<packages>
<package name="0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt;&lt;p&gt;
0603, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUINO_DUE1" library="arduino_due_shield" package="ARDUINO_DUE_SHIELD" value=""/>
<element name="X1" library="con-vg" package="MABC96L" value="MABC96L"/>
<element name="C1" library="cap-master" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="cap-master" package="0603" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="adafruit" package="C1210" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="adafruit" package="C1210" value="10uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="DGND">
<contactref element="X1" pad="C4"/>
<contactref element="X1" pad="B7"/>
<contactref element="X1" pad="A10"/>
<contactref element="X1" pad="C12"/>
<contactref element="X1" pad="B15"/>
<contactref element="X1" pad="A18"/>
<contactref element="X1" pad="C20"/>
<contactref element="X1" pad="B23"/>
<contactref element="X1" pad="A26"/>
<contactref element="X1" pad="A29"/>
<contactref element="X1" pad="B29"/>
<contactref element="X1" pad="C29"/>
<contactref element="X1" pad="A30"/>
<contactref element="X1" pad="B30"/>
<contactref element="X1" pad="C30"/>
<contactref element="X1" pad="A31"/>
<contactref element="X1" pad="B31"/>
<contactref element="X1" pad="C31"/>
<contactref element="X1" pad="A32"/>
<contactref element="X1" pad="B32"/>
<contactref element="X1" pad="C32"/>
<contactref element="X1" pad="A25"/>
<contactref element="X1" pad="B25"/>
<contactref element="X1" pad="C25"/>
<contactref element="ARDUINO_DUE1" pad="GND_5"/>
<contactref element="ARDUINO_DUE1" pad="GND_3"/>
<contactref element="ARDUINO_DUE1" pad="GND_2"/>
<contactref element="ARDUINO_DUE1" pad="GND_4"/>
<contactref element="ARDUINO_DUE1" pad="GND"/>
<contactref element="ARDUINO_DUE1" pad="GND_1"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="SDO">
<contactref element="X1" pad="B2"/>
<contactref element="ARDUINO_DUE1" pad="MISO"/>
</signal>
<signal name="SDIN">
<contactref element="X1" pad="C1"/>
<contactref element="ARDUINO_DUE1" pad="MOSI"/>
</signal>
<signal name="SCLK">
<contactref element="X1" pad="B1"/>
<contactref element="ARDUINO_DUE1" pad="SPCK"/>
</signal>
<signal name="SDO1">
</signal>
<signal name="SYNC[1]1">
</signal>
<signal name="5V1">
</signal>
<signal name="SDO_CON[1]1">
</signal>
<signal name="SCLK_CON[1]1">
</signal>
<signal name="LDAC_CON[1]1">
</signal>
<signal name="SDO2">
</signal>
<signal name="SYNC[1]2">
</signal>
<signal name="5V2">
</signal>
<signal name="SDO_CON[1]2">
</signal>
<signal name="SDO3">
</signal>
<signal name="SYNC[1]3">
</signal>
<signal name="5V3">
</signal>
<signal name="SDO_CON[1]3">
</signal>
<signal name="SYNC_CON[1]1">
</signal>
<signal name="N$20">
</signal>
<signal name="+15V1">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="+REF_10V[1]1">
</signal>
<signal name="-REF_10V[1]1">
</signal>
<signal name="+15V2">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="+REF_10V[1]2">
</signal>
<signal name="-REF_10V[1]2">
</signal>
<signal name="+15V3">
</signal>
<signal name="N$37">
</signal>
<signal name="N$38">
</signal>
<signal name="N$39">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="+REF_10V[1]3">
</signal>
<signal name="-REF_10V[1]3">
</signal>
<signal name="VCC1">
</signal>
<signal name="+15V4">
</signal>
<signal name="+REF_10V[1]4">
</signal>
<signal name="-REF_10V[1]4">
</signal>
<signal name="VREFPS[1]1">
</signal>
<signal name="VREFPF[1]1">
</signal>
<signal name="VREFNF[1]1">
</signal>
<signal name="VOUT[1]1">
</signal>
<signal name="VOUT_BUF[1]1">
</signal>
<signal name="VCC2">
</signal>
<signal name="+15V5">
</signal>
<signal name="-15V1">
</signal>
<signal name="+REF_10V[1]5">
</signal>
<signal name="VREFNS[1]1">
</signal>
<signal name="VREFPS[1]2">
</signal>
<signal name="VREFPF[1]2">
</signal>
<signal name="VREFNF[1]2">
</signal>
<signal name="VOUT[1]2">
</signal>
<signal name="INV[1]1">
</signal>
<signal name="VOUT_BUF[1]2">
</signal>
<signal name="VCC3">
</signal>
<signal name="+15V6">
</signal>
<signal name="-15V2">
</signal>
<signal name="+REF_10V[1]6">
</signal>
<signal name="-REF_10V[1]6">
</signal>
<signal name="VREFNS[1]2">
</signal>
<signal name="VREFPS[1]3">
</signal>
<signal name="VREFPF[1]3">
</signal>
<signal name="VREFNF[1]3">
</signal>
<signal name="VOUT[1]3">
</signal>
<signal name="INV[1]2">
</signal>
<signal name="VOUT_BUF[1]3">
</signal>
<signal name="!SYNCA!8">
<contactref element="X1" pad="A1"/>
<contactref element="ARDUINO_DUE1" pad="53"/>
</signal>
<signal name="!RDY!/!SYNCB!8">
<contactref element="X1" pad="A2"/>
<contactref element="ARDUINO_DUE1" pad="51"/>
</signal>
<signal name="!LDAC!">
<contactref element="X1" pad="C2"/>
<contactref element="ARDUINO_DUE1" pad="52"/>
</signal>
<signal name="IDA8">
<contactref element="X1" pad="A3"/>
<contactref element="ARDUINO_DUE1" pad="50"/>
</signal>
<signal name="IDB8">
<contactref element="X1" pad="B3"/>
<contactref element="ARDUINO_DUE1" pad="48"/>
</signal>
<signal name="IOA8">
<contactref element="X1" pad="C3"/>
<contactref element="ARDUINO_DUE1" pad="49"/>
</signal>
<signal name="IOB8">
<contactref element="X1" pad="A4"/>
<contactref element="ARDUINO_DUE1" pad="47"/>
</signal>
<signal name="IOC8">
<contactref element="X1" pad="B4"/>
<contactref element="ARDUINO_DUE1" pad="46"/>
</signal>
<signal name="!SYNCA!7">
<contactref element="X1" pad="A5"/>
<contactref element="ARDUINO_DUE1" pad="45"/>
</signal>
<signal name="!RDY!/!SYNCB!7">
<contactref element="X1" pad="B5"/>
<contactref element="ARDUINO_DUE1" pad="43"/>
</signal>
<signal name="IDA7">
<contactref element="X1" pad="C5"/>
<contactref element="ARDUINO_DUE1" pad="44"/>
</signal>
<signal name="IDB7">
<contactref element="X1" pad="A6"/>
<contactref element="ARDUINO_DUE1" pad="42"/>
</signal>
<signal name="IOA7">
<contactref element="X1" pad="B6"/>
<contactref element="ARDUINO_DUE1" pad="40"/>
</signal>
<signal name="IOB7">
<contactref element="X1" pad="C6"/>
<contactref element="ARDUINO_DUE1" pad="41"/>
</signal>
<signal name="IOC7">
<contactref element="X1" pad="A7"/>
<contactref element="ARDUINO_DUE1" pad="39"/>
</signal>
<signal name="!SYNCA!6">
<contactref element="X1" pad="C7"/>
<contactref element="ARDUINO_DUE1" pad="38"/>
</signal>
<signal name="!RDY!/!SYNCB!6">
<contactref element="X1" pad="A8"/>
<contactref element="ARDUINO_DUE1" pad="37"/>
</signal>
<signal name="IDA6">
<contactref element="X1" pad="B8"/>
<contactref element="ARDUINO_DUE1" pad="35"/>
</signal>
<signal name="IDB6">
<contactref element="X1" pad="C8"/>
<contactref element="ARDUINO_DUE1" pad="36"/>
</signal>
<signal name="IOA6">
<contactref element="X1" pad="A9"/>
<contactref element="ARDUINO_DUE1" pad="34"/>
</signal>
<signal name="IOB6">
<contactref element="X1" pad="B9"/>
<contactref element="ARDUINO_DUE1" pad="32"/>
</signal>
<signal name="IOC6">
<contactref element="X1" pad="C9"/>
<contactref element="ARDUINO_DUE1" pad="33"/>
</signal>
<signal name="!SYNCA!5">
<contactref element="X1" pad="B10"/>
<contactref element="ARDUINO_DUE1" pad="30"/>
</signal>
<signal name="!RDY!/!SYNCB!5">
<contactref element="X1" pad="C10"/>
<contactref element="ARDUINO_DUE1" pad="31"/>
</signal>
<signal name="IDA5">
<contactref element="X1" pad="A11"/>
<contactref element="ARDUINO_DUE1" pad="29"/>
</signal>
<signal name="IDB5">
<contactref element="X1" pad="B11"/>
<contactref element="ARDUINO_DUE1" pad="27"/>
</signal>
<signal name="IOA5">
<contactref element="X1" pad="C11"/>
<contactref element="ARDUINO_DUE1" pad="28"/>
</signal>
<signal name="IOB5">
<contactref element="X1" pad="A12"/>
<contactref element="ARDUINO_DUE1" pad="26"/>
</signal>
<signal name="IOC5">
<contactref element="X1" pad="B12"/>
<contactref element="ARDUINO_DUE1" pad="25"/>
</signal>
<signal name="!SYNCA!4">
<contactref element="X1" pad="A13"/>
<contactref element="ARDUINO_DUE1" pad="24"/>
</signal>
<signal name="!RDY!/!SYNCB!4">
<contactref element="X1" pad="B13"/>
<contactref element="ARDUINO_DUE1" pad="22"/>
</signal>
<signal name="IDA4">
<contactref element="X1" pad="C13"/>
<contactref element="ARDUINO_DUE1" pad="23"/>
</signal>
<signal name="IDB4">
<contactref element="X1" pad="A14"/>
<contactref element="ARDUINO_DUE1" pad="2"/>
</signal>
<signal name="IOA4">
<contactref element="X1" pad="B14"/>
<contactref element="ARDUINO_DUE1" pad="4"/>
</signal>
<signal name="IOB4">
<contactref element="X1" pad="C14"/>
<contactref element="ARDUINO_DUE1" pad="3"/>
</signal>
<signal name="IOC4">
<contactref element="X1" pad="A15"/>
<contactref element="ARDUINO_DUE1" pad="5"/>
</signal>
<signal name="!SYNCA!3">
<contactref element="X1" pad="C15"/>
<contactref element="ARDUINO_DUE1" pad="6"/>
</signal>
<signal name="!RDY!/!SYNCB!3">
<contactref element="X1" pad="A16"/>
<contactref element="ARDUINO_DUE1" pad="7"/>
</signal>
<signal name="IDA3">
<contactref element="X1" pad="B16"/>
<contactref element="ARDUINO_DUE1" pad="9"/>
</signal>
<signal name="IDB3">
<contactref element="X1" pad="C16"/>
<contactref element="ARDUINO_DUE1" pad="8"/>
</signal>
<signal name="IOA3">
<contactref element="X1" pad="A17"/>
<contactref element="ARDUINO_DUE1" pad="10"/>
</signal>
<signal name="IOB3">
<contactref element="X1" pad="B17"/>
<contactref element="ARDUINO_DUE1" pad="12"/>
</signal>
<signal name="IOC3">
<contactref element="X1" pad="C17"/>
<contactref element="ARDUINO_DUE1" pad="11"/>
</signal>
<signal name="!SYNCA!2">
<contactref element="X1" pad="B18"/>
</signal>
<signal name="!RDY!/!SYNCB!2">
<contactref element="X1" pad="C18"/>
</signal>
<signal name="IDA2">
<contactref element="X1" pad="A19"/>
</signal>
<signal name="IDB2">
<contactref element="X1" pad="B19"/>
</signal>
<signal name="IOA2">
<contactref element="X1" pad="C19"/>
</signal>
<signal name="IOB2">
<contactref element="X1" pad="A20"/>
</signal>
<signal name="IOC2">
<contactref element="X1" pad="B20"/>
</signal>
<signal name="!SYNCA!1">
<contactref element="X1" pad="A21"/>
</signal>
<signal name="!RDY!/!SYNCB!1">
<contactref element="X1" pad="B21"/>
</signal>
<signal name="IDA1">
<contactref element="X1" pad="C21"/>
</signal>
<signal name="IDB1">
<contactref element="X1" pad="A22"/>
</signal>
<signal name="IOA1">
<contactref element="X1" pad="B22"/>
</signal>
<signal name="IOB1">
<contactref element="X1" pad="C22"/>
</signal>
<signal name="IOC1">
<contactref element="X1" pad="A23"/>
</signal>
<signal name="!SYNCA!0">
<contactref element="X1" pad="C23"/>
</signal>
<signal name="!RDY!/!SYNCB!0">
<contactref element="X1" pad="A24"/>
</signal>
<signal name="IDA0">
<contactref element="X1" pad="B24"/>
</signal>
<signal name="IDB0">
<contactref element="X1" pad="C24"/>
</signal>
<signal name="DVDD">
<contactref element="X1" pad="B26"/>
<contactref element="X1" pad="C26"/>
<contactref element="X1" pad="A27"/>
<contactref element="X1" pad="B27"/>
<contactref element="X1" pad="C27"/>
<contactref element="X1" pad="A28"/>
<contactref element="X1" pad="B28"/>
<contactref element="X1" pad="C28"/>
<contactref element="ARDUINO_DUE1" pad="5V0"/>
<contactref element="ARDUINO_DUE1" pad="5V0_2"/>
<contactref element="ARDUINO_DUE1" pad="5V0_1"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="ARDUINO_DUE1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
