(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 339)
    (zones 0)
    (modules 23)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.508)
    (user_via 1.016 0.508)
    (user_via 1.524 0.762)
    (user_via 2.032 1.016)
    (user_via 2.032 1.524)
    (user_via 2.54 1.524)
    (user_via 2.54 2.032)
    (uvia_size 2)
    (uvia_drill 1)
    (uvias_allowed no)
    (uvia_min_size 1)
    (uvia_min_drill 1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VDD)
  (net 2 /5VA)
  (net 3 "Net-(D1-Pad2)")
  (net 4 /VIN)
  (net 5 /SCLK)
  (net 6 /SDO)
  (net 7 /CS)
  (net 8 /LATCH)
  (net 9 /SIG_IN)
  (net 10 GND)
  (net 11 VCC)
  (net 12 /PD)
  (net 13 "Net-(R3-Pad2)")
  (net 14 "Net-(J1-Pad6)")
  (net 15 "Net-(J2-Pad1)")
  (net 16 "Net-(J2-Pad4)")
  (net 17 "Net-(R2-Pad3)")
  (net 18 "Net-(U1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 2)
    (uvia_drill 1)
    (add_net /5VA)
    (add_net /CS)
    (add_net /LATCH)
    (add_net /PD)
    (add_net /SCLK)
    (add_net /SDO)
    (add_net /SIG_IN)
    (add_net /VDD)
    (add_net /VIN)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(R2-Pad3)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net VCC)
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 135.636 99.695)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U2 (at 0 2.3622) (layer B.SilkS))
    (fp_text value OPA355NA (at 0 -2.9) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 5 smd rect (at 1.35 0) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (pad 6 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (pad 4 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 12 /PD))
    (pad 3 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 9 /SIG_IN))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SHDR8W60P254_2X4_1016X508X850P (layer F.Cu) (tedit 5DCDE698)
    (at 156.337 101.854)
    (descr 2214S-8)
    (tags Connector)
    (fp_text reference J2 (at 7.62 -4.699) (layer F.SilkS))
    (fp_text value 2214S-08SG-85 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SDO))
    (pad 4 thru_hole circle (at 2.54 -2.54 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 8 /LATCH))
    (pad 6 thru_hole circle (at 5.08 -2.54 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCLK))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 11 VCC))
    (pad 8 thru_hole circle (at 7.62 -2.54 90) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 11 VCC))
  )
  (module Connectors:Pin_d1.0mm_L10.0mm (layer F.Cu) (tedit 59B3E075)
    (at 153.162 101.092)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference CS (at 0 -2.286) (layer F.SilkS))
    (fp_text value TEST (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /CS))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 146.05 95.885 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0.0762 -1.8796 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 134.366 93.472 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -1.524 -1.778 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /5VA))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 138.811 100.457 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0.0254 -1.7526) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 146.05 92.964 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0.762 2.286 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /VIN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 155.067 93.218 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 164.211 95.123 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.54 0.381 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SOT95P280X145-6N (layer B.Cu) (tedit 5DCDE667)
    (at 148.971 95.885)
    (descr "DBV (R-PDSO-G6)")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 0 -2.667) (layer B.SilkS))
    (fp_text value ADS7886SDBVT (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.25 0.95 270) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (pad 2 smd rect (at -1.25 0 270) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -1.25 -0.95 270) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 /VIN))
    (pad 4 smd rect (at 1.25 -0.95 270) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCLK))
    (pad 5 smd rect (at 1.25 0 270) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 /SDO))
    (pad 6 smd rect (at 1.25 0.95 270) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 /CS))
    (model "C:/Users/Jonathan Chandler/Documents/SamacSys_PCB_Library/KiCad/3D_Models/ADS7886SDBVT.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SHDR8W60P254_2X4_1016X508X850P (layer F.Cu) (tedit 5DCDE698)
    (at 131.445 99.314 90)
    (descr 2214S-8)
    (tags Connector)
    (fp_text reference J1 (at 7.493 2.667 180) (layer F.SilkS))
    (fp_text value 2214S-08SG-85 (at 0 0 90) (layer F.SilkS) hide)
    (pad 8 thru_hole circle (at 7.62 -2.54 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 2 /5VA))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 2 /5VA))
    (pad 6 thru_hole circle (at 5.08 -2.54 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SIG_IN))
    (pad 4 thru_hole circle (at 2.54 -2.54 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 156.337 96.012 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.0254 1.397 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCLK))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:TC33X-2_1 (layer F.Cu) (tedit 5DCD0946)
    (at 142.24 95.504)
    (descr TC33X-2_1)
    (tags Resistor)
    (attr smd)
    (fp_text reference R2 (at -3.175 0.209) (layer F.SilkS))
    (fp_text value TC33X-2-101E (at -0.337 0.209) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1 1.7 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /PD))
    (pad 2 smd rect (at 0 -1.55 90) (size 1.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /VIN))
    (pad 3 smd rect (at 1 1.7 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R2-Pad3)"))
    (model C:/SamacSys_PCB_Library/KiCad/SamacSys_Parts.3dshapes/TC33X-2-101E.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 161.036 91.313)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.921 0) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 /CS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 144.6784 92.837 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.143 -2.286 180) (layer F.SilkS))
    (fp_text value 1M (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 158.496 92.202 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.397 -1.651) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 VCC))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d1.0mm_L10.0mm (layer F.Cu) (tedit 59B3E075)
    (at 150.114 101.092)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference VIN (at 0 -2.286) (layer F.SilkS))
    (fp_text value TEST (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d1.0mm_L10.0mm (layer F.Cu) (tedit 59B3E075)
    (at 147.066 101.092)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference VDD (at 0 -2.286) (layer F.SilkS))
    (fp_text value TEST (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VDD))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d1.0mm_L10.0mm (layer F.Cu) (tedit 59B3E075)
    (at 144.018 100.965)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (fp_text reference PD (at 0.127 -2.159) (layer F.SilkS))
    (fp_text value TEST (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 /PD))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d1.0mm_L10.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 137.414 94.361)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at 1.651 -2.54) (layer B.SilkS))
    (fp_text value LP5907MFX-3.3 (at 0 -2.9) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 /5VA))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 /5VA))
    (pad 4 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 /VDD))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 161.544 96.901 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.7432 -0.1778) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /LATCH))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 135.636 99.822 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D1 (at 0 -1.778) (layer F.SilkS))
    (fp_text value BAT_63-02V_H6327 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /PD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Jonathan Chandler/Documents/SamacSys_PCB_Library/KiCad/3D_Models/BAT_63-02V_H6327.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Jonathan Chandler/Documents/SamacSys_PCB_Library/KiCad/3D_Models/BAT_63-02V_H6327.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 161.036 94.234)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U3 (at 0 2.9) (layer B.SilkS))
    (fp_text value 74LVC1G240 (at 0 -2.9) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 5 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 11 VCC))
    (pad 4 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 /LATCH))
    (pad 1 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ADC Mezzanine 0.5" (at 135.128 102.362) (layer F.SilkS))
  (gr_text 1 (at 154.686 102.108) (layer F.SilkS))
  (gr_text 1 (at 133.477 99.314) (layer F.SilkS))
  (gr_line (start 165.862 89.789) (end 165.862 103.251) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.381 89.789) (end 165.862 89.789) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.381 103.251) (end 127.381 89.789) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.862 103.251) (end 127.381 103.251) (layer Edge.Cuts) (width 0.15))
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 127.762 90.17) (xy 127.762 102.87) (xy 165.481 102.87) (xy 165.481 90.20175)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 127.762 90.17) (xy 127.762 102.87) (xy 165.481 102.87) (xy 165.481 90.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.336 94.618072) (xy 148.336 89.792072) (xy 148.082 89.792072) (xy 148.082 94.618072)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.336 103.251) (xy 148.336 97.155) (xy 148.082 97.155) (xy 148.082 103.251)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 136.11225 98.044) (xy 136.11225 99.441) (xy 135.15975 99.441) (xy 135.15975 98.044)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 133.477 101.092) (xy 135.128 101.092) (xy 135.128 100.203) (xy 133.477 100.203)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 136.144 98.298) (xy 137.795 98.298) (xy 137.795 99.187) (xy 136.144 99.187)
      )
    )
  )
)
