(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 34)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 FLAT_TX_AUDIO_INPUT)
  (net 3 SPKR-)
  (net 4 PTT)
  (net 5 SQL_COR)
  (net 6 RSSI)
  (net 7 FLAT_RX_AUDIO)
  (net 8 PIN2)
  (net 9 PIN4)
  (net 10 PIN6)
  (net 11 PIN12)
  (net 12 PIN14)
  (net 13 PIN16)
  (net 14 PIN9)
  (net 15 PIN13)
  (net 16 +12V)
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net FLAT_RX_AUDIO)
    (add_net FLAT_TX_AUDIO_INPUT)
    (add_net GND)
    (add_net PIN12)
    (add_net PIN13)
    (add_net PIN14)
    (add_net PIN16)
    (add_net PIN2)
    (add_net PIN4)
    (add_net PIN6)
    (add_net PIN9)
    (add_net PTT)
    (add_net RSSI)
    (add_net SPKR-)
    (add_net SQL_COR)
  )
  (module Connectors_JST:JST_XH_S06B-XH-A_06x2.50mm_Angled (layer F.Cu) (tedit 5E5F9971)
    (at 161.156 60.96)
    (descr "JST XH series connector, S06B-XH-A, side entry type, through hole")
    (tags "connector jst xh tht side horizontal angled 2.50mm")
    (fp_text reference J2 (at -1.009 -4.1275) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Male (at 6.25 10.3) (layer F.Fab))
    (fp_text user %R (at -0.0565 -1.905) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 12.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 RSSI))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 FLAT_RX_AUDIO))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 FLAT_TX_AUDIO_INPUT))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 SQL_COR))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 PTT))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Connectors_JST.3dshapes/JST_XH_S06B-XH-A_06x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module oe7mbt:conn_02x08_liegend (layer F.Cu) (tedit 5CAF65E9)
    (at 162.814 51.562)
    (fp_text reference J1 (at -2.54 4.826) (layer F.SilkS) hide)
    (fp_text value GM3XX (at 2.286 2.54) (layer F.Fab))
    (fp_text user 1 (at -2.794 4.826 180) (layer B.SilkS))
    (fp_text user 16 (at 14.986 4.826 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.794 2.032) (size 1.524 4) (layers *.Mask B.Cu B.Paste)
      (net 3 SPKR-))
    (pad 2 smd rect (at -2.794 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 8 PIN2))
    (pad 4 smd rect (at -0.254 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 9 PIN4))
    (pad 6 smd rect (at 2.286 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 10 PIN6))
    (pad 8 smd rect (at 4.826 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 5 SQL_COR))
    (pad 10 smd rect (at 7.366 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 16 +12V))
    (pad 12 smd rect (at 9.906 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 11 PIN12))
    (pad 14 smd rect (at 12.446 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 12 PIN14))
    (pad 16 smd rect (at 14.986 2.032) (size 1.524 4) (layers F.Cu F.Paste F.Mask)
      (net 13 PIN16))
    (pad 3 smd rect (at -0.254 2.032) (size 1.524 4) (layers B.Cu B.Paste B.Mask)
      (net 4 PTT))
    (pad 5 smd rect (at 2.286 2.032) (size 1.524 4) (layers B.Cu B.Paste B.Mask)
      (net 2 FLAT_TX_AUDIO_INPUT))
    (pad 7 smd rect (at 4.826 2.032) (size 1.524 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 7.366 2.032) (size 1.524 4) (layers B.Cu B.Paste B.Mask)
      (net 14 PIN9))
    (pad 11 smd rect (at 9.906 2.032) (size 1.524 4) (layers B.Cu B.Paste B.Mask)
      (net 7 FLAT_RX_AUDIO))
    (pad 13 smd rect (at 12.446 2.032) (size 1.524 4) (layers B.Cu B.Paste B.Mask)
      (net 15 PIN13))
    (pad 15 smd rect (at 14.986 2.032) (size 1.524 4) (layers B.Cu B.Paste B.Mask)
      (net 6 RSSI))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x08_P2.54mm_Vertical.step
      (offset (xyz -2.8 0.5 -2.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 -90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5E5F9966)
    (at 178.308 59.944)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0.0635 -1.9685) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 -270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +12V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text OE7MBT/2020 (at 165.227 58.928) (layer B.SilkS))
  (gr_line (start 176.784 70.612) (end 157.988 70.612) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 66.04) (end 176.784 70.612) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 51.308) (end 180.34 66.04) (layer Edge.Cuts) (width 0.15))
  (gr_text "GND\n" (at 178.308 64.516) (layer B.SilkS))
  (gr_text +12V (at 178.308 57.912) (layer B.SilkS))
  (gr_line (start 157.988 70.612) (end 157.988 51.308) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.988 51.308) (end 180.34 51.308) (layer Edge.Cuts) (width 0.15))
  (gr_text RSSI (at 173.736 67.056 270) (layer B.SilkS))
  (gr_text "RX A" (at 171.196 67.056 270) (layer B.SilkS))
  (gr_text "TX A" (at 168.656 67.056 270) (layer B.SilkS))
  (gr_text SQL (at 166.116 66.548 270) (layer B.SilkS))
  (gr_text PTT (at 163.576 66.548 270) (layer B.SilkS))
  (gr_text "GND\n" (at 161.036 66.548 270) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.988 70.612) (xy 157.988 51.308) (xy 180.34 51.308) (xy 180.34 70.612)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.988 51.308) (xy 180.34 51.308) (xy 180.34 70.612) (xy 157.988 70.612)
      )
    )
  )
)
