(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 22)
    (zones 0)
    (modules 22)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.254)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 1.27)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BR1-Pad+)")
  (net 2 "Net-(BR1-PadAC1)")
  (net 3 "Net-(BR1-PadAC2)")
  (net 4 Earth)
  (net 5 "Net-(H1-Pad1)")
  (net 6 "Net-(H2-Pad1)")
  (net 7 "Net-(H3-Pad1)")
  (net 8 "Net-(H4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 1.27)
    (trace_width 0.508)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(BR1-Pad+)")
    (add_net "Net-(BR1-PadAC1)")
    (add_net "Net-(BR1-PadAC2)")
    (add_net "Net-(H1-Pad1)")
    (add_net "Net-(H2-Pad1)")
    (add_net "Net-(H3-Pad1)")
    (add_net "Net-(H4-Pad1)")
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 214 113)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 8 "Net-(H4-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 214 62)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 "Net-(H3-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 28 113)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 6 "Net-(H2-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 56DDBCCA)
    (at 28 62)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 "Net-(H1-Pad1)"))
  )
  (module GSIB2560-E3-45:DIOB_GSIB2560-E3-45 (layer F.Cu) (tedit 0)
    (at 75 88 90)
    (fp_text reference BR1 (at -12.7 -4.05 90) (layer F.SilkS))
    (fp_text value GSIB2560-E3-45 (at -12.065 4.205 90) (layer F.SilkS))
    (pad + thru_hole rect (at -12.5 0.75 90) (size 2.06 2.06) (drill 1.37) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
    (pad AC1 thru_hole circle (at -2.5 0.75 90) (size 2.06 2.06) (drill 1.37) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
    (pad AC2 thru_hole circle (at 5 0.75 90) (size 2.06 2.06) (drill 1.37) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
    (pad - thru_hole circle (at 12.5 0.75 90) (size 2.06 2.06) (drill 1.37) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module film:QXL2E104KTPT (layer F.Cu) (tedit 0)
    (at 54 94 270)
    (fp_text reference C1 (at -7.5 0 90) (layer F.SilkS))
    (fp_text value ".1uF 250V" (at -7.5 -3.81 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -15.000001 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
  )
  (module film:QXL2E104KTPT (layer F.Cu) (tedit 0)
    (at 111 82 270)
    (fp_text reference C2 (at -7.5 0 90) (layer F.SilkS))
    (fp_text value ".1uF 250V" (at -7.5 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
    (pad 1 thru_hole circle (at -15.000001 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
  )
  (module film:QXL2E104KTPT (layer F.Cu) (tedit 0)
    (at 99 67 90)
    (fp_text reference C3 (at -7.5 0 90) (layer F.SilkS))
    (fp_text value ".1uF 250V" (at -16.51 2.54 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -15.000001 0 90) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module film:QXL2E104KTPT (layer F.Cu) (tedit 0)
    (at 99 92 90)
    (fp_text reference C4 (at -7.5 0 90) (layer F.SilkS))
    (fp_text value ".1uF 250V" (at -7.5 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
    (pad 1 thru_hole circle (at -15.000001 0 90) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
  )
  (module film:QXL2E104KTPT (layer F.Cu) (tedit 0)
    (at 111 107 270)
    (fp_text reference C5 (at -7.5 0 90) (layer F.SilkS))
    (fp_text value ".1uF 250V" (at 5.08 1.27 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -15.000001 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module footprints:UKW1J682MRD (layer F.Cu) (tedit 0)
    (at 171 65 90)
    (fp_text reference C6 (at -6.2484 0 90) (layer F.SilkS))
    (fp_text value "6800uF 63V" (at -6.2484 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 1 thru_hole rect (at -12.4968 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
  )
  (module footprints:UKW1J682MRD (layer F.Cu) (tedit 0)
    (at 139 97 90)
    (fp_text reference C7 (at -6.2484 0 90) (layer F.SilkS))
    (fp_text value "6800uF 63V" (at -6.2484 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -12.4968 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module footprints:UKW1J682MRD (layer F.Cu) (tedit 0)
    (at 139 65 90)
    (fp_text reference C8 (at -6.2484 0 90) (layer F.SilkS))
    (fp_text value "6800uF 63V" (at -6.2484 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 1 thru_hole rect (at -12.4968 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
  )
  (module footprints:UKW1J682MRD (layer F.Cu) (tedit 0)
    (at 171 97 90)
    (fp_text reference C9 (at -6.2484 0 90) (layer F.SilkS))
    (fp_text value "6800uF 63V" (at -6.2484 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -12.4968 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 34 76 90)
    (fp_text reference J1 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 43 76 90)
    (fp_text reference J2 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(BR1-PadAC2)"))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 34.225 97 90)
    (fp_text reference J3 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 43 97 90)
    (fp_text reference J4 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(BR1-PadAC1)"))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 206 75 90)
    (fp_text reference J5 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 213 75 90)
    (fp_text reference J6 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(BR1-Pad+)"))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 213 99 90)
    (fp_text reference J7 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (module footprints2:TE_1217861-1 (layer F.Cu) (tedit 5E520D95)
    (at 206 99 90)
    (fp_text reference J8 (at -1.61889 -2.207614 90) (layer F.SilkS))
    (fp_text value 1217861-1 (at 1.07735 2.294773 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 Earth))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 Earth))
  )
  (gr_text LOL! (at 43 113) (layer F.SilkS))
  (gr_line (start 219 57) (end 23 57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 219 118) (end 219 57) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 23 118) (end 219 118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 23 57) (end 23 118) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name "Net-(BR1-Pad+)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 118) (xy 74 118) (xy 74 57) (xy 219 57)
      )
    )
  )
  (zone (net 4) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 219 118) (xy 74 118) (xy 74 57) (xy 219 57)
      )
    )
  )
)
