(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 74)
    (no_connects 0)
    (area 99.328667 24.2635 132.767143 51.129001)
    (thickness 1.6)
    (drawings 54)
    (tracks 390)
    (zones 0)
    (modules 45)
    (nets 30)
  )
  (page A4)
  (title_block
    (title lpwatch)
    (date 2018-03-05)
    (rev 1)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1)
    (user_trace_width 0.152)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory OUT/gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(D101-Pad2)")
  (net 2 VCC)
  (net 3 GND)
  (net 4 /VCCA)
  (net 5 /PB6)
  (net 6 /PB7)
  (net 7 /PA10)
  (net 8 /PA8)
  (net 9 /PA9)
  (net 10 /PB1)
  (net 11 /PA2)
  (net 12 /PA3)
  (net 13 /PA5)
  (net 14 /PA4)
  (net 15 /PA7)
  (net 16 /PB0)
  (net 17 /PA6)
  (net 18 /PA1)
  (net 19 /PA0)
  (net 20 /NRST)
  (net 21 /SPI1_SCK)
  (net 22 /SPI1_MOSI)
  (net 23 /SPI1_MISO)
  (net 24 /SYS_SWCLK)
  (net 25 /SYS_SWDIO)
  (net 26 /BOOT0)
  (net 27 /OSC32_IN)
  (net 28 /OSC32_OUT)
  (net 29 /SPI1_NSS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /OSC32_IN)
    (add_net /OSC32_OUT)
    (add_net GND)
    (add_net "Net-(D101-Pad2)")
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (net_class PWR_ANALOG ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VCCA)
  )
  (net_class SIG ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BOOT0)
    (add_net /NRST)
    (add_net /PA0)
    (add_net /PA1)
    (add_net /PA10)
    (add_net /PA2)
    (add_net /PA3)
    (add_net /PA4)
    (add_net /PA5)
    (add_net /PA6)
    (add_net /PA7)
    (add_net /PA8)
    (add_net /PA9)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB6)
    (add_net /PB7)
    (add_net /SPI1_MISO)
    (add_net /SPI1_MOSI)
    (add_net /SPI1_NSS)
    (add_net /SPI1_SCK)
    (add_net /SYS_SWCLK)
    (add_net /SYS_SWDIO)
  )
  (module w_smd_leds:Led_0603 (layer F.Cu) (tedit 5A9D2F12)
    (at 127 41.529)
    (descr "SMD LED, 0603")
    (fp_text reference D101 (at 0 -1.0795 180) (layer F.SilkS))
    (fp_text value LED (at 0 -1.905) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /PA8))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D101-Pad2)"))
    (model walter/smd_leds/led_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 5A9D2F06)
    (at 127 42.672 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R101 (at -1.8415 0.0635 450) (layer F.SilkS))
    (fp_text value 470R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D101-Pad2)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 5A9C8FE5)
    (at 116.84 41.529 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C101 (at -2.4765 -0.635 270) (layer F.SilkS))
    (fp_text value 2p7 (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 27 /OSC32_IN))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 5A9C8F8A)
    (at 116.84 43.815 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C102 (at -2.54 1.651 180) (layer F.SilkS))
    (fp_text value 2p7 (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 28 /OSC32_OUT))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0603 (layer F.Cu) (tedit 5A9D4E28)
    (at 114.808 45.4152)
    (descr "Inductor SMD, 0603")
    (fp_text reference L101 (at -1.016 -1.9177 270) (layer F.SilkS))
    (fp_text value INDUCTOR (at -3.556 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.63754 0) (size 0.635 1.016) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.63754 0) (size 0.635 1.016) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCA))
    (model walter/smd_inductors/inductor_smd_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0603 (layer F.Cu) (tedit 5A9CA1B5)
    (at 114.8588 47.498)
    (descr "SMT capacitor, 0603")
    (fp_text reference C110 (at 2.7305 0.6985) (layer F.SilkS))
    (fp_text value 1u (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCA))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 5A9C8FD3)
    (at 123.698 44.45 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C112 (at 0 -1.016 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 5A9CA3B5)
    (at 125.984 44.196 180)
    (descr "SMT capacitor, 0805")
    (fp_text reference C113 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0.9906 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -0.9525 0 180) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 5A9D3581)
    (at 115.062 46.5836)
    (descr "SMT capacitor, 0402")
    (fp_text reference C114 (at 2.9972 0.6604 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCA))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 5A9C9110)
    (at 110.236 47.117 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R119 (at 0.40132 -0.94996 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 /PA4))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 5A9D4E30)
    (at 109.1565 40.0685 90)
    (descr "SMT resistor, 0402")
    (fp_text reference R120 (at 1.5875 0.8255 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 26 /BOOT0))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 5A9C90A9)
    (at 112.268 47.117)
    (descr "SMT capacitor, 0402")
    (fp_text reference C111 (at -0.08636 0.97282) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 14 /PA4))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:UFQFPN28 (layer F.Cu) (tedit 5A9D3998)
    (at 119.634 43.434)
    (fp_text reference U110 (at 1.905 3.2385) (layer F.SilkS))
    (fp_text value STM32L011G4U6 (at 0.24 -4.951) (layer F.Fab) hide)
    (pad 21 smd rect (at 1.7653 -1.4986 45) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 25 /SYS_SWDIO))
    (pad 22 smd rect (at 1.4986 -1.7653 45) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 24 /SYS_SWCLK))
    (pad 14 smd rect (at 1.4986 1.7653 315) (size 0.23 0.15) (layers F.Cu F.Paste F.Mask)
      (net 16 /PB0))
    (pad 15 smd rect (at 1.7653 1.4986 315) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 10 /PB1))
    (pad 7 smd rect (at -1.7653 1.4986 45) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA1))
    (pad 8 smd rect (at -1.4986 1.7653 45) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 11 /PA2))
    (pad 1 smd rect (at -1.7653 -1.4986 315) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 26 /BOOT0))
    (pad 28 smd rect (at -1.4986 -1.7653 315) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB7))
    (pad 21 smd rect (at 1.725 -1.425) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 25 /SYS_SWDIO))
    (pad 22 smd rect (at 1.425 -1.725 90) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 24 /SYS_SWCLK))
    (pad 15 smd rect (at 1.725 1.425) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 10 /PB1))
    (pad 14 smd rect (at 1.425 1.725 90) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 16 /PB0))
    (pad 8 smd rect (at -1.425 1.725 90) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 11 /PA2))
    (pad 7 smd rect (at -1.725 1.425) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA1))
    (pad 1 smd rect (at -1.725 -1.425) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 26 /BOOT0))
    (pad 28 smd rect (at -1.425 -1.725 90) (size 0.2 0.15) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB7))
    (pad 24 smd rect (at 0.5 -1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /SPI1_SCK))
    (pad 22 smd rect (at 1.5 -1.975 90) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /SYS_SWCLK))
    (pad 23 smd rect (at 1 -1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /SPI1_NSS))
    (pad 26 smd rect (at -0.5 -1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /SPI1_MOSI))
    (pad 25 smd rect (at 0 -1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /SPI1_MISO))
    (pad 27 smd rect (at -1 -1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /PB6))
    (pad 28 smd rect (at -1.5 -1.975 90) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB7))
    (pad 21 smd rect (at 1.975 -1.5) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /SYS_SWDIO))
    (pad 20 smd rect (at 1.85 -1) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /PA10))
    (pad 18 smd rect (at 1.85 0) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /PA8))
    (pad 19 smd rect (at 1.85 -0.5) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /PA9))
    (pad 16 smd rect (at 1.85 1) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 15 smd rect (at 1.975 1.5) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /PB1))
    (pad 17 smd rect (at 1.85 0.5) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 8 smd rect (at -1.5 1.975 90) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /PA2))
    (pad 9 smd rect (at -1 1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /PA3))
    (pad 11 smd rect (at 0 1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /PA5))
    (pad 10 smd rect (at -0.5 1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /PA4))
    (pad 13 smd rect (at 1 1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /PA7))
    (pad 14 smd rect (at 1.5 1.975 90) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /PB0))
    (pad 12 smd rect (at 0.5 1.85 90) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /PA6))
    (pad 5 smd rect (at -1.85 0.5) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /VCCA))
    (pad 7 smd rect (at -1.975 1.5) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /PA1))
    (pad 6 smd rect (at -1.85 1) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /PA0))
    (pad 3 smd rect (at -1.85 -0.5) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /OSC32_OUT))
    (pad 4 smd rect (at -1.85 0) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /NRST))
    (pad 2 smd rect (at -1.85 -1) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /OSC32_IN))
    (pad 1 smd rect (at -1.975 -1.5) (size 0.35 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /BOOT0))
  )
  (module mylib:smd_push_mod0 (layer F.Cu) (tedit 5A9C911F)
    (at 111.4425 42.418 90)
    (descr "SMD Pushbutton")
    (autoplace_cost180 10)
    (fp_text reference SW101 (at 1.143 1.143 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 2.79908 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.59918 0 90) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 /PA4))
    (pad 2 smd rect (at 3.59918 0 90) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/switch/smd_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:ABS07AIG (layer F.Cu) (tedit 5A9D4E25)
    (at 115.316 42.3545 270)
    (fp_text reference X101 (at -1.0795 1.524 450) (layer F.SilkS))
    (fp_text value CRYSTAL (at 0.4 2 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.275 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 /OSC32_OUT))
    (pad 1 smd rect (at -1.275 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 /OSC32_IN))
    (model 1rel/Abracon_ABS07AIG-32.768kHz-1-T.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F1C)
    (at 107.95 44.45 180)
    (fp_text reference P101 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F1F)
    (at 107.95 41.91 180)
    (fp_text reference P102 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8ED6)
    (at 118.11 36.83)
    (fp_text reference P103 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 /SPI1_SCK))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EC9)
    (at 110.49 36.83)
    (fp_text reference P104 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /SPI1_MOSI))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8ECD)
    (at 113.03 36.83)
    (fp_text reference P105 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /SPI1_MISO))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EE9)
    (at 125.73 36.83)
    (fp_text reference P106 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 /SYS_SWCLK))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EEF)
    (at 128.27 36.83)
    (fp_text reference P107 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 /SYS_SWDIO))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8FA3)
    (at 123.19 39.37)
    (fp_text reference P108 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /NRST))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EF2)
    (at 130.81 36.83)
    (fp_text reference P111 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EDF)
    (at 123.19 36.83)
    (fp_text reference P112 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EC4)
    (at 107.95 36.83)
    (fp_text reference P113 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 VCC))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EDA)
    (at 120.65 36.83)
    (fp_text reference P114 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F11)
    (at 110.49 49.53)
    (fp_text reference P115 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /PA0))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F0E)
    (at 113.03 49.53)
    (fp_text reference P116 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /PA1))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F0B)
    (at 115.57 49.53)
    (fp_text reference P117 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /PA2))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F06)
    (at 118.11 49.53)
    (fp_text reference P118 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 /PA3))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F03)
    (at 120.65 49.53)
    (fp_text reference P119 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 /PA4))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F00)
    (at 123.19 49.53)
    (fp_text reference P120 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /PA5))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EFE)
    (at 125.73 49.53)
    (fp_text reference P121 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /PA6))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EFB)
    (at 128.27 49.53)
    (fp_text reference P122 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /PA7))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8EF9)
    (at 130.81 49.53)
    (fp_text reference P123 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /PB0))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F2D)
    (at 130.81 46.99 90)
    (fp_text reference P124 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 /PB1))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F2F)
    (at 130.81 44.45 90)
    (fp_text reference P125 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /PA8))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F32)
    (at 130.81 41.91 90)
    (fp_text reference P126 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 /PA9))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F36)
    (at 130.81 39.37 90)
    (fp_text reference P127 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /PA10))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F14)
    (at 107.95 49.53)
    (fp_text reference P128 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /PB6))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F19)
    (at 107.95 46.99)
    (fp_text reference P129 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /PB7))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8F27)
    (at 107.95 39.37)
    (fp_text reference P109 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 /BOOT0))
  )
  (module mylib:pin_2.54 (layer F.Cu) (tedit 5A9C8ECF)
    (at 115.57 36.83)
    (fp_text reference P110 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /SPI1_NSS))
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 5A9D39B9)
    (at 121.539 39.0525 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C103 (at 1.4605 0.4445 540) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 /NRST))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text lpwatch (at 119.38 25.4635) (layer Cmts.User))
  (dimension 25.908 (width 0.1) (layer Dwgs.User)
    (gr_text "25.908 mm" (at 119.126 29.718) (layer Dwgs.User))
    (feature1 (pts (xy 106.426 37.592) (xy 106.426 27.78)))
    (feature2 (pts (xy 132.334 37.592) (xy 132.334 27.78)))
    (crossbar (pts (xy 132.334 30.48) (xy 106.426 30.48)))
    (arrow1a (pts (xy 106.426 30.48) (xy 107.552504 29.893579)))
    (arrow1b (pts (xy 106.426 30.48) (xy 107.552504 31.066421)))
    (arrow2a (pts (xy 132.334 30.48) (xy 131.207496 29.893579)))
    (arrow2b (pts (xy 132.334 30.48) (xy 131.207496 31.066421)))
  )
  (dimension 15.748 (width 0.1) (layer Dwgs.User)
    (gr_text "15.748 mm" (at 102.362 43.18 270) (layer Dwgs.User))
    (feature1 (pts (xy 107.95 51.054) (xy 100.424 51.054)))
    (feature2 (pts (xy 107.95 35.306) (xy 100.424 35.306)))
    (crossbar (pts (xy 103.124 35.306) (xy 103.124 51.054)))
    (arrow1a (pts (xy 103.124 51.054) (xy 102.537579 49.927496)))
    (arrow1b (pts (xy 103.124 51.054) (xy 103.710421 49.927496)))
    (arrow2a (pts (xy 103.124 35.306) (xy 102.537579 36.432504)))
    (arrow2b (pts (xy 103.124 35.306) (xy 103.710421 36.432504)))
  )
  (gr_text USART2 (at 111.1504 44.1452 90) (layer B.SilkS))
  (gr_text SPI1 (at 115.8748 39.7256) (layer B.SilkS))
  (gr_text GND (at 121.92 39.37) (layer B.SilkS))
  (gr_text RX (at 110.236 45.72) (layer B.SilkS))
  (gr_text VCC (at 110.49 38.354) (layer B.SilkS))
  (gr_text PA10 (at 129.794 40.386) (layer B.SilkS))
  (gr_text PA9 (at 129.794 42.164) (layer B.SilkS))
  (gr_text PA8 (at 129.794 43.688) (layer B.SilkS))
  (gr_text PB1 (at 129.794 45.72) (layer B.SilkS))
  (gr_text PB0 (at 130.048 48.006) (layer B.SilkS))
  (gr_text PA7 (at 128.016 48.006) (layer B.SilkS))
  (gr_text PA6 (at 125.984 48.006) (layer B.SilkS))
  (gr_text PA5 (at 123.698 48.006) (layer B.SilkS))
  (gr_text PA4 (at 121.412 48.006) (layer B.SilkS))
  (gr_text PA3 (at 119.126 48.006) (layer B.SilkS))
  (gr_text PA2 (at 116.84 48.006) (layer B.SilkS))
  (gr_text PA1 (at 114.808 48.006) (layer B.SilkS))
  (gr_text PA0 (at 112.649 48.006) (layer B.SilkS))
  (gr_text TX (at 110.236 47.8028) (layer B.SilkS))
  (gr_text VCC (at 110.744 43.688) (layer B.SilkS))
  (gr_text GND (at 110.998 42.164) (layer B.SilkS))
  (gr_text BOOT0 (at 111.76 40.386) (layer B.SilkS))
  (gr_text MOSI (at 112.776 38.354) (layer B.SilkS))
  (gr_text MISO (at 115.062 38.354) (layer B.SilkS))
  (gr_text NSS (at 117.348 38.354) (layer B.SilkS))
  (gr_line (start 106.426 51.054) (end 106.426 35.306) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.334 51.054) (end 106.426 51.054) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.334 35.306) (end 132.334 51.054) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.426 35.306) (end 132.334 35.306) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 122.428 38.354) (layer B.SilkS))
  (gr_text VCC (at 130.048 38.354) (layer B.SilkS))
  (gr_text DIO (at 127.762 38.354) (layer B.SilkS))
  (gr_text CLK (at 125.984 38.354) (layer B.SilkS))
  (gr_text SCK (at 119.634 38.354) (layer B.SilkS))
  (gr_text NRST (at 124.206 40.894) (layer B.SilkS))
  (gr_text "rel/2018-03\nlpwatch rev1\n" (at 127.254 45.212) (layer B.SilkS))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 132.334 51.054) (xy 106.426 51.054) (xy 106.426 35.306) (xy 132.334 35.306)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 132.334 51.054) (xy 106.426 51.054) (xy 106.426 35.306) (xy 132.334 35.306)
      )
    )
  )
)
