(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6002)
    (drawings 22)
    (tracks 9)
    (zones 0)
    (modules 9)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1.4)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.25)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160 100)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00008_00000000)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VCC)
  (net 3 /5V)
  (net 4 /VBus)
  (net 5 /GPIO15)
  (net 6 +3V3)
  (net 7 /SDA)
  (net 8 /SCL)
  (net 9 /GPIO16)
  (net 10 /RST)
  (net 11 "Net-(J2-Pad3)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net /5V)
    (add_net /GPIO15)
    (add_net /GPIO16)
    (add_net /RST)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VBus)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(J2-Pad3)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 5AA5C652)
    (at 192.54 105.08 180)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Expansion (at 1.27 12.49 180) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VBus))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /5V))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SDA))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SCL))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIO15))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO16))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /RST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad locked (layer F.Cu) (tedit 5AA5985C)
    (at 160 70)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad locked (layer F.Cu) (tedit 5AA59862)
    (at 184 118)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad locked (layer F.Cu) (tedit 5AA59869)
    (at 136 118)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 138.791 86.919 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_THT:C_Disc_D6.0mm_W4.4mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 169.144 93.142 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*4.4mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 4.4mm Capacitor")
    (fp_text reference C1 (at 2.5 -3.51 90) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 3.51 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /VCC))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D6.0mm_W4.4mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D6.0mm_W4.4mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 169.144 107.62 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*4.4mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 4.4mm Capacitor")
    (fp_text reference C2 (at 2.54 3.302 270) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 3.51 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D6.0mm_W4.4mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5861378E)
    (at 151.11 79.299 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J2 (at -8.45 5.75 90) (layer F.SilkS))
    (fp_text value 12V (at -6.2 -5.5 270) (layer F.Fab))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad3)"))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 2 /VCC))
  )
  (module adafruit:adafruit-TO220-NOHOLE (layer F.Cu) (tedit 5C1474FD)
    (at 162.794 100.254 90)
    (attr virtual)
    (fp_text reference U1 (at -11.176 -6.096 90) (layer F.SilkS))
    (fp_text value "LD1117S50 TO220" (at 1.397 -3.429 90) (layer F.SilkS) hide)
    (fp_text user A17,5mm (at -0.889 -8.382 90) (layer F.SilkS))
    (fp_text user 1 (at -2.54 -0.635 90) (layer Dwgs.User))
    (fp_text user 2 (at 0 -0.635 90) (layer Dwgs.User))
    (fp_text user 3 (at 2.54 -0.635 90) (layer Dwgs.User))
    (pad 1 thru_hole oval (at -2.54 6.35 270) (size 1.6764 3.3528) (drill 1.1176) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 6.35 270) (size 1.6764 3.3528) (drill 1.1176) (layers *.Cu *.Mask)
      (net 3 /5V))
    (pad 3 thru_hole oval (at 2.54 6.35 270) (size 1.6764 3.3528) (drill 1.1176) (layers *.Cu *.Mask)
      (net 2 /VCC))
  )
  (gr_text SCL (at 194.544 97.333 90) (layer F.SilkS))
  (gr_text SDA (at 194.544 100.381 90) (layer F.SilkS))
  (gr_text 5V (at 194.417 102.667 90) (layer F.SilkS))
  (gr_text VBus (at 193.909 107.239) (layer F.SilkS))
  (gr_text Vcc (at 188.448 105.08) (layer F.SilkS))
  (gr_text 3V3 (at 188.448 102.54) (layer F.SilkS))
  (gr_text GND (at 188.448 100) (layer F.SilkS))
  (gr_text IO15 (at 188.448 97.46) (layer F.SilkS))
  (gr_text RST (at 188.448 94.92) (layer F.SilkS))
  (gr_text IO16 (at 193.655 92.634) (layer F.SilkS))
  (gr_text SCL (at 194.544 97.333 90) (layer B.SilkS))
  (gr_text SDA (at 194.544 100.381 90) (layer B.SilkS))
  (gr_text 5V (at 194.417 102.667 90) (layer B.SilkS))
  (gr_text VBus (at 193.909 107.239) (layer B.SilkS))
  (gr_text IO16 (at 193.655 92.634) (layer B.SilkS))
  (gr_text Vcc (at 188.448 105.08) (layer B.SilkS))
  (gr_text 3V3 (at 188.448 102.54) (layer B.SilkS))
  (gr_text GND (at 188.448 100) (layer B.SilkS))
  (gr_text IO15 (at 188.448 97.46) (layer B.SilkS))
  (gr_text RST (at 188.448 94.92) (layer B.SilkS))
  (gr_text "nixies.us\nOne Tube Clock\n12V Power Adapter" (at 137.267 87.3) (layer B.Mask))
  (gr_circle (center 160 100) (end 195 100) (layer Edge.Cuts) (width 0.127))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (priority 14)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.54 108.89) (xy 134.6 108.89) (xy 134.6 91.11) (xy 162.54 91.11)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.9 61.9) (xy 198.1 61.9) (xy 198.1 138.1) (xy 121.9 138.1)
      )
    )
  )
  (zone (net 2) (net_name /VCC) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.83 63.17) (xy 196.83 136.83) (xy 123.17 136.83) (xy 123.17 63.17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.5 91) (xy 162.5 91) (xy 162.5 109) (xy 134.5 109)
      )
    )
  )
)
