<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="58.4075" y2="0" width="0" layer="20"/>
<wire x1="58.4075" y1="0" x2="58.4075" y2="33.01" width="0" layer="20"/>
<wire x1="58.4075" y1="33.01" x2="0" y2="33.01" width="0" layer="20"/>
<wire x1="0" y1="33.01" x2="0" y2="0" width="0" layer="20"/>
<text>+5V</text>
<text>GND</text>
<text>/OE</text>
<text>LE</text>
<text>DIN</text>
<text>CLK</text>
<text>+5V</text>
<text>GND</text>
<text>/OE</text>
<text>LE</text>
<text>DOUT</text>
<text>CLK</text>
<hole x="55.245" y="29.845" drill="3.2"/>
<hole x="55.245" y="3.175" drill="3.2"/>
<hole x="3.175" y="29.845" drill="3.2"/>
<hole x="3.175" y="3.175" drill="3.2"/>
<text>D. Fisher, 2015/07, LED Driver Rev. A</text>
<text>electronicfish.wordpress.com</text>
<text>IN</text>
<text>OUT</text>
<text>GND</text>
<text>~OE</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL2">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="dfisher">
<packages>
<package name="DIP-24">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="CAP-PTH-SMALL2" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/10" value="760"/>
<element name="U1" library="dfisher" package="DIP-24" value="MAX6971">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT0" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT1" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT2" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT3" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT4" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT5" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT6" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT7" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT8" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT9" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT10" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT11" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT12" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT13" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT14" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT15" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="20"/>
<contactref element="OUT15" pad="K"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="19"/>
<contactref element="OUT14" pad="K"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="18"/>
<contactref element="OUT13" pad="K"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="17"/>
<contactref element="OUT12" pad="K"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="16"/>
<contactref element="OUT11" pad="K"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="15"/>
<contactref element="OUT10" pad="K"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="14"/>
<contactref element="OUT9" pad="K"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="13"/>
<contactref element="OUT8" pad="K"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="12"/>
<contactref element="OUT7" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="11"/>
<contactref element="OUT6" pad="K"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="10"/>
<contactref element="OUT5" pad="K"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="9"/>
<contactref element="OUT4" pad="K"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="8"/>
<contactref element="OUT3" pad="K"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="7"/>
<contactref element="OUT2" pad="K"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="6"/>
<contactref element="OUT1" pad="K"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="5"/>
<contactref element="OUT0" pad="K"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="24"/>
<contactref element="C1" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="OUT0" pad="A"/>
<contactref element="OUT1" pad="A"/>
<contactref element="OUT2" pad="A"/>
<contactref element="OUT3" pad="A"/>
<contactref element="OUT4" pad="A"/>
<contactref element="OUT5" pad="A"/>
<contactref element="OUT6" pad="A"/>
<contactref element="OUT7" pad="A"/>
<contactref element="OUT8" pad="A"/>
<contactref element="OUT9" pad="A"/>
<contactref element="OUT10" pad="A"/>
<contactref element="OUT11" pad="A"/>
<contactref element="OUT12" pad="A"/>
<contactref element="OUT13" pad="A"/>
<contactref element="OUT14" pad="A"/>
<contactref element="OUT15" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="JP3" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="JP3" pad="3"/>
<contactref element="U1" pad="22"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
