(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+12V")
	(net 2 "unconnected-(J1-Pad3)")
	(net 3 "GND")
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 142 80)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TitanPowerOrg:PJ_102ah"
		(layer "F.Cu")
		(at 220.5 85 -90)
		(property "Reference" "J1"
			(at 2.5 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Barrel_Jack_Switch"
			(at -5.5 -2.9 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TitanPowerOrg:PJ_102ah"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Barrel Jack with an internal switch"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -6 2.4 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 2.2 2.8)
			(drill oval 0.6 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -6 0 270)
			(size 2.2 2.8)
			(drill oval 0.6 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -3 4.7 270)
			(size 2.8 2.2)
			(drill oval 1.6 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(J1-Pad3)")
			(pintype "passive+no_connect")
		)
	)
	(footprint "TitanPowerOrg:Molex_398900306"
		(layer "F.Cu")
		(at 175 80 180)
		(property "Reference" "J4"
			(at 0 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x06"
			(at 8.5 -2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TitanPowerOrg:Molex_398900306"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr through_hole)
		(fp_text user "2"
			(at 4.5 3.1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "6"
			(at 24.5 3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at 19.5 3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at 9.5 3.1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4"
			(at 14.5 3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -0.5 3.2 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 21.5 -2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 142 100)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H4"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TitanPowerOrg:Keystone_575"
		(layer "F.Cu")
		(at 197.5 96.5)
		(property "Reference" "J3"
			(at -5.5 4.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TitanPowerOrg:Keystone_575"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.keyelco.com/userAssets/file/M65p111.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Banana Jack Solder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 11 11)
			(drill 5.5)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "power_in")
		)
	)
	(footprint "TitanPowerOrg:Molex_398900306"
		(layer "F.Cu")
		(at 210 80 180)
		(property "Reference" "J5"
			(at 0 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x06"
			(at 8.5 -2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TitanPowerOrg:Molex_398900306"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr through_hole)
		(fp_text user "3"
			(at 9.5 3.1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "6"
			(at 24.5 3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4"
			(at 14.5 3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 4.5 3.1 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at 19.5 3 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -0.5 3.2 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 21.5 -2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 230 80)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 230 100)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "TitanPowerOrg:Keystone_575"
		(layer "F.Cu")
		(at 162.5 97)
		(property "Reference" "J2"
			(at -7 2.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TitanPowerOrg:Keystone_575"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.keyelco.com/userAssets/file/M65p111.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Banana Jack Solder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "TitanOrgPower_Dev_0018.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 11 11)
			(drill 5.5)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pintype "power_in")
		)
	)
	(gr_arc
		(start 138 80)
		(mid 139.171573 77.171573)
		(end 142 76)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 230 76)
		(mid 232.828427 77.171573)
		(end 234 80)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142 104)
		(end 230 104)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 142 104)
		(mid 139.171573 102.828427)
		(end 138 100)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234 100)
		(mid 232.828427 102.828427)
		(end 230 104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 230 76)
		(end 142 76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138 80)
		(end 138 100)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234 100)
		(end 234 80)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 189.5 91 0)
		(layer "F.SilkS")
	)
	(gr_text "+12V"
		(at 151.5 91 0)
		(layer "F.SilkS")
	)
	(gr_text "Titan Organizer\nPower Distribution\nDEV_0018 v. 1"
		(at 174 99.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+12v"
		(at 224 88.5 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "+12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145 103.5) (xy 138.5 97) (xy 138.5 83) (xy 145 76.5) (xy 227 76.5) (xy 233.5 83) (xy 233.5 97)
				(xy 227 103.5)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.5 103) (xy 138.5 97) (xy 138.5 83) (xy 145 76.5) (xy 227 76.5) (xy 233.5 83) (xy 233.5 97)
				(xy 227 103.5) (xy 145 103.5)
			)
		)
	)
)
