<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="48.26" y1="0" x2="48.26" y2="36.83" width="0" layer="20"/>
<wire x1="25.4" y1="12.7" x2="0" y2="12.7" width="0" layer="20"/>
<wire x1="0" y1="12.7" x2="0" y2="0" width="0" layer="20"/>
<text>+an</text>
<text>-cath</text>
<text>out</text>
<wire x1="25.4" y1="36.83" x2="25.4" y2="12.7" width="0" layer="20"/>
<wire x1="48.26" y1="36.83" x2="25.4" y2="36.83" width="0" layer="20"/>
<wire x1="0" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<text>short press=mode</text>
<text>Filament sensor V3.13 Mar 2021</text>
<text>Objects with Intelligence LLC</text>
<text>+an</text>
<text>+ca</text>
<text>+5v</text>
<text>out</text>
<text>gnd</text>
<text>flash=absolute</text>
<text>const=ratiometric</text>
<text>G</text>
<text>D</text>
<text>C</text>
<text>I2C</text>
<text>LED2</text>
<text>long press=calibrate</text>
<text>Pushbutton</text>
<text>LED</text>
<text>USB</text>
<text>I2C</text>
<text>sda</text>
<text>G</text>
<text>scl</text>
<text>LED</text>
<text>Power</text>
<text>gnd</text>
<text>+5v</text>
<text>Filament Sensor V4
Filip Mulier
Objects with Intelligence LLC
License:
Creative Commons-Attribution-NonCommercial</text>
</plain>
<libraries>
<library name="filip">
<packages>
<package name="MA03-2SMT">
</package>
<package name="SCREWHOLE2-56">
<description>2-56 screw hole</description>
</package>
<package name="1X02_2.54_SCREWTERM">
</package>
<package name="1X03_2.54_SCREWTERM">
</package>
<package name="MCP6001_SC70-5">
</package>
<package name="SO16NBC">
<description>MLX75306 image sensor package.  Line indicate optical sensor</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="cap-master">
<packages>
<package name="0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt;&lt;p&gt;
0603, grid 0.0125 inch</description>
</package>
<package name="0805">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt;&lt;p&gt;
0805, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="LEDC2012X80N">
<description>&lt;b&gt;150080BS75000&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="TSX-3225V">
<description>&lt;b&gt;TSX-3225V&lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="SOT65P210X110-5N">
<description>&lt;b&gt;5-Lead Plastic Package (SC-70)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="FUSC3216X75N">
<description>&lt;b&gt;0ZCJ0025FF2E&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="KMR621NG">
<description>&lt;b&gt;kmr6&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOP65P210X110-6N">
<description>&lt;b&gt;SOT363&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="USB_jacks">
<packages>
<package name="CONN5_ZX62D-B-5PA8_HIR">
</package>
</packages>
</library>
<library name="ATMEGA32U4">
<packages>
<package name="44ML_ATM">
</package>
</packages>
</library>
<library name="JST">
<packages>
<package name="JST_SM03B-SRSS-TB(LF)(SN)">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV1" library="filip" package="MA03-2SMT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="cap-master" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0603" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="filip" package="SCREWHOLE2-56" value="MOUNT-HOLE"/>
<element name="H3" library="filip" package="SCREWHOLE2-56" value="MOUNT-HOLE"/>
<element name="H2" library="filip" package="SCREWHOLE2-56" value="MOUNT-HOLE"/>
<element name="JP2" library="filip" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
<element name="JP1" library="filip" package="1X03_2.54_SCREWTERM" value=""/>
<element name="PAD1" library="wirepad" package="1,6/0,8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="filip" package="MCP6001_SC70-5" value="MCP6001LT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SamacSys_Parts" package="LEDC2012X80N" value="150080RS75000">
<attribute name="DESCRIPTION" value="LED,Wurth Elektronik,150080RS75000 Wurth Elektronik 150080RS75000, WL-SMCW Series Red LED, 625 nm 2012 (0805) Clear, Rectangle Lens SMD package"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MOUSER_PART_NUMBER" value="710-150080RS75000"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Wurth-Elektronik/150080RS75000?qs=LlUlMxKIyB2jdCo7bnfgew%3D%3D"/>
<attribute name="MANUFACTURER_NAME" value="Wurth Elektronik"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="150080RS75000"/>
<attribute name="NAME"/>
</element>
<element name="Y1" library="SamacSys_Parts" package="TSX-3225V" value="TSX-3225_16.0000MF18X-AC3">
<attribute name="DESCRIPTION" value="MHz Range crystal unit"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MOUSER_PART_NUMBER" value="732-TX325-16F18X-AC3"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Epson-Timing/TSX-3225-160000MF18X-AC3?qs=tC2qD9afNgpyT7dDEnDRhg%3D%3D"/>
<attribute name="MANUFACTURER_NAME" value="Epson Timing"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="TSX-3225 16.0000MF18X-AC3"/>
<attribute name="NAME"/>
</element>
<element name="IC4" library="SamacSys_Parts" package="SOT65P210X110-5N" value="MIC5365-3.3YC5_TR">
<attribute name="RS_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="LDO Regulator Pos 3.0V 0.15A 5-Pin SC-70 T/R"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MIC5365-3.0YC5 TR"/>
<attribute name="NAME"/>
</element>
<element name="IC3" library="filip" package="SO16NBC" value="MLX75306">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="USB_jacks" package="CONN5_ZX62D-B-5PA8_HIR" value="USB">
<attribute name="VENDOR" value="Hirose"/>
<attribute name="SOURCELIBRARY" value="Hirose_2018-12-15"/>
<attribute name="COPYRIGHT" value=""/>
<attribute name="BUILT_BY" value=""/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ZX62D-B-5PA8(30)"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="ATMEGA32U4" package="44ML_ATM" value="ATMEGA32U4-AU">
<attribute name="VENDOR" value="Atmel"/>
<attribute name="SOURCELIBRARY" value="Atmel_2011-04-02"/>
<attribute name="BUILT_BY" value="EMA_UL_Team"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATMEGA32U4-AU"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="cap-master" package="0603" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="cap-master" package="0603" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="cap-master" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0603" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0603" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="cap-master" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="cap-master" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="cap-master" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="cap-master" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="cap-master" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="cap-master" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="cap-master" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="cap-master" package="0603" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="SamacSys_Parts" package="FUSC3216X75N" value="500ma">
<attribute name="HEIGHT" value="0.75mm"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="0ZCJ0025FF2E"/>
<attribute name="MANUFACTURER_NAME" value="Bel Circuit Protection"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="BEL FUSE - CIRCUIT PROTECTION - 0ZCJ0025FF2E - FUSE, RESETTABLE PTC, 16VDC, 0.25A, SMD"/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SamacSys_Parts" package="KMR621NG" value="KMR631NGULCLFS">
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="KMR631NGULCLFS"/>
<attribute name="MANUFACTURER_NAME" value="C &amp; K COMPONENTS"/>
<attribute name="MOUSER_PART_NUMBER" value="611-KMR631NGULCLFS"/>
<attribute name="DESCRIPTION" value="KMR631NGULCLFS (Tactile Switches)"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/CK/KMR631NGULCLFS?qs=HXFqYaX1Q2xBA5gT0%2FzYzA%3D%3D"/>
<attribute name="NAME"/>
</element>
<element name="IC2" library="SamacSys_Parts" package="SOP65P210X110-6N" value="74LVC2G34GW,125">
<attribute name="DESCRIPTION" value="74LVC2G34 - Dual buffer gate@en-us"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Nexperia/74LVC2G34GW125?qs=me8TqzrmIYUOkg5J0C6mqA%3D%3D"/>
<attribute name="MANUFACTURER_NAME" value="Nexperia"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="74LVC2G34GW,125"/>
<attribute name="MOUSER_PART_NUMBER" value="771-LVC2G34GW125"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="NAME"/>
</element>
<element name="IC5" library="SamacSys_Parts" package="SOP65P210X110-6N" value="74LVC2G34GW,125">
<attribute name="DESCRIPTION" value="74LVC2G34 - Dual buffer gate@en-us"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Nexperia/74LVC2G34GW125?qs=me8TqzrmIYUOkg5J0C6mqA%3D%3D"/>
<attribute name="MANUFACTURER_NAME" value="Nexperia"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="74LVC2G34GW,125"/>
<attribute name="MOUSER_PART_NUMBER" value="771-LVC2G34GW125"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="JST" package="JST_SM03B-SRSS-TB(LF)(SN)" value="SM03B-SRSS-TB(LF)(SN)">
<attribute name="PACKAGE" value="None"/>
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount, Right Angle 3 position 0.039 (1.00mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1803-1-ND"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SM03B-SRSS-TB(LF)(SN)/?ref=eda"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM03B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
</element>
<element name="C12" library="cap-master" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="cap-master" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="P3"/>
<contactref element="U1" pad="43"/>
<contactref element="Y1" pad="4"/>
<contactref element="Y1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="5"/>
<contactref element="C9" pad="1"/>
<contactref element="J2" pad="GND1"/>
<contactref element="C14" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="35"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC4" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="SV1" pad="P$6"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="LED1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="J1" pad="S2"/>
<contactref element="J1" pad="S1"/>
<contactref element="S1" pad="4"/>
<contactref element="J2" pad="MOUNT_3" route="any" routetag="A.CASE_GND"/>
<contactref element="J2" pad="MOUNT_2" route="any" routetag="A.CASE_GND"/>
<contactref element="J2" pad="PAD_2" route="any" routetag="A.CASE_GND"/>
<contactref element="J2" pad="PAD_1" route="any" routetag="A.CASE_GND"/>
<contactref element="J2" pad="MOUNT_4" route="any" routetag="A.CASE_GND"/>
<contactref element="J2" pad="MOUNT_1" route="any" routetag="A.CASE_GND"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="JP1" pad="P1"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="44"/>
<contactref element="C13" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="IC1" pad="5"/>
<contactref element="F1" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="JP2" pad="P1"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="XTAL1">
<contactref element="U1" pad="17"/>
<contactref element="Y1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="U1" pad="16"/>
<contactref element="Y1" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="C14" pad="2"/>
<contactref element="J2" pad="VBUS1"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="6"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="D_N">
<contactref element="U1" pad="3"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D_P">
<contactref element="U1" pad="4"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="LED_IND">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="SCLK">
<contactref element="U1" pad="9"/>
<contactref element="SV1" pad="P$3"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="10"/>
<contactref element="SV1" pad="P$4"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="11"/>
<contactref element="SV1" pad="P$1"/>
<contactref element="IC5" pad="6"/>
</signal>
<signal name="/RESET">
<contactref element="U1" pad="13"/>
<contactref element="SV1" pad="P$5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="D1_N">
<contactref element="J2" pad="D+1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="D1_P">
<contactref element="J2" pad="D-1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="RXD1">
<contactref element="U1" pad="20"/>
</signal>
<signal name="TXD1">
<contactref element="U1" pad="21"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="42"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="PWM_OUT">
<contactref element="U1" pad="29"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="PWM_LED">
<contactref element="U1" pad="30"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="LEDSW2">
<contactref element="PAD1" pad="1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="LEDSW1">
<contactref element="U1" pad="28"/>
<contactref element="JP2" pad="P2"/>
</signal>
<signal name="PB">
<contactref element="U1" pad="31"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="SCLK1">
<contactref element="IC3" pad="1"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="MISO1">
<contactref element="IC3" pad="2"/>
<contactref element="IC5" pad="1"/>
</signal>
<signal name="MOSI1">
<contactref element="IC3" pad="3"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="FRAME1">
<contactref element="IC3" pad="7"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="CS1">
<contactref element="IC3" pad="8"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="+3V3">
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC4" pad="5"/>
<contactref element="C8" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC2" pad="5"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="LED1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="CS">
<contactref element="U1" pad="1"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="FRAME">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="ADC9">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="P2"/>
</signal>
<signal name="POW_EN">
<contactref element="IC4" pad="3"/>
<contactref element="R9" pad="2"/>
<contactref element="SV1" pad="P$2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="PF5">
<contactref element="U1" pad="38"/>
</signal>
<signal name="PF6">
<contactref element="U1" pad="37"/>
</signal>
<signal name="PF7">
<contactref element="U1" pad="36"/>
</signal>
<signal name="PD4">
<contactref element="U1" pad="25"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
