(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/Vref")
  (net 2 "GND")
  (net 3 "+VDC")
  (net 4 "/Vout")
  (net 5 "Net-(U1--IN2)")
  (net 6 "/Triangle")
  (net 7 "Net-(D1-K)")
  (net 8 "/PWM")
  (net 9 "unconnected-(J1-Pin_2-Pad2)")
  (net 10 "unconnected-(J2-Pin_2-Pad2)")
  (net 11 "Net-(U1-+IN1)")
  (net 12 "Net-(U1-+IN2)")
  (net 13 "/sqrWav")
  (net 14 "/Vsense")
  (net 15 "/2.5Vref")
  (net 16 "/feedback")
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 154.686 97.282 -90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at -3.302 0.254 -180) (layer "F.SilkS"))
    (fp_text value "47u" (at 0 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 4 "/Vout") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 129.8194 97.536)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at -3.048 0.254) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 3 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 115.348 88.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "40.2k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 3 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 1 "/Vref") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 121.4534 99.314)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 5 "Net-(U1--IN2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 6 "/Triangle") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 121.682 87.63)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "8.3k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 11 "Net-(U1-+IN1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 13 "/sqrWav") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 151.13 97.282 -90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C6" (at -3.302 0.254 -180) (layer "F.SilkS"))
    (fp_text value "47u" (at 0 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 4 "/Vout") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 113.824 99.568 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at -2.794 0 -180) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 3 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical" (layer "F.Cu")
    (at 107.442 100.838 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-5.08; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1836309 8A 320V")
    (tags "phoenix_contact connector MCV_01x03_G_5.08mm")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J2" (at 14.224 -3.81) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x03" (at 5.08 4.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 -3.65 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1388888889)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.8 3.6) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(J2-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 10.16 0 90) (size 1.8 3.6) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 3 "+VDC") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 121.4694 95.25 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 3.3594 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 12 "Net-(U1-+IN2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 121.7234 90.17 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 3.3594 0) (layer "F.SilkS"))
    (fp_text value "3.48k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 11 "Net-(U1-+IN1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 115.348 92.964 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 3.048 0) (layer "F.SilkS"))
    (fp_text value "0.01u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "/Vref") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical" (layer "F.Cu")
    (at 161.036 90.678 -90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-5.08; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1836309 8A 320V")
    (tags "phoenix_contact connector MCV_01x03_G_5.08mm")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "screw terminal")
    (attr through_hole)
    (fp_text reference "J1" (at -4.064 0 -180) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x03" (at 5.08 4.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 -3.65 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.8 3.6) (drill 1.2) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1388888889)
      (net 4 "/Vout") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.8 3.6) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(J1-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 10.16 0 270) (size 1.8 3.6) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 121.412 101.346)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.794 0 180) (layer "F.SilkS"))
    (fp_text value "2.0k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 11 "Net-(U1-+IN1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 6 "/Triangle") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 121.4534 97.282)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -3.5974 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 13 "/sqrWav") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 5 "Net-(U1--IN2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder" (layer "F.Cu")
    (at 147.574 97.282 -90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at -3.302 0 -180) (layer "F.SilkS"))
    (fp_text value "47u" (at 0 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 4 "/Vout") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (at 142.494 99.314)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "40V 600mV@1A 1A SOD-323 Schottky Barrier Diodes, SOD-323")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D2" (at -3.556 0.254) (layer "F.SilkS"))
    (fp_text value "1N5819WS" (at 0 2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.127 -1.905) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 7 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 121.4694 93.218)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 3 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 12 "Net-(U1-+IN2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1210_3225Metric_Pad1.42x2.65mm_HandSolder" (layer "F.Cu")
    (at 142.494 95.758)
    (descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 0.254 -2.28) (layer "F.SilkS"))
    (fp_text value "100u" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0) (size 1.425 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392982)
      (net 7 "Net-(D1-K)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0) (size 1.425 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392982)
      (net 4 "/Vout") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 115.348 90.932 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 3.048 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 1 "/Vref") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 137.2385 89.154)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Low-dropout high current voltage reference, 1.250V, ±0.4% accuracy, SOT-23")
    (property "ki_keywords" "voltage reference ldo")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "MAX6101" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+VDC") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/2.5Vref") (pinfunction "OUT") (pintype "power_out"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 141.732 91.694 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 1.778) (layer "F.SilkS"))
    (fp_text value "16.9k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 4 "/Vout") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 14 "/Vsense") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (at 136.652 95.758 180)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "40V 600mV@1A 1A SOD-323 Schottky Barrier Diodes, SOD-323")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D1" (at -0.127 -1.905 180) (layer "F.SilkS"))
    (fp_text value "1N5819WS" (at 0 2.1 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.127 -1.905 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 7 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2272727273)
      (net 8 "/PWM") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "opampSwitcher:R_14_ADI-M" (layer "F.Cu")
    (at 129.8194 91.44)
    (tags "AD8040ARZ ")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "AD8040ARZ")
    (attr smd)
    (fp_text reference "U1" (at -5.1054 -4.572 unlocked) (layer "F.SilkS"))
    (fp_text value "AD8040ARZ" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -2.5146 -3.81) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/sqrWav") (pinfunction "VOUT1") (pintype "unspecified"))
    (pad "2" smd rect (at -2.5146 -2.54) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/Vref") (pinfunction "-IN1") (pintype "unspecified"))
    (pad "3" smd rect (at -2.5146 -1.27) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(U1-+IN1)") (pinfunction "+IN1") (pintype "unspecified"))
    (pad "4" smd rect (at -2.5146 0) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+VDC") (pinfunction "+VS") (pintype "power_in"))
    (pad "5" smd rect (at -2.5146 1.27) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U1-+IN2)") (pinfunction "+IN2") (pintype "unspecified"))
    (pad "6" smd rect (at -2.5146 2.54) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(U1--IN2)") (pinfunction "-IN2") (pintype "unspecified"))
    (pad "7" smd rect (at -2.5146 3.81) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/Triangle") (pinfunction "VOUT2") (pintype "unspecified"))
    (pad "8" smd rect (at 2.5146 3.81) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/PWM") (pinfunction "VOUT3") (pintype "unspecified"))
    (pad "9" smd rect (at 2.5146 2.54) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/Triangle") (pinfunction "-IN3") (pintype "unspecified"))
    (pad "10" smd rect (at 2.5146 1.27) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/feedback") (pinfunction "+IN3") (pintype "unspecified"))
    (pad "11" smd rect (at 2.5146 0) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "-VS") (pintype "power_in"))
    (pad "12" smd rect (at 2.5146 -1.27) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/2.5Vref") (pinfunction "+IN4") (pintype "unspecified"))
    (pad "13" smd rect (at 2.5146 -2.54) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/Vsense") (pinfunction "-IN4") (pintype "unspecified"))
    (pad "14" smd rect (at 2.5146 -3.81) (size 2.286 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/feedback") (pinfunction "VOUT4") (pintype "unspecified"))
    (model "${KIPRJMOD}/R_14_ADI.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 137.16 92.202 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "opampSwitcher.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.778) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 14 "/Vsense") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 102.108 85.598) (end 102.108 104.394)
    (layer "Edge.Cuts"))
  (gr_line (start 102.108 104.394) (end 166.37 104.394)
    (layer "Edge.Cuts"))
  (gr_line (start 166.37 104.394) (end 166.37 85.598)
    (layer "Edge.Cuts"))
  (gr_line (start 166.37 85.598) (end 102.108 85.598)
    (layer "Edge.Cuts"))
  (gr_text "Gnd" (at 113.538 101.854) (layer "B.SilkS"))
  (gr_text "Vout" (at 157.226 91.186) (layer "B.SilkS"))
  (gr_text "Gnd" (at 157.734 102.362) (layer "B.SilkS"))
  (gr_text "Vin 5V-12V" (at 119.38 91.694) (layer "B.SilkS"))
  (gr_text "Vout\n3.3V" (at 153.416 90.932) (layer "F.SilkS"))
  (gr_text "Gnd" (at 153.67 102.362) (layer "F.SilkS"))
  (gr_text "Gnd" (at 111.252 103.378) (layer "F.SilkS"))
  (gr_text "Vin 5V-12V" (at 105.156 87.63) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 156.464 97.79)
        (xy 143.002 97.79)
        (xy 143.002 100.838)
        (xy 156.464 100.838)
      )
    )
  )
  (zone (net 4) (net_name "/Vout") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 143.764 93.726)
        (xy 143.764 97.282)
        (xy 156.464 97.282)
        (xy 156.464 93.726)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 102.362 85.852)
        (xy 102.362 104.14)
        (xy 166.116 104.14)
        (xy 166.116 85.852)
      )
    )
  )
)
