(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 43)
    (no_connects 0)
    (area 100.999999 79.899999 118.100001 104.600001)
    (thickness 0.8)
    (drawings 32)
    (tracks 226)
    (zones 0)
    (modules 21)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.2)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.1 2.1)
    (pad_drill 2.1)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x20000_00000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(R4-Pad2)")
  (net 4 /VID_SWITCH)
  (net 5 "Net-(J1-Pad1)")
  (net 6 /VID_SENSE)
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(J3-Pad3)")
  (net 9 /SCK)
  (net 10 /MISO)
  (net 11 /MOSI)
  (net 12 /RST)
  (net 13 "Net-(C5-Pad1)")
  (net 14 "Net-(Q1-Pad1)")
  (net 15 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net /VID_SENSE)
    (add_net /VID_SWITCH)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D091A)
    (at 106.52 94.7 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A5D079D)
    (at 111.1 94.8)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MAX4624/5 (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad3)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D0930)
    (at 102.1 88.375 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 10uf (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D0936)
    (at 102.1 85.375 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A5D090F)
    (at 108.01 94.67 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5A5E00A5)
    (at 110.38 87.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /VID_SENSE))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 5AEB1B1E)
    (at 105.9 87.3 90)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.19 1.26 90) (layer F.SilkS))
    (fp_text value ATTINY25 (at 0 3.68 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.65 -1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 /RST))
    (pad 2 smd rect (at -3.65 -0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R4-Pad2)"))
    (pad 3 smd rect (at -3.65 0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (pad 4 smd rect (at -3.65 1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3.65 1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 6 smd rect (at 3.65 0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 7 smd rect (at 3.65 -0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 8 smd rect (at 3.65 -1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:USB_3_PADS (layer F.Cu) (tedit 5A5E0461)
    (at 116.9 89.4 90)
    (fp_text reference J1 (at 0.3 1.6 90) (layer F.SilkS) hide)
    (fp_text value EV100 (at 0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.25 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.25 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /VID_SENSE))
  )
  (module KiCadCustomLibs:USB_3_PADS (layer F.Cu) (tedit 5A5E042A)
    (at 116.9 94.9 90)
    (fp_text reference J3 (at 0.3 1.6 90) (layer F.SilkS) hide)
    (fp_text value DVR_VIDEO (at 0.1 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.25 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.25 0 90) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad3)"))
  )
  (module KiCadCustomLibs:POWER2PIN (layer F.Cu) (tedit 5A5E0466)
    (at 116.9 85.4 90)
    (fp_text reference J4 (at 0.1 1.8 90) (layer F.SilkS) hide)
    (fp_text value PWR (at 0.3 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 2 smd rect (at 0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module KiCadCustomLibs:POWER2PIN (layer F.Cu) (tedit 5A5E0441)
    (at 116.9 98.85 90)
    (fp_text reference J5 (at 0.1 1.8 90) (layer F.SilkS) hide)
    (fp_text value PWR_DVR (at 0.3 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module KiCadCustomLibs:Pads_prog_6pin1.25mm (layer F.Cu) (tedit 5A5E082B)
    (at 104.95 81.3 180)
    (fp_text reference J6 (at 0.5 2 180) (layer F.SilkS) hide)
    (fp_text value PROG (at 0 -2.25 180) (layer F.Fab) hide)
    (pad 6 smd oval (at 3.125 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd oval (at -3.125 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 5 smd oval (at 1.875 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -1.875 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 3 smd oval (at -0.625 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 4 smd oval (at 0.625 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /RST))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A5E1569)
    (at 114.1 98.95 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 22uf (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:POWER2PIN (layer F.Cu) (tedit 5AB389E5)
    (at 116.9 102.85 270)
    (fp_text reference J2 (at 0.16 -3.76 270) (layer F.SilkS) hide)
    (fp_text value Buttons (at 0.3 -1.6 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.9 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 2 smd rect (at 0.9 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5AB38A4F)
    (at 111.2 99.3)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value "AO3415 (P)" (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB38BC7)
    (at 110.73 102.05)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB39C57)
    (at 102.35 94.31 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer F.Cu) (tedit 5AB3AA99)
    (at 111.11 83.96)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value B5819WS (at 0.1 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.85) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB56501)
    (at 110.38 90.44)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 4.7K (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AB56516)
    (at 110.375 92 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 47K (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VID_SWITCH))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:ESC_PWR_PAD (layer F.Cu) (tedit 59AD59DE)
    (at 113 81.55)
    (fp_text reference J7 (at 0 1.6) (layer F.SilkS) hide)
    (fp_text value SuperCap (at -0.1 -1.6) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (gr_text "Super\nCap+" (at 110.85 81.66) (layer F.SilkS))
  (gr_text RST (at 104.34 82.59 90) (layer B.SilkS))
  (gr_line (start 101.1 80) (end 114 80) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 101.1 97.1) (end 108.5 97.1) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 101.1 97.1) (end 101.1 80) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 118 83.5) (end 118 104.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 108.5 104.5) (end 108.5 97.1) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 108.5 104.5) (end 118 104.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_text "nppc\n2018" (at 111.65 102.67) (layer B.SilkS))
  (gr_text V2.0 (at 110.13 103.72) (layer F.SilkS))
  (gr_line (start 114 83.5) (end 118 83.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 114 80) (end 114 83.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_text 5V (at 114.09 85.51) (layer F.SilkS))
  (gr_text EV100 (at 111.69 89.04) (layer F.SilkS))
  (gr_text DVR (at 116.35 92.5) (layer F.SilkS))
  (gr_text Vout (at 115.1 93.7) (layer F.SilkS))
  (gr_text Vin (at 115.5 96.1) (layer F.SilkS))
  (gr_text SigG (at 115.04 88.21) (layer F.SilkS))
  (gr_text VidG (at 115.06 90.68) (layer F.SilkS))
  (gr_text - (at 115.5 98 90) (layer F.SilkS))
  (gr_text - (at 115.4 84.5 90) (layer F.SilkS))
  (gr_text + (at 115.5 99.7) (layer F.SilkS))
  (gr_text + (at 115.45 86.25) (layer F.SilkS))
  (gr_text + (at 101.83 82.99) (layer F.SilkS))
  (gr_text SCK (at 105.61 82.68 90) (layer B.SilkS))
  (gr_text MISO (at 106.82 82.9 90) (layer B.SilkS))
  (gr_text MOSI (at 108.11 82.93 90) (layer B.SilkS))
  (gr_text K3 (at 115.47 101.95) (layer F.SilkS))
  (gr_text K1 (at 115.49 103.72) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 99 79) (xy 119 79) (xy 119 106) (xy 99 106)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 100 105) (xy 120 105) (xy 120 80) (xy 100 80)
      )
    )
  )
)
