(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 25)
    (no_connects 2)
    (area 136.124999 95.924999 171.375001 112.075001)
    (thickness 1.6)
    (drawings 17)
    (tracks 129)
    (zones 0)
    (modules 14)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(P1-Pad5)")
  (net 4 "Net-(P1-Pad8)")
  (net 5 "Net-(P1-Pad10)")
  (net 6 "Net-(P1-Pad11)")
  (net 7 "Net-(P1-Pad13)")
  (net 8 "Net-(P1-Pad14)")
  (net 9 "Net-(P1-Pad15)")
  (net 10 "Net-(P1-Pad16)")
  (net 11 "Net-(P2-Pad1)")
  (net 12 "Net-(P2-Pad6)")
  (net 13 "Net-(U1-Pad4)")
  (net 14 "Net-(C1-Pad1)")
  (net 15 "Net-(C2-Pad2)")
  (net 16 "Net-(P1-Pad7)")
  (net 17 "Net-(P1-Pad6)")
  (net 18 "Net-(P1-Pad3)")
  (net 19 "Net-(P1-Pad2)")
  (net 20 "Net-(P1-Pad1)")
  (net 21 "Net-(JP2-Pad1)")
  (net 22 "Net-(JP2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(U1-Pad4)")
  )
  (module Brain_Duino:HM-13 (layer F.Cu) (tedit 581B7FF2)
    (at 158.3 104.25 270)
    (descr "Itead HC-05/HC-06 serial Bluetooth module")
    (fp_text reference P1 (at 0 -14.59992 270) (layer F.SilkS))
    (fp_text value HM-13 (at -1.75 0.9 360) (layer F.SilkS))
    (pad 8 smd rect (at -7.09986 4.50088 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad8)"))
    (pad 7 smd rect (at -7.09986 2.99974 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P1-Pad7)"))
    (pad 6 smd rect (at -7.09986 1.50114 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P1-Pad6)"))
    (pad 5 smd rect (at -7.09986 0 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad5)"))
    (pad 4 smd rect (at -7.09986 -1.50114 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(JP2-Pad2)"))
    (pad 3 smd rect (at -7.09986 -2.99974 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at -7.09986 -4.50088 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad2)"))
    (pad 1 smd rect (at -7.09986 -5.99948 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad1)"))
    (pad 9 smd rect (at 6.59986 4.50088 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (pad 10 smd rect (at 6.59986 2.99974 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad10)"))
    (pad 11 smd rect (at 6.59986 1.50114 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad11)"))
    (pad 12 smd rect (at 6.59986 0 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 6.59986 -1.50114 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad13)"))
    (pad 14 smd rect (at 6.59986 -2.99974 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad14)"))
    (pad 15 smd rect (at 6.59986 -4.50088 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad15)"))
    (pad 16 smd rect (at 6.59986 -5.99948 270) (size 1.69926 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad16)"))
    (model walter/rf_modules/itead_hc-05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:0402 (layer F.Cu) (tedit 581B75E5)
    (at 149.8477 110.9 180)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference R4 (at 0.0477 1.3 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0.635 180) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad15)"))
    (pad 2 smd rect (at 0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57C365A3)
    (at 146.8 110.9)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.3) (layer F.SilkS))
    (fp_text value LED (at 0 1.5) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 581B75BC)
    (at 150.5 105.5 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 2.6 0 180) (layer F.SilkS))
    (fp_text value LP2985-3.3 (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Brain_Duino:Bluetooth_Socket (layer F.Cu) (tedit 57C4247F)
    (at 137.3 97.82)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 2.5 -1.12) (layer F.SilkS))
    (fp_text value BLUETOOTH_SOCKET (at -2.5 5.98 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C1-Pad1)"))
    (pad 3 thru_hole rect (at 0 5.08) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P1-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(JP2-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad6)"))
  )
  (module freetronics_footprints:0402_CAP (layer F.Cu) (tedit 581B7773)
    (at 150.4 102.8 180)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference C1 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 0.635 180) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:0402_CAP (layer F.Cu) (tedit 581B75D0)
    (at 150.7 108 180)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference C2 (at 2.1 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 0.635 180) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:0402 (layer F.Cu) (tedit 581B75ED)
    (at 142.6 108.2)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference R1 (at 0 -1.2) (layer F.SilkS))
    (fp_text value 1k (at 0 0.635) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0.6477 0) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(JP2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:0402 (layer F.Cu) (tedit 581B75FC)
    (at 145.5 108.2 180)
    (descr <b>CAPACITOR</b><p>)
    (fp_text reference R3 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value 2k (at 0 0.635 180) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.6477 0 180) (size 0.6985 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(JP2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:SW_PUSHBUTTON_SMD (layer F.Cu) (tedit 581B7635)
    (at 145.7 98.9 180)
    (attr smd)
    (fp_text reference SW1 (at -4.2 0 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 3.15 180) (layer Eco1.User) hide)
    (pad 2 smd rect (at -2.667 1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.667 1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.667 -1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad11)"))
    (pad 1 smd rect (at -2.667 -1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad11)"))
    (model switch.3dshapes/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:SJ_OPEN (layer F.Cu) (tedit 581B75DC)
    (at 145.4 104.2 270)
    (descr "<b>Solder jumper</b>")
    (fp_text reference JP1 (at 0.9 1.7 270) (layer F.SilkS))
    (fp_text value JUMPER (at 0 1.6 270) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 14 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 15 "Net-(C2-Pad2)"))
  )
  (module w_logo:Logo_silk_CC-BY-SA_10x4.5mm (layer B.Cu) (tedit 0)
    (at 154.6 106.7 180)
    (descr "CC BY-SA logo, 10x4.5mm")
    (fp_text reference G*** (at 1.9 -0.5 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 1.9 1.7 180) (layer B.SilkS) hide)
  )
  (module freetronics_footprints:LOGO_OSHW_silkscreen_2mm (layer F.Cu) (tedit 0)
    (at 142 104.3)
    (fp_text reference LOGO_OSHW_silkscreen_2mm (at 0 1.05918) (layer F.SilkS) hide)
    (fp_text value val** (at 0 -1.05918) (layer F.SilkS) hide)
  )
  (module freetronics_footprints:SJ_OPEN (layer F.Cu) (tedit 581B8A9C)
    (at 142.5 110.6)
    (descr "<b>Solder jumper</b>")
    (fp_text reference JP2 (at -2.8 0) (layer F.SilkS))
    (fp_text value JUMPER (at 0 1.6) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.762 0) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 21 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0.762 0) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 22 "Net-(JP2-Pad2)"))
  )
  (gr_text "JP2 - for 3.3V RX" (at 144.3 111.1) (layer B.SilkS))
  (gr_text "JP1 - for 3.3V VCC" (at 144.2 109.7) (layer B.SilkS))
  (gr_text www.brain-duino.com (at 154.4 103.4) (layer B.SilkS))
  (gr_text "Silver Kuusik" (at 154.80678 100.902276) (layer B.SilkS))
  (gr_text "CC-BY-SA 4.0\n" (at 154.80678 99.702276) (layer B.SilkS))
  (gr_text "3 Nov 2016" (at 154.80678 102.102276) (layer B.SilkS))
  (gr_text "HM-13 breakout v0.1" (at 154.80678 96.902276) (layer B.SilkS))
  (gr_text RX (at 139.8 108) (layer F.SilkS))
  (gr_text TX (at 139.9 105.4) (layer F.SilkS))
  (gr_text GND (at 139.9 103) (layer F.SilkS))
  (gr_text VCC (at 139.9 100.4) (layer F.SilkS))
  (dimension 16 (width 0.3) (layer Margin)
    (gr_text "16.000 mm" (at 175.85 104 90) (layer Margin))
    (feature1 (pts (xy 171.3 96) (xy 177.2 96)))
    (feature2 (pts (xy 171.3 112) (xy 177.2 112)))
    (crossbar (pts (xy 174.5 112) (xy 174.5 96)))
    (arrow1a (pts (xy 174.5 96) (xy 175.086421 97.126504)))
    (arrow1b (pts (xy 174.5 96) (xy 173.913579 97.126504)))
    (arrow2a (pts (xy 174.5 112) (xy 175.086421 110.873496)))
    (arrow2b (pts (xy 174.5 112) (xy 173.913579 110.873496)))
  )
  (dimension 34 (width 0.3) (layer Margin)
    (gr_text "34.000 mm" (at 154.3 91.253665) (layer Margin))
    (feature1 (pts (xy 171.3 96) (xy 171.3 89.903665)))
    (feature2 (pts (xy 137.3 96) (xy 137.3 89.903665)))
    (crossbar (pts (xy 137.3 92.603665) (xy 171.3 92.603665)))
    (arrow1a (pts (xy 171.3 92.603665) (xy 170.173496 93.190086)))
    (arrow1b (pts (xy 171.3 92.603665) (xy 170.173496 92.017244)))
    (arrow2a (pts (xy 137.3 92.603665) (xy 138.426504 93.190086)))
    (arrow2b (pts (xy 137.3 92.603665) (xy 138.426504 92.017244)))
  )
  (gr_line (start 136.2 112) (end 136.2 96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.3 112) (end 136.2 112) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.3 96) (end 171.3 112) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.2 96) (end 171.3 96) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.2 96) (xy 171.3 96) (xy 171.3 112) (xy 136.2 112)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.3 96) (xy 171.3 112) (xy 136.2 112) (xy 136.2 96)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.3 96) (xy 165.9 96) (xy 165.9 112) (xy 171.3 112)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.9 96) (xy 171.3 96) (xy 171.3 112) (xy 165.9 112)
      )
    )
  )
)
