<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="8.255" y1="0.9525" x2="17.145" y2="0.9525" width="0" layer="20"/>
<wire x1="7.3025" y1="15.875" x2="7.3025" y2="13.0175" width="0" layer="20"/>
<wire x1="7.3025" y1="4.7625" x2="7.3025" y2="1.905" width="0" layer="20"/>
<text>AVR 8-pin
ISP Adapter</text>
<text>HokieGeek</text>
<wire x1="7.3025" y1="13.0175" x2="2.2225" y2="13.0175" width="0" layer="20"/>
<wire x1="2.2225" y1="13.0175" x2="1.27" y2="12.065" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="12.065" x2="1.27" y2="5.715" width="0" layer="20"/>
<wire x1="2.2225" y1="4.7625" x2="7.3025" y2="4.7625" width="0" layer="20"/>
<wire x1="17.145" y1="16.8275" x2="8.255" y2="16.8275" width="0" layer="20"/>
<wire x1="18.0975" y1="15.875" x2="18.0975" y2="1.905" width="0" layer="20"/>
<wire x1="8.255" y1="16.8275" x2="7.3025" y2="15.875" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="5.715" x2="2.2225" y2="4.7625" width="0" layer="20" curve="90"/>
<wire x1="7.3025" y1="1.905" x2="8.255" y2="0.9525" width="0" layer="20" curve="90"/>
<wire x1="18.0975" y1="15.875" x2="17.145" y2="16.8275" width="0" layer="20" curve="90"/>
<wire x1="17.145" y1="0.9525" x2="18.0975" y2="1.905" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
</package>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="ic-package" package="DIL08" value="">
<attribute name="VALUE"/>
</element>
<element name="AVR" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="LEFT" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="RIGHT" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="AVR" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="AVR" pad="2"/>
<contactref element="RIGHT" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="PIN6">
<contactref element="AVR" pad="1"/>
<contactref element="RIGHT" pad="3"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="PIN7">
<contactref element="AVR" pad="3"/>
<contactref element="RIGHT" pad="2"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="PIN1">
<contactref element="AVR" pad="5"/>
<contactref element="LEFT" pad="4"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="PIN5">
<contactref element="AVR" pad="4"/>
<contactref element="RIGHT" pad="4"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="PIN3">
<contactref element="LEFT" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="PIN2">
<contactref element="LEFT" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
