(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "./")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VCCTx")
	(net 3 "Net-(Q1-S)")
	(net 4 "V_USB")
	(net 5 "Net-(J1-D-)")
	(net 6 "Net-(J1-D+)")
	(net 7 "Net-(U2-~{RESET})")
	(net 8 "unconnected-(J1-ID-Pad4)")
	(net 9 "Net-(Q1-G)")
	(net 10 "TX_EN")
	(net 11 "TX_Data")
	(net 12 "Net-(U2-TXD{slash}D0)")
	(net 13 "Net-(U2-RXD{slash}D1)")
	(net 14 "RX_Data")
	(net 15 "Net-(U2-USBDP)")
	(net 16 "Net-(U2-USBDM)")
	(net 17 "unconnected-(U1-N.C.-Pad11)")
	(net 18 "unconnected-(U2-~{RTS}{slash}D2-Pad8)")
	(net 19 "unconnected-(U2-~{CTS}{slash}D3-Pad11)")
	(net 20 "Net-(U2-3V3OUT)")
	(footprint "isr_custom_lib:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
		(layer "F.Cu")
		(at 109.083 82.8988 -90)
		(descr "WDFN, 12 Pin (https://www.diodes.com/assets/Datasheets/PAM2306.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "WDFN NoLead")
		(property "Reference" "U2"
			(at -2.1776 2.8094 0)
			(layer "F.SilkS")
		)
		(property "Value" "FT234XD"
			(at 0 2.45 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WDFN*1EP*3x3mm*P0.45mm*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.425 -0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.425 0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.425 -0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.425 0.625 270)
			(size 0.69 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.45 -1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U2-USBDM)")
			(pinfunction "USBDM")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -1.45 -0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-~{RESET})")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.45 -0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-3V3OUT)")
			(pinfunction "3V3OUT")
			(pintype "power_out")
		)
		(pad "4" smd roundrect
			(at -1.45 0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "V_USB")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -1.45 0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -1.45 1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "TX_EN")
			(pinfunction "CBUS0")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 1.45 1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(U2-TXD{slash}D0)")
			(pinfunction "TXD/D0")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 1.45 0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "unconnected-(U2-~{RTS}{slash}D2-Pad8)")
			(pinfunction "~{RTS}/D2")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 1.45 0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-3V3OUT)")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 1.45 -0.225 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U2-RXD{slash}D1)")
			(pinfunction "RXD/D1")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 1.45 -0.675 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "unconnected-(U2-~{CTS}{slash}D3-Pad11)")
			(pinfunction "~{CTS}/D3")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 1.45 -1.125 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U2-USBDP)")
			(pinfunction "USBDP")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.7 2.5)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "isr_custom_lib:C_0402_1005Metric"
		(layer "F.Cu")
		(at 111.506 78.8901 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -1.9812 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.16 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.6256 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-~{RESET})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0402_1005Metric"
		(layer "F.Cu")
		(at 106.8552 85.6996)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 2.6188 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5468 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-3V3OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:FF-FE50MLNR"
		(layer "F.Cu")
		(at 97.24898 74.80554 180)
		(property "Reference" "U1"
			(at -2.97942 2.72034 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at -3.31 2.91 180)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at -3.31 -1.59 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -3.31 -1.59 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(solder_mask_margin 0.127)
		(solder_paste_margin_ratio -0)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.19 -8.05 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.127)
		)
		(pad "2" thru_hole circle
			(at -3.31 -1.59 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 11 "TX_Data")
			(pinfunction "DataIn")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -5.85 -2.86 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" thru_hole circle
			(at -3.31 -4.13 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole circle
			(at -5.85 -5.4 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCCTx")
			(pinfunction "VCCTx")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at -3.31 -6.67 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCCTx")
			(pinfunction "VccTx")
			(pintype "power_in")
		)
		(pad "7" thru_hole circle
			(at -3.31 -9.43 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCCTx")
			(pinfunction "VccRx")
			(pintype "power_in")
		)
		(pad "8" thru_hole circle
			(at -5.85 -10.7 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCCTx")
			(pinfunction "VccRx")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at -3.31 -11.97 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" thru_hole circle
			(at -5.85 -13.24 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 14 "RX_Data")
			(pinfunction "DataOut")
			(pintype "output")
		)
		(pad "11" thru_hole circle
			(at -3.31 -14.51 180)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U1-N.C.-Pad11)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 0 -16.1 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Paste" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "isr_custom_lib:C_0402_1005Metric"
		(layer "F.Cu")
		(at 114.9096 84.6328 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -1.9304 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.16 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.4224 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "V_USB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:USB_Micro-B_Molex_47346-0001"
		(layer "F.Cu")
		(at 118.618 82.8548 90)
		(descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
		(tags "Micro B USB SMD")
		(property "Reference" "J1"
			(at 5.1308 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "USB_B_Micro"
			(at 0 4.6 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 2.67 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 1.2 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3 -1.46 90)
			(size 0.45 1.38)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "V_USB")
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at -0.65 -1.46 90)
			(size 0.45 1.38)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(J1-D-)")
			(pinfunction "D-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.46 90)
			(size 0.45 1.38)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J1-D+)")
			(pinfunction "D+")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.65 -1.46 90)
			(size 0.45 1.38)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(J1-ID-Pad4)")
			(pinfunction "ID")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.3 -1.46 90)
			(size 0.45 1.38)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "6" smd rect
			(at -3.375 1.2 90)
			(size 1.65 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.4875 -1.375 90)
			(size 1.425 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -1.15 1.2 90)
			(size 1.8 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.55 1.2 90)
			(size 1 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.4875 -1.375 90)
			(size 1.425 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 3.375 1.2 90)
			(size 1.65 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:R_0402_1005Metric"
		(layer "F.Cu")
		(at 112.0956 81.4578 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -1.7472 -0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.17 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.4424 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-D-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U2-USBDM)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:SOT-23"
		(layer "F.Cu")
		(at 108.9152 73.2259 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at -0.0254 2.9464 180)
			(layer "F.SilkS")
		)
		(property "Value" "DMN2004"
			(at 0 2.4 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "TX_EN")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(Q1-G)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:R_0402_1005Metric"
		(layer "F.Cu")
		(at 106.2208 87.1728 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -0.0528 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.17 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.7018 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U2-RXD{slash}D1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "RX_Data")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0402_1005Metric"
		(layer "F.Cu")
		(at 115.443 82.268 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -2.2072 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "47pF"
			(at 0 1.16 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.75 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J1-D+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0805_2012Metric"
		(layer "F.Cu")
		(at 109.855 76.0961 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -2.7178 -0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.68 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "V_USB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0402_1005Metric"
		(layer "F.Cu")
		(at 109.327 77.7471 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -1.925 -0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1.4786 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "V_USB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:R_0402_1005Metric"
		(layer "F.Cu")
		(at 109.327 78.8901)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -1.8342 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.4786 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "V_USB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U2-~{RESET})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:R_0402_1005Metric"
		(layer "F.Cu")
		(at 112.0956 84.3534 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.17 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.9398 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J1-D+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U2-USBDP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0402_1005Metric"
		(layer "F.Cu")
		(at 113.6904 83.947 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at -2.0066 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "47pF"
			(at 0 1.16 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.6002 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-D-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:R_0402_1005Metric"
		(layer "F.Cu")
		(at 106.17 84.328 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -0.002 1.2192 0)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.17 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.9652 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(U2-TXD{slash}D0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "TX_Data")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0805_2012Metric"
		(layer "B.Cu")
		(at 110.871 76.52 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.9108 0.0254 90)
			(layer "B.SilkS")
		)
		(property "Value" "6.8uF"
			(at 0 -1.68 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CGA4J1X5R1C685K125AC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:D_0603_1608Metric"
		(layer "B.Cu")
		(at 111.3508 82.2707 -90)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1"
			(at -2.9209 0.0028 90)
			(layer "B.SilkS")
		)
		(property "Value" "SP1103C-01UTG"
			(at 0 -1.43 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "V_USB")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:SOT-23"
		(layer "B.Cu")
		(at 106.299 77.216 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 3 0)
			(layer "B.SilkS")
		)
		(property "Value" "SI2369BDS-T1-GE3"
			(at 0 -2.4 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(Q1-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCCTx")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Conrads:744043003_WE-TPC-4828"
		(layer "B.Cu")
		(at 117.1956 79.4032 180)
		(property "Reference" "L1"
			(at 0 3.175 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 -0.127 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1 -0.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd custom
			(at 0 2 180)
			(size 0.508 0.508)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "Net-(Q1-S)")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_line
					(start -2.4 -1.2)
					(end -2.4 0.199999)
					(width 0.0508)
				)
				(gr_line
					(start 0.900617 -0.51706)
					(end 1.539553 -1.2)
					(width 0.0508)
				)
				(gr_line
					(start -1.539553 -1.2)
					(end -2.4 -1.2)
					(width 0.0508)
				)
				(gr_line
					(start -2.199999 0.4)
					(end 2.199999 0.4)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 0.199999)
					(end 2.4 -1.2)
					(width 0.0508)
				)
				(gr_poly
					(pts
						(xy -2.4 0.4) (xy -2.4 -1.2) (xy -1.539553 -1.2) (xy -0.900617 -0.51706) (xy 0 -0.265001) (xy 0.900617 -0.51706)
						(xy 1.539553 -1.2) (xy 2.4 -1.2) (xy 2.4 0.4)
					)
					(width 0.1)
					(fill yes)
				)
				(gr_line
					(start -0.900617 -0.51706)
					(end 0 -0.265001)
					(width 0.0508)
				)
				(gr_line
					(start 0 -0.265001)
					(end 0.900617 -0.51706)
					(width 0.0508)
				)
				(gr_line
					(start -1.539553 -1.2)
					(end -0.900617 -0.51706)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 -1.2)
					(end 1.539553 -1.2)
					(width 0.0508)
				)
				(gr_line
					(start 2.199999 0.4)
					(end 2.4 0.4)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 0.199999)
					(end -2.4 0.4)
					(width 0.0508)
				)
				(gr_line
					(start 1.539553 -1.2)
					(end 2.4 -1.2)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 0.4)
					(end -2.199999 0.4)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 -1.2)
					(end -1.539553 -1.2)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 0.199999)
					(end -2.4 -1.2)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 -1.2)
					(end 2.4 0.199999)
					(width 0.0508)
				)
				(gr_line
					(start 2.199999 0.4)
					(end -2.199999 0.4)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 0.4)
					(end 2.4 0.199999)
					(width 0.0508)
				)
			)
		)
		(pad "2" smd custom
			(at 0 -2.08 180)
			(size 0.508 0.508)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "V_USB")
			(pinfunction "2")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_line
					(start -1.539553 1.28)
					(end -2.4 1.28)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 1.28)
					(end -2.4 -0.119999)
					(width 0.0508)
				)
				(gr_line
					(start -2.199999 -0.32)
					(end 2.199999 -0.32)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 -0.119999)
					(end 2.4 1.28)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 -0.32)
					(end -2.199999 -0.32)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 -0.119999)
					(end -2.4 -0.32)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 1.28)
					(end 1.539553 1.28)
					(width 0.0508)
				)
				(gr_line
					(start 0 0.345001)
					(end 0.900617 0.59706)
					(width 0.0508)
				)
				(gr_line
					(start 2.199999 -0.32)
					(end 2.4 -0.32)
					(width 0.0508)
				)
				(gr_line
					(start 2.199999 -0.32)
					(end -2.199999 -0.32)
					(width 0.0508)
				)
				(gr_line
					(start -2.4 -0.119999)
					(end -2.4 1.28)
					(width 0.0508)
				)
				(gr_line
					(start -1.539553 1.28)
					(end -0.900617 0.59706)
					(width 0.0508)
				)
				(gr_poly
					(pts
						(xy -2.4 1.28) (xy -2.4 -0.32) (xy 2.4 -0.32) (xy 2.4 1.28) (xy 1.539553 1.28) (xy 0.900617 0.59706)
						(xy 0 0.345001) (xy -0.900617 0.59706) (xy -1.539553 1.28)
					)
					(width 0.1)
					(fill yes)
				)
				(gr_line
					(start 0.900617 0.59706)
					(end 1.539553 1.28)
					(width 0.0508)
				)
				(gr_line
					(start -1.539553 1.28)
					(end -2.4 1.28)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 1.28)
					(end 2.4 -0.119999)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 -0.32)
					(end 2.4 -0.119999)
					(width 0.0508)
				)
				(gr_line
					(start 2.4 1.28)
					(end 1.539553 1.28)
					(width 0.0508)
				)
				(gr_line
					(start -0.900617 0.59706)
					(end 0 0.345001)
					(width 0.0508)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "isr_custom_lib:R_0402_1005Metric"
		(layer "B.Cu")
		(at 108.966 77.089 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 2.1082 0.0508 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.17 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.651 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(Q1-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0805_2012Metric"
		(layer "B.Cu")
		(at 113.3348 80.584 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.6568 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "6.8uF"
			(at 0 -1.68 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CGA4J1X5R1C685K125AC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "V_USB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0805_2012Metric"
		(layer "B.Cu")
		(at 106.045 80.264 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0.0254 -1.8288 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCCTx")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "isr_custom_lib:C_0805_2012Metric"
		(layer "B.Cu")
		(at 106.172 85.471)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FS3_Companion.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VCCTx")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 90.7796 70.1548)
		(end 121.2596 95.5548)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Fireset3 Internal\nto micro-USB"
		(at 114.8588 90.0176 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.254)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.1397)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 90.678 69.9516) (xy 121.3104 69.9516) (xy 121.3104 95.8088) (xy 90.678 95.8088)
			)
		)
	)
	(embedded_fonts no)
)
