(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 80)
    (zones 0)
    (modules 5)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J2-Pad4)")
  (net 7 "Net-(J2-Pad5)")
  (net 8 "Net-(J2-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net VCC)
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x02_P1.27mm_Vertical (layer F.Cu) (tedit 5EF2AE5D)
    (at 142.3 58.1 270)
    (descr "Through hole straight pin header, 1x02, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695 90) (layer F.SilkS) hide)
    (fp_text value power (at 0 2.965 90) (layer F.Fab))
    (fp_text user %R (at 0 0.635 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical (layer F.Cu) (tedit 5EF2AE44)
    (at 139.1 58.1 270)
    (descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.27mm single row")
    (fp_text reference J2 (at 0 -1.695 270) (layer F.SilkS) hide)
    (fp_text value pins (at 0 8.045 270) (layer F.Fab))
    (fp_text user %R (at 0 3.175) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 127.6 61.875 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FPC4-59453-041110EDHLF:59453041110EDHLF (layer F.Cu) (tedit 5E35FAD9)
    (at 138 63.6 180)
    (descr 59453-041110EDHLF-2)
    (tags Connector)
    (attr smd)
    (fp_text reference J3 (at 0 1.175) (layer F.SilkS) hide)
    (fp_text value 59453-041110EDHLF (at 0 1.175) (layer F.SilkS) hide)
    (pad MP2 smd rect (at 1.49 1.35 180) (size 0.52 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad MP1 smd rect (at -1.49 1.35 180) (size 0.52 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.75 -0.1 180) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 3 smd rect (at 0.25 -0.1 180) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -0.25 -0.1 180) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 1 smd rect (at -0.75 -0.1 180) (size 0.3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Package_SO:SOIJ-8_5.3x5.3mm_P1.27mm (layer B.Cu) (tedit 5A02F2D3)
    (at 129.4 62.3 270)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.68 270) (layer B.SilkS) hide)
    (fp_text value ATtiny85-20SU (at 0 -3.68 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 3.65 1.905 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 7 smd rect (at 3.65 0.635 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 6 smd rect (at 3.65 -0.635 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 5 smd rect (at 3.65 -1.905 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 4 smd rect (at -3.65 -1.905 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.65 -0.635 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 2 smd rect (at -3.65 0.635 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 1 smd rect (at -3.65 1.905 270) (size 1.7 0.65) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIJ-8_5.3x5.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 143.1 57) (end 143.1 67.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.6 57) (end 143.1 57) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.6 67.1) (end 126.6 57) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.1 67.1) (end 126.6 67.1) (layer Edge.Cuts) (width 0.1))
  (dimension 0.141421 (width 0.15) (layer Dwgs.User)
    (gr_text "0.141 mm" (at 144.919239 58.619239 45) (layer Dwgs.User))
    (feature1 (pts (xy 143.6 57.2) (xy 144.464662 58.064662)))
    (feature2 (pts (xy 143.5 57.3) (xy 144.364662 58.164662)))
    (crossbar (pts (xy 143.95 57.75) (xy 144.05 57.65)))
    (arrow1a (pts (xy 144.05 57.65) (xy 143.668104 58.861221)))
    (arrow1b (pts (xy 144.05 57.65) (xy 142.838779 58.031896)))
    (arrow2a (pts (xy 143.95 57.75) (xy 145.161221 57.368104)))
    (arrow2b (pts (xy 143.95 57.75) (xy 144.331896 56.538779)))
  )
  (gr_text "X Y R L D U" (at 135.9 59.2) (layer F.SilkS))
  (gr_text GND (at 142.2 59.8 270) (layer F.SilkS))
  (gr_text v0.3 (at 133.9 65.3) (layer B.SilkS))
  (gr_text orangeglo (at 138.6 62.1 45) (layer B.SilkS))
  (gr_text CircleBoy (at 131.8 65.6) (layer F.SilkS))
  (gr_text 3-5 (at 140.9 59.8 270) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.1 67.1) (xy 126.6 67.1) (xy 126.6 57) (xy 143.1 57)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.1 67.1) (xy 126.6 67.1) (xy 126.6 57) (xy 143.1 57)
      )
    )
  )
)
