(kicad_pcb (version 4) (host pcbnew 4.0.6+dfsg1-1)
  (general
    (links 0)
    (no_connects 0)
    (area 94.116316 137.5 154.200001 221.250001)
    (thickness 1.6)
    (drawings 23)
    (tracks 0)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.6)
    (user_trace_width 2)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.33)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFCCE7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 SDA)
  (net 4 SCL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.33)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net SCL)
    (add_net SDA)
  )
  (module mrmeeseeks:Badgelife-Shitty-2x2 (layer B.Cu) (tedit 5B64DA9E)
    (at 128.95 180)
    (descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x02 2.54mm double row")
    (fp_text reference X1 (at 0 0) (layer B.Fab))
    (fp_text value Badgelife_shitty_connector (at 0 -4.2) (layer B.Fab))
    (pad 4 thru_hole circle (at 1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 3 thru_hole oval (at 1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 1 thru_hole oval (at -1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at -1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module badgelife_dev_board:biohacking (layer F.Cu) (tedit 0)
    (at 128.45 170.3)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module badgelife_dev_board:biohacking (layer F.Cu) (tedit 0)
    (at 128.4 170.3)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_circle (center 128.95 170.25) (end 143.55 182) (layer Edge.Cuts) (width 0.15))
  (dimension 6.500769 (width 0.3) (layer Dwgs.User)
    (gr_text "6.501 mm" (at 99.902029 145.192277 270.881404) (layer Dwgs.User))
    (feature1 (pts (xy 115.7 148.2) (xy 98.602189 148.463044)))
    (feature2 (pts (xy 115.6 141.7) (xy 98.502189 141.963044)))
    (crossbar (pts (xy 101.20187 141.92151) (xy 101.30187 148.42151)))
    (arrow1a (pts (xy 101.30187 148.42151) (xy 100.69819 147.30416)))
    (arrow1b (pts (xy 101.30187 148.42151) (xy 101.870893 147.286119)))
    (arrow2a (pts (xy 101.20187 141.92151) (xy 100.632847 143.056901)))
    (arrow2b (pts (xy 101.20187 141.92151) (xy 101.80555 143.03886)))
  )
  (dimension 27.2 (width 0.3) (layer Dwgs.User)
    (gr_text "27.200 mm" (at 128.5 138.85) (layer Dwgs.User))
    (feature1 (pts (xy 142.1 149) (xy 142.1 137.5)))
    (feature2 (pts (xy 114.9 149) (xy 114.9 137.5)))
    (crossbar (pts (xy 114.9 140.2) (xy 142.1 140.2)))
    (arrow1a (pts (xy 142.1 140.2) (xy 140.973496 140.786421)))
    (arrow1b (pts (xy 142.1 140.2) (xy 140.973496 139.613579)))
    (arrow2a (pts (xy 114.9 140.2) (xy 116.026504 140.786421)))
    (arrow2b (pts (xy 114.9 140.2) (xy 116.026504 139.613579)))
  )
  (dimension 2.54 (width 0.3) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 145.876 152.146 90) (layer Dwgs.User))
    (feature1 (pts (xy 138.684 150.876) (xy 147.226 150.876)))
    (feature2 (pts (xy 138.684 153.416) (xy 147.226 153.416)))
    (crossbar (pts (xy 144.526 153.416) (xy 144.526 150.876)))
    (arrow1a (pts (xy 144.526 150.876) (xy 145.112421 152.002504)))
    (arrow1b (pts (xy 144.526 150.876) (xy 143.939579 152.002504)))
    (arrow2a (pts (xy 144.526 153.416) (xy 145.112421 152.289496)))
    (arrow2b (pts (xy 144.526 153.416) (xy 143.939579 152.289496)))
  )
  (dimension 2.54 (width 0.3) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 145.622 172.466 270) (layer Dwgs.User))
    (feature1 (pts (xy 138.684 173.736) (xy 146.972 173.736)))
    (feature2 (pts (xy 138.684 171.196) (xy 146.972 171.196)))
    (crossbar (pts (xy 144.272 171.196) (xy 144.272 173.736)))
    (arrow1a (pts (xy 144.272 173.736) (xy 143.685579 172.609496)))
    (arrow1b (pts (xy 144.272 173.736) (xy 144.858421 172.609496)))
    (arrow2a (pts (xy 144.272 171.196) (xy 143.685579 172.322504)))
    (arrow2b (pts (xy 144.272 171.196) (xy 144.858421 172.322504)))
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.35 150.75) (xy 144.15 150.75) (xy 152.5 181.6) (xy 128.8 194.35) (xy 105.35 179.6)
        (xy 109.35 152.9)
      )
    )
  )
)
