(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 34)
    (zones 0)
    (modules 4)
    (nets 18)
  )
  (page USLetter)
  (title_block
    (title "Tally Output Adapter board for SWTALGPI8")
    (date 2022-05-04)
    (rev 20220504-3)
    (company "Chibi Circuitz")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.7)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J2-Pad23)")
  (net 3 "Net-(J2-Pad22)")
  (net 4 "Net-(J2-Pad21)")
  (net 5 "Net-(J2-Pad20)")
  (net 6 "Net-(J2-Pad19)")
  (net 7 "Net-(J2-Pad18)")
  (net 8 "Net-(J2-Pad17)")
  (net 9 "Net-(J2-Pad16)")
  (net 10 "Net-(Input1-Pad10)")
  (net 11 "Net-(Input1-Pad9)")
  (net 12 "Net-(Input1-Pad8)")
  (net 13 "Net-(Input1-Pad7)")
  (net 14 "Net-(Input1-Pad6)")
  (net 15 "Net-(Input1-Pad5)")
  (net 16 "Net-(Input1-Pad4)")
  (net 17 "Net-(Input1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.7)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(Input1-Pad10)")
    (add_net "Net-(Input1-Pad3)")
    (add_net "Net-(Input1-Pad4)")
    (add_net "Net-(Input1-Pad5)")
    (add_net "Net-(Input1-Pad6)")
    (add_net "Net-(Input1-Pad7)")
    (add_net "Net-(Input1-Pad8)")
    (add_net "Net-(Input1-Pad9)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 150.114 103.759 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference LOGO1 (at 0 0.381) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0 -1.397) (layer B.Fab) hide)
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-10-3.5-H_1x10_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F49)
    (at 144.5 105.25 180)
    (descr "Terminal Block Phoenix PT-1,5-10-3.5-H, 10 pins, pitch 3.5mm, size 35x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-10-3.5-H pitch 3.5mm size 35x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference Input1 (at 33.756 -2.446) (layer F.SilkS))
    (fp_text value 1984840 (at 15.619 3.571) (layer F.Fab))
    (fp_text user %R (at 33.756 -2.446) (layer F.Fab))
    (pad 10 thru_hole circle (at 31.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(Input1-Pad10)"))
    (pad 9 thru_hole circle (at 28 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(Input1-Pad9)"))
    (pad 8 thru_hole circle (at 24.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(Input1-Pad8)"))
    (pad 7 thru_hole circle (at 21 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(Input1-Pad7)"))
    (pad 6 thru_hole circle (at 17.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(Input1-Pad6)"))
    (pad 5 thru_hole circle (at 14 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(Input1-Pad5)"))
    (pad 4 thru_hole circle (at 10.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(Input1-Pad4)"))
    (pad 3 thru_hole circle (at 7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(Input1-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model C:/Users/Doug/Documents/KiCad/library/3d/1984840.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-10-3.5-H_1x10_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F49)
    (at 113 117.75)
    (descr "Terminal Block Phoenix PT-1,5-10-3.5-H, 10 pins, pitch 3.5mm, size 35x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-10-3.5-H pitch 3.5mm size 35x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference Output1 (at -2.129 -2.18) (layer F.SilkS))
    (fp_text value 1984840 (at 15.373 3.535) (layer F.Fab))
    (fp_text user %R (at -2.129 -2.18) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad23)"))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad22)"))
    (pad 3 thru_hole circle (at 7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad21)"))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad20)"))
    (pad 5 thru_hole circle (at 14 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad19)"))
    (pad 6 thru_hole circle (at 17.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad18)"))
    (pad 7 thru_hole circle (at 21 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad17)"))
    (pad 8 thru_hole circle (at 24.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad16)"))
    (pad 9 thru_hole circle (at 28 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 31.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model C:/Users/Doug/Documents/KiCad/library/3d/1984840.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Connector_Dsub:DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles (layer B.Cu) (tedit 59FEDEE2)
    (at 143.9 110.1 180)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J2 (at -2.912 -3.565) (layer B.SilkS))
    (fp_text value DB25_Male_MountingHoles (at 16.62 -8.73) (layer B.Fab))
    (fp_text user %R (at 16.62 -1.42) (layer B.Fab))
    (pad 0 thru_hole circle (at 40.17 -1.42 180) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 0 thru_hole circle (at -6.93 -1.42 180) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole circle (at 31.855 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 29.085 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole circle (at 26.315 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad23)"))
    (pad 22 thru_hole circle (at 23.545 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad22)"))
    (pad 21 thru_hole circle (at 20.775 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad21)"))
    (pad 20 thru_hole circle (at 18.005 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad20)"))
    (pad 19 thru_hole circle (at 15.235 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad19)"))
    (pad 18 thru_hole circle (at 12.465 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad18)"))
    (pad 17 thru_hole circle (at 9.695 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad17)"))
    (pad 16 thru_hole circle (at 6.925 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad16)"))
    (pad 15 thru_hole circle (at 4.155 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at 1.385 -2.84 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole circle (at 33.24 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 30.47 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 27.7 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 24.93 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(Input1-Pad10)"))
    (pad 9 thru_hole circle (at 22.16 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Input1-Pad9)"))
    (pad 8 thru_hole circle (at 19.39 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(Input1-Pad8)"))
    (pad 7 thru_hole circle (at 16.62 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(Input1-Pad7)"))
    (pad 6 thru_hole circle (at 13.85 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(Input1-Pad6)"))
    (pad 5 thru_hole circle (at 11.08 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(Input1-Pad5)"))
    (pad 4 thru_hole circle (at 8.31 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(Input1-Pad4)"))
    (pad 3 thru_hole circle (at 5.54 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(Input1-Pad3)"))
    (pad 2 thru_hole circle (at 2.77 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles.wrl
      (offset (xyz 0 0 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "chibicircuitz.com\n/tally" (at 109.855 116.205) (layer B.SilkS))
  (gr_text "GND    8   7   6   5   4   3   2   1" (at 112.395 120.523) (layer B.SilkS))
  (gr_text "GND    8   7   6   5   4   3   2   1" (at 112.395 102.362) (layer B.SilkS))
  (gr_text "Designed by\nChibi Circuitz" (at 109.855 120.015) (layer B.SilkS))
  (gr_text "Tally Output\nAdapter\nv20220505\nfor SWTALGPI8" (at 109.601 103.886) (layer B.SilkS))
  (gr_text GND (at 143.637 112.395) (layer F.SilkS))
  (gr_text "Designed by\nChibi Circuitz" (at 146.812 120.523) (layer F.SilkS))
  (gr_text "Tally Output\nAdapter\nv20220505\nfor\nSWTALGPI8" (at 147.066 104.902) (layer F.SilkS))
  (gr_arc (start 153.5 121.5) (end 153.5 122.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 153.5 101.5) (end 154.5 101.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101 101.5) (end 101 100.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101 121.5) (end 100 121.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.5 100.5) (end 101 100.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.5 121.5) (end 154.5 101.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101 122.5) (end 153.5 122.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 101.5) (end 100 121.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.483 101.473) (xy 154.483 121.666) (xy 153.416 122.555) (xy 100.965 122.428) (xy 100 121.412)
        (xy 99.949 101.727) (xy 101.219 100.584) (xy 153.594 100.584)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.432 101.473) (xy 154.432 121.539) (xy 153.416 122.428) (xy 101.016 122.428) (xy 100 121.412)
        (xy 100 101.854) (xy 101.092 100.584) (xy 153.543 100.584)
      )
    )
  )
)
