(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 89)
    (tracks 96)
    (zones 0)
    (modules 19)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 DGND)
  (net 2 AGND)
  (net 3 DATA_RX)
  (net 4 DATA_TX)
  (net 5 "Net-(J1-Pad11)")
  (net 6 5V)
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J4-Pad2)")
  (net 9 "Net-(J5-Pad2)")
  (net 10 "Net-(J7-Pad5)")
  (net 11 "Net-(J7-Pad6)")
  (net 12 "Net-(J1-Pad39)")
  (net 13 "Net-(J1-Pad37)")
  (net 14 "Net-(J1-Pad35)")
  (net 15 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net AGND)
    (add_net DATA_RX)
    (add_net DATA_TX)
    (add_net DGND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad39)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J7-Pad5)")
    (add_net "Net-(J7-Pad6)")
  )
  (module Symbol:weare (layer F.Cu) (tedit 0)
    (at 186.75 135)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbol:were (layer B.Cu) (tedit 0)
    (at 226 127.5 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 4.5) (layer B.SilkS) hide)
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 66 56)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 180R (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 5V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 68.54 64.5 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value POWER (at 1.27 3.96) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 DGND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B772AC7)
    (at 74.75 81.25)
    (descr "JST EH series connector, B03B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH side entry")
    (fp_text reference J5 (at 2.5 -2.8) (layer F.SilkS))
    (fp_text value TDS (at 2.5 4) (layer F.SilkS))
    (fp_text user %R (at 2.5 1.5) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 AGND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B772AC7)
    (at 182.5 71 90)
    (descr "JST EH series connector, B03B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH side entry")
    (fp_text reference J3 (at 9 0.25 180) (layer F.SilkS))
    (fp_text value Turbidity (at 1.5 6.5 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 AGND))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B772AC7)
    (at 182.5 84.5 90)
    (descr "JST EH series connector, B03B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH side entry")
    (fp_text reference J4 (at 9 0.25 180) (layer F.SilkS))
    (fp_text value pH (at 2.25 4 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 5V))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Dsub:DSUB-9_Female_Vertical_P2.77x2.84mm (layer F.Cu) (tedit 59FEDEE2)
    (at 168 126 270)
    (descr "9-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 25mm")
    (fp_text reference J7 (at -22 1.5) (layer F.SilkS))
    (fp_text value Umbilical (at 11.5 1 180) (layer F.SilkS))
    (fp_text user %R (at -5.54 1.42 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 5V))
    (pad 3 thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 DATA_RX))
    (pad 4 thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 DATA_TX))
    (pad 5 thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J7-Pad5)"))
    (pad 6 thru_hole circle (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J7-Pad6)"))
    (pad 7 thru_hole circle (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-9_Female_Vertical_P2.77x2.84mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A430)
    (at 128.75 93.55)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J8 (at 0 -2.77) (layer F.SilkS))
    (fp_text value "UART Console Connector" (at 0 15.47) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J7-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J7-Pad6)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 156.75 62.25)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 5V))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 166.91 69.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 2.5 180) (layer F.SilkS))
    (fp_text value 6.2K (at 4.91 -2.5 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad35)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 156.75 77)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad35)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 171.5 93.25 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 2.5 180) (layer F.SilkS))
    (fp_text value 1.5K (at 5.08 -2.5 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad37)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 161.25 100.25)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.3K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad37)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 82.5 73 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5 -2.37 90) (layer F.SilkS))
    (fp_text value 5.1K (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad39)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 74.25 62.84 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5 2.25 270) (layer F.SilkS))
    (fp_text value 5.1K (at 5 -2.5 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad39)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 AGND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x23_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A424)
    (at 149.72 70.75)
    (descr "Through hole straight socket strip, 2x23, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x23 2.54mm double row")
    (fp_text reference J1 (at -1.27 -2.77) (layer F.SilkS))
    (fp_text value BB_P9 (at -1.27 58.65) (layer F.Fab))
    (fp_text user %R (at -1.27 27.94 90) (layer F.Fab))
    (pad 46 thru_hole oval (at -2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 44 thru_hole oval (at -2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 42 thru_hole oval (at -2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at -2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad39)"))
    (pad 38 thru_hole oval (at -2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad37)"))
    (pad 36 thru_hole oval (at -2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad35)"))
    (pad 34 thru_hole oval (at -2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 AGND))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at -2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at -2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at -2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at -2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 DATA_RX))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at -2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 DATA_TX))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at -2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 5V))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 5V))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x23_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x23_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A424)
    (at 101.5 70.75)
    (descr "Through hole straight socket strip, 2x23, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x23 2.54mm double row")
    (fp_text reference J2 (at -1.27 -2.77) (layer F.SilkS))
    (fp_text value BB_P8 (at -1.27 58.65) (layer F.Fab))
    (fp_text user %R (at -1.27 27.94 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 DGND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at -2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at -2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at -2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at -2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at -2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at -2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at -2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at -2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at -2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at -2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 42 thru_hole oval (at -2.54 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 44 thru_hole oval (at -2.54 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 46 thru_hole oval (at -2.54 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x23_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5B772AC7)
    (at 182.5 58 90)
    (descr "JST EH series connector, B03B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH side entry")
    (fp_text reference J6 (at 9 0.5 180) (layer F.SilkS))
    (fp_text value Temp (at 2 5.5 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 1.5 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 5V))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad11)"))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 DGND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B03B-EH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 35x25mm (at 77.25 116.5) (layer Dwgs.User))
  (dimension 42 (width 0.15) (layer Dwgs.User)
    (gr_text "42.000 mm" (at 48.45 114.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 64.25 93.25) (xy 49.163579 93.25)))
    (feature2 (pts (xy 64.25 135.25) (xy 49.163579 135.25)))
    (crossbar (pts (xy 49.75 135.25) (xy 49.75 93.25)))
    (arrow1a (pts (xy 49.75 93.25) (xy 50.336421 94.376504)))
    (arrow1b (pts (xy 49.75 93.25) (xy 49.163579 94.376504)))
    (arrow2a (pts (xy 49.75 135.25) (xy 50.336421 134.123496)))
    (arrow2b (pts (xy 49.75 135.25) (xy 49.163579 134.123496)))
  )
  (dimension 32 (width 0.15) (layer Dwgs.User)
    (gr_text "32.000 mm" (at 77.75 89.45) (layer Dwgs.User))
    (feature1 (pts (xy 93.75 95.75) (xy 93.75 90.163579)))
    (feature2 (pts (xy 61.75 95.75) (xy 61.75 90.163579)))
    (crossbar (pts (xy 61.75 90.75) (xy 93.75 90.75)))
    (arrow1a (pts (xy 93.75 90.75) (xy 92.623496 91.336421)))
    (arrow1b (pts (xy 93.75 90.75) (xy 92.623496 90.163579)))
    (arrow2a (pts (xy 61.75 90.75) (xy 62.876504 91.336421)))
    (arrow2b (pts (xy 61.75 90.75) (xy 62.876504 90.163579)))
  )
  (gr_circle (center 90.25 96.75) (end 91.85 96.75) (layer Edge.Cuts) (width 0.15))
  (dimension 28 (width 0.15) (layer Dwgs.User)
    (gr_text "28.000 mm" (at 245.3 65.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 228.5 79.75) (xy 244.586421 79.75)))
    (feature2 (pts (xy 228.5 51.75) (xy 244.586421 51.75)))
    (crossbar (pts (xy 244 51.75) (xy 244 79.75)))
    (arrow1a (pts (xy 244 79.75) (xy 243.413579 78.623496)))
    (arrow1b (pts (xy 244 79.75) (xy 244.586421 78.623496)))
    (arrow2a (pts (xy 244 51.75) (xy 243.413579 52.876504)))
    (arrow2b (pts (xy 244 51.75) (xy 244.586421 52.876504)))
  )
  (dimension 38 (width 0.15) (layer Dwgs.User)
    (gr_text "38.000 mm" (at 212 42.45) (layer Dwgs.User))
    (feature1 (pts (xy 231 54.25) (xy 231 43.163579)))
    (feature2 (pts (xy 193 54.25) (xy 193 43.163579)))
    (crossbar (pts (xy 193 43.75) (xy 231 43.75)))
    (arrow1a (pts (xy 231 43.75) (xy 229.873496 44.336421)))
    (arrow1b (pts (xy 231 43.75) (xy 229.873496 43.163579)))
    (arrow2a (pts (xy 193 43.75) (xy 194.126504 44.336421)))
    (arrow2b (pts (xy 193 43.75) (xy 194.126504 43.163579)))
  )
  (dimension 31 (width 0.15) (layer Dwgs.User)
    (gr_text "31.000 mm" (at 209.5 80.45) (layer Dwgs.User))
    (feature1 (pts (xy 225 85.5) (xy 225 81.163579)))
    (feature2 (pts (xy 194 85.5) (xy 194 81.163579)))
    (crossbar (pts (xy 194 81.75) (xy 225 81.75)))
    (arrow1a (pts (xy 225 81.75) (xy 223.873496 82.336421)))
    (arrow1b (pts (xy 225 81.75) (xy 223.873496 81.163579)))
    (arrow2a (pts (xy 194 81.75) (xy 195.126504 82.336421)))
    (arrow2b (pts (xy 194 81.75) (xy 195.126504 81.163579)))
  )
  (dimension 42 (width 0.15) (layer Dwgs.User)
    (gr_text "42.000 mm" (at 236.55 103.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 222.5 124.5) (xy 235.836421 124.5)))
    (feature2 (pts (xy 222.5 82.5) (xy 235.836421 82.5)))
    (crossbar (pts (xy 235.25 82.5) (xy 235.25 124.5)))
    (arrow1a (pts (xy 235.25 124.5) (xy 234.663579 123.373496)))
    (arrow1b (pts (xy 235.25 124.5) (xy 235.836421 123.373496)))
    (arrow2a (pts (xy 235.25 82.5) (xy 234.663579 83.626504)))
    (arrow2b (pts (xy 235.25 82.5) (xy 235.836421 83.626504)))
  )
  (gr_text 35x25mm (at 210 101.75) (layer Dwgs.User))
  (gr_circle (center 197 75.7) (end 198.6 75.7) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 197 55.7) (end 198.6 55.7) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 59.5 138.25) (end 61.1 138.25) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 59.5 49.25) (end 61.1 49.25) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 230.5 49.25) (end 232.1 49.25) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 197.1 85.9) (end 197.1 87.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 222.1 85.9) (end 222.1 87.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 197.1 120.9) (end 197.1 122.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 227 75.7) (end 228.6 75.7) (layer Edge.Cuts) (width 0.15))
  (gr_text "Pollution Identification System\nThe Pennsylvania State University 2020\nRevision 001" (at 208 134.5) (layer F.SilkS))
  (gr_text we're (at 221 127.5) (layer B.SilkS))
  (gr_circle (center 230.5 138) (end 232.1 138) (layer Edge.Cuts) (width 0.15))
  (gr_text 30x20mm (at 213 68.5) (layer Dwgs.User))
  (gr_text "Beaglebone Black\nIndustrial" (at 125.25 71.25) (layer F.SilkS))
  (dimension 171 (width 0.3) (layer Dwgs.User)
    (gr_text "171.000 mm" (at 145 27.65) (layer Dwgs.User))
    (feature1 (pts (xy 230.5 49.25) (xy 230.5 29.163579)))
    (feature2 (pts (xy 59.5 49.25) (xy 59.5 29.163579)))
    (crossbar (pts (xy 59.5 29.75) (xy 230.5 29.75)))
    (arrow1a (pts (xy 230.5 29.75) (xy 229.373496 30.336421)))
    (arrow1b (pts (xy 230.5 29.75) (xy 229.373496 29.163579)))
    (arrow2a (pts (xy 59.5 29.75) (xy 60.626504 30.336421)))
    (arrow2b (pts (xy 59.5 29.75) (xy 60.626504 29.163579)))
  )
  (dimension 89 (width 0.3) (layer Dwgs.User)
    (gr_text "89.000 mm" (at 38.65 93.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 59.5 138.25) (xy 40.163579 138.25)))
    (feature2 (pts (xy 59.5 49.25) (xy 40.163579 49.25)))
    (crossbar (pts (xy 40.75 49.25) (xy 40.75 138.25)))
    (arrow1a (pts (xy 40.75 138.25) (xy 40.163579 137.123496)))
    (arrow1b (pts (xy 40.75 138.25) (xy 41.336421 137.123496)))
    (arrow2a (pts (xy 40.75 49.25) (xy 40.163579 50.376504)))
    (arrow2b (pts (xy 40.75 49.25) (xy 41.336421 50.376504)))
  )
  (dimension 180 (width 0.3) (layer Dwgs.User)
    (gr_text "180.000 mm" (at 145 21.9) (layer Dwgs.User))
    (feature1 (pts (xy 235 53.5) (xy 235 23.413579)))
    (feature2 (pts (xy 55 53.5) (xy 55 23.413579)))
    (crossbar (pts (xy 55 24) (xy 235 24)))
    (arrow1a (pts (xy 235 24) (xy 233.873496 24.586421)))
    (arrow1b (pts (xy 235 24) (xy 233.873496 23.413579)))
    (arrow2a (pts (xy 55 24) (xy 56.126504 24.586421)))
    (arrow2b (pts (xy 55 24) (xy 56.126504 23.413579)))
  )
  (dimension 98 (width 0.3) (layer Dwgs.User)
    (gr_text "98.000 mm" (at 33.400001 93.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 65 142.75) (xy 34.91358 142.75)))
    (feature2 (pts (xy 65 44.75) (xy 34.91358 44.75)))
    (crossbar (pts (xy 35.500001 44.75) (xy 35.500001 142.75)))
    (arrow1a (pts (xy 35.500001 142.75) (xy 34.91358 141.623496)))
    (arrow1b (pts (xy 35.500001 142.75) (xy 36.086422 141.623496)))
    (arrow2a (pts (xy 35.500001 44.75) (xy 34.91358 45.876504)))
    (arrow2b (pts (xy 35.500001 44.75) (xy 36.086422 45.876504)))
  )
  (gr_line (start 62.75 44.75) (end 227.5 44.75) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 227.5 52.25) (end 227.5 44.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 62.75 52.5) (end 55 52.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 227.5 142.5) (end 62.75 142.754031) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 227.5 135) (end 227.5 142.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 62.75 135) (end 55 135.25) (angle -88.15238973) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 235 52.25) (end 235 135) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55 52.5) (end 55 135.25) (layer Edge.Cuts) (width 0.15))
  (gr_text "Total Disolved Solids" (at 78.5 113.75) (layer F.SilkS))
  (gr_text "pH Sensor" (at 209.5 98.5) (layer F.SilkS))
  (gr_text "Turbidity Sensor" (at 213 65.5) (layer F.SilkS))
  (dimension 25 (width 0.3) (layer Dwgs.User)
    (gr_text "25.000 mm" (at 77.75 143.85) (layer Dwgs.User))
    (feature1 (pts (xy 90.25 131.75) (xy 90.25 142.336421)))
    (feature2 (pts (xy 65.25 131.75) (xy 65.25 142.336421)))
    (crossbar (pts (xy 65.25 141.75) (xy 90.25 141.75)))
    (arrow1a (pts (xy 90.25 141.75) (xy 89.123496 142.336421)))
    (arrow1b (pts (xy 90.25 141.75) (xy 89.123496 141.163579)))
    (arrow2a (pts (xy 65.25 141.75) (xy 66.376504 142.336421)))
    (arrow2b (pts (xy 65.25 141.75) (xy 66.376504 141.163579)))
  )
  (dimension 35 (width 0.3) (layer Dwgs.User)
    (gr_text "35.000 mm" (at 54.216301 114.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 65.25 96.75) (xy 55.72988 96.75)))
    (feature2 (pts (xy 65.25 131.75) (xy 55.72988 131.75)))
    (crossbar (pts (xy 56.316301 131.75) (xy 56.316301 96.75)))
    (arrow1a (pts (xy 56.316301 96.75) (xy 56.902722 97.876504)))
    (arrow1b (pts (xy 56.316301 96.75) (xy 55.72988 97.876504)))
    (arrow2a (pts (xy 56.316301 131.75) (xy 56.902722 130.623496)))
    (arrow2b (pts (xy 56.316301 131.75) (xy 55.72988 130.623496)))
  )
  (gr_circle (center 65.25 96.75) (end 66.85 96.75) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 90.25 131.75) (end 91.85 131.75) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 65.25 131.75) (end 66.85 131.75) (layer Edge.Cuts) (width 0.15))
  (dimension 35 (width 0.3) (layer Dwgs.User)
    (gr_text "35.000 mm" (at 229.4 103.4 90) (layer Dwgs.User))
    (feature1 (pts (xy 222.1 85.9) (xy 227.886421 85.9)))
    (feature2 (pts (xy 222.1 120.9) (xy 227.886421 120.9)))
    (crossbar (pts (xy 227.3 120.9) (xy 227.3 85.9)))
    (arrow1a (pts (xy 227.3 85.9) (xy 227.886421 87.026504)))
    (arrow1b (pts (xy 227.3 85.9) (xy 226.713579 87.026504)))
    (arrow2a (pts (xy 227.3 120.9) (xy 227.886421 119.773496)))
    (arrow2b (pts (xy 227.3 120.9) (xy 226.713579 119.773496)))
  )
  (dimension 25 (width 0.3) (layer Dwgs.User)
    (gr_text "25.000 mm" (at 209.6 129.85) (layer Dwgs.User))
    (feature1 (pts (xy 197.1 120.9) (xy 197.1 128.336421)))
    (feature2 (pts (xy 222.1 120.9) (xy 222.1 128.336421)))
    (crossbar (pts (xy 222.1 127.75) (xy 197.1 127.75)))
    (arrow1a (pts (xy 197.1 127.75) (xy 198.226504 127.163579)))
    (arrow1b (pts (xy 197.1 127.75) (xy 198.226504 128.336421)))
    (arrow2a (pts (xy 222.1 127.75) (xy 220.973496 127.163579)))
    (arrow2b (pts (xy 222.1 127.75) (xy 220.973496 128.336421)))
  )
  (dimension 20 (width 0.3) (layer Dwgs.User)
    (gr_text "20.000 mm" (at 239.85 65.7 270) (layer Dwgs.User))
    (feature1 (pts (xy 227 75.7) (xy 238.336421 75.7)))
    (feature2 (pts (xy 227 55.7) (xy 238.336421 55.7)))
    (crossbar (pts (xy 237.75 55.7) (xy 237.75 75.7)))
    (arrow1a (pts (xy 237.75 75.7) (xy 237.163579 74.573496)))
    (arrow1b (pts (xy 237.75 75.7) (xy 238.336421 74.573496)))
    (arrow2a (pts (xy 237.75 55.7) (xy 237.163579 56.826504)))
    (arrow2b (pts (xy 237.75 55.7) (xy 238.336421 56.826504)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 212 46.35) (layer Dwgs.User))
    (feature1 (pts (xy 227 55.7) (xy 227 47.863579)))
    (feature2 (pts (xy 197 55.7) (xy 197 47.863579)))
    (crossbar (pts (xy 197 48.45) (xy 227 48.45)))
    (arrow1a (pts (xy 227 48.45) (xy 225.873496 49.036421)))
    (arrow1b (pts (xy 227 48.45) (xy 225.873496 47.863579)))
    (arrow2a (pts (xy 197 48.45) (xy 198.126504 49.036421)))
    (arrow2b (pts (xy 197 48.45) (xy 198.126504 47.863579)))
  )
  (gr_circle (center 222.1 120.9) (end 222.1 122.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 227 55.7) (end 228.6 55.7) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name AGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.75 49.25) (xy 230 49.25) (xy 230 137.5) (xy 60 137.5)
      )
    )
  )
  (zone (net 6) (net_name 5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 230 137.5) (xy 230 49.25) (xy 59.75 49.25) (xy 60 137.5) (xy 66.5 137.5)
      )
    )
  )
)
